ÍÎÂÎÐÎÑÑÈÉÑÊÈÉ ÌÎÐÑÊÎÉ ÑÀÉÒ.
www.mga-nvr.ru
======================

#################################
Îòâåòû íà CES 5.0 â êîíöå
#################################

AAET	Transistor
AAJT	A large temperature drop across the drier.
AALB	30 litres pr. nautical mile.
AAWE	lowering of at least one lifeboat after any necessary preparation for launching
ABAF	He has control of the navigation and movement of the vessel
ABAM	Cavitation
ABBG	Figure 1
ABDQ	Water Pump Pliers
ABEN	not less than 180m
ABFC	One long blast followed by two short blasts at intervals of not more than 2 min
ABHV	Forward breast line is given by C on the figure
ABKJ	By soft machine scrubbing with red pad and a renewing of polish only where there is heavy traffic (f.i. in the middle of corridors and not the whole floor).
ABLH	Yes, even if he/ she did not die while onboard.
ABPJ	The employer/master.
ACAJ	Secure hatches
ACBX	To avoid pollution.
ACGC	Ensure that the chart and the GPS use same datum
ACKJ	Chemical foams
ACMU	Atmosphere is not combustible in either situation.
ACPG	By smothering and also by providing some cooling 
ACXK	2 h, 2 candelas (about 1,7 mile range at normal meteorological sight) 
ACYL	Notify the Chief Officer or officer on duty and run the ventilation for at least 15min
ADLS	Charts, nautical publications, GMDSS log, Oil Record book(s)
ADNN	Machinery spaces of category A
ADTB	Because they wanted to make sure that the ship could be turned safely.
ADVC	Yes - any consular official can detain a vessel
AECJ	The water can be applied in a fine spray starting from the front in a sweeping motion.
AECL	Sodium Hydroxide Solution
AEFB	First aspect confirm death. Notify company, and next-of-kin, and if on board to be advised and comforted as may be required.  Arrange to have body moved to freezer area. Notify local agents and British Consul when abroad. Entry to be made in Record of Bir
AEKV	Every three months
AEMQ	Red
AENE	To prevent the steam and water in the boiler from discharging out by the feed line, if a feed line fracture or a joint in the line blows.
AEOG	To determine wether the ship is seaworthy
AEPT	Disperse or dissolve the oil into the water
AEPV	Yes, the bottles can be dumped if they are ground so that the resulting particles can pass through a screen with 25 mm openings
AFCL	5% by volume.
AFRF	routine
AFTY	select  the telex in on-line position
AFYY	When unsaturated chemical compounds are heated under pressure, the molecules react with each other and form large molecules.
AGCH	Flat file
AGEC	A tank is only to be considered as gas free when no traces of flammable and/or poisonous gas are measured and in addition O2 content is measured to be 21 %.
AGGL	All mentioned.
AGGM	Fairlead is given by C on the figure
AGLK	30 months / 5 years
AGRJ	Get out of the engine room as soon as possible. 
AGXI	High delivery pressure
AGYC	Specific heat
AHCF	does not sustain burning or continue melting after being totally enveloped in a fire for a period of 2seconds
AHCJ	This call will normally be followed by a DSC acknowlegment call
AHGM	Emergency Position Indicating Radio Beacon.
AHIC	23:23
AHIF	at least 12 distributed on both sides of the ship
AHJU	To avoid uncontrolled decomposition the cargo should be discharged overboard.
AHTR	The HSE has authority only where an interface exists between the ship and shore e.g. means of access regs. In a serious case, they would contact the local Marine Officer 
AHWA	Vessels with bulbous bow, LPG- and LNG-vessels must provide their own projector
AHWE	Panama lead is given by C on the figure
AHWF	Tell the jettyman to stop loading immediately.
AHXB	outside the sea areas A1, A2 and A3
AIGK	Good eyesight and able to communicate with the OOW (officer on watch)
AIHG	Water-tube boilers are more efficient and contains less water. They suffer from major damages when run dry during operation.
AIIW	The bottom washing starts whilst there is still a small amount of cargo in the tank.
AINU	Checking that passengers and crew are suitably dressed and lifejackets correctly donned
AINY	F1B
AIQE	Stop the washing process and not resume until the oxygen content in the tank is below 8%.
AISX	Near to the deck, crawl out keeping your face as near to the deck as possible.
AISY	Test pressure equal to 1.5 times the maximum allowable working pressure
AIWE	have separate draining pumps of sufficient capacity
AIWH	Start water-spray
AIXA	A 2 stroke engine has an ignition every time the piston reaches its top position.
AJBF	In Section 6 of the Act.
AJMX	Vitamin B
AJSP	SARSAT-COSPAS EPIRBS
AJUH	Every four years
AJWX	interrupt
AJXS	0,5 - 1 watt
AKAH	Cavitation
AKAJ	Insufficient amount of bowl closing water
AKFY
Any of the below
AKQA	At such locations that at least two jets not emanating from the same hydrant may reach any part of the ship normally accessible to the crew while the ship is being navigated, one of these jets coming from a single length of hose (the other jet may come from a connection of several lengths of hoses)
AKRP	During loading/discharging of persistent/non persistent oil?
AKRT	1 min
AKRW	the sea areas
ALEN	Orange
ALIJ	Yes.
ALUC	Public announcement system to be used for informing. The cabin attendant should proceed to their cabin section, and search all cabins. If the area is inaccessible report to their superior.
AMAX	two efficient painters
AMDH	Alarm instruction
AMDJ	Act according to the check list "during crude oil washing".
AMEG	G2B
AMGW	Employment agreement, report on seamen and documentation that the seafarer has the necessary qualifications, health certificate, record of service
AMHQ	He shall arrange for proper care within what he may find to be reasonable expenses
AMMR	Every 5 years
AMPX	In the cargo tanks we use either float or radar type gauge to control the liquid level
AMWO	Stretch a painter from fore to aft
AMYI	red 
ANBU	In the port where the occurance took place/ first port of call after the occurance took place - postponed only in exceptional cases and pursuant to provisions.
ANDG	starting and operating the lifeboat engine
ANML	Protect against corrosion
ANMN	Fresh water system failure
ANNG	Capacitor
ANOY	4
ANQS	Steering gear and alarm system
ANSH	As the piston passes "The Lubrication Points" in an upward direction.
ANSK	Decreasing the speed of rotation will decrease the discharge pressure.
ANSM	Rectifier
ANXC	The Chief Engineer
AOBP	Open steam valve very slowly, considering system expansion.
AOBR	Valve in the outlet line partly closed.
AODG	Immediately stop the discharging.
AOHG	Once a week.
AOHJ	The AB's Certificate (or equivalent), the seaman's discharge book, the medical certificate 
AOJD	17 - 20° C 
AOMD	Piston rod
AOML	2.15 V
AOQQ	Maritime Rescue Coordinating Centre
AOWN	Maritime Mobile Service Identity
AOYB	details of the general emergency alarm signal consisting of seven or more short blasts, followed by one long blast. 
APAO	The water level is between the water cock connection of the boiler, and the bottom of the gauge glass. It is safe to put feed water into the boiler.
APGH	Have all scuppers plugged
APGN	Notify Ch.Eng., find cause of leakage, remedy the leakage and then immediately start cleaning of the tank top.
APHL	Collect water/cargo to be pumped out
APKM	They are going to weigh the anchor
APKU	After 20 minutes
APLT	Collect rain water
APRH	20 000 dwt
AQAM	Sufficient amount for fifteen hours operation at full capacity
AQBL	The assistance of the vessel is no longer required
AQBN	the sun
AQCA	A thick rope to tie up the ship.
AQCC	OSC to be designated by an appropriate RCC or RSC.
AQEO	By soft machine scrubbing with red pad and a renewing of polish only where there is heavy traffic (f.i. in the middle of corridors and not the whole floor).
AQEY	1,5 Bar
AQHE	booster pump coming on the line and discharging properly
AQSA	Foam that is not a "alcohol resistant" type and water spray.
ARAF	Two lettres
ARAJ	10-200
ARGA	an EGC-message destined for ships of a certain company
ARGG	Means of Access Regs
ARJL	It requires less maintenance
ARMX	All answers
ARNT	Exhaust valve
ARQG	With IOPP certificate we mean International Oil Pollution Prevention certificate and the ship is classed to prevent oil pollution
ARSY	Jacket water cooler is clogged.
ARUM	No, food waste can not be dumped overboard
ASQC	Density, viscosity, flow rate, temperature, gravity disc diameter
ASQX	An approved hook with a locking device
ASUJ	Regulating freon liquid flow to the evaporator.
ASXU	position
ASYN	the direction of the electrical field
ATCS	The ITU List of Callsigns and Numerical Identities of Stations used by the Maritime Mobile and Maritime Mobile-Satellite Services
ATLV	be secured in a manner as not to interfere with abandonment procedures
ATVX	ground wave
AUAY	85% of the gas can be discharged into the space within two minutes
AUBY	8 minutes
AUDN	J3E
AUIH	Milk and cheese
AUIJ	user of the installation
	
AUNF	By producing and making available anonymous reports of incidents and accidents
AUSG	1 VHF RT + DSC+ DSC watch receiver - 1 or 2 SART - 1 NAVTEX and/or 1 EGC receiver and/or 1 HF NBDP watch receiver - 2 or 3 VHF portable - 1 EPIRB - 1 MF RT + DSC+ DSC watch receiver - 1 HF RT + DSC+ DSC watch receiver
AUYI	Oil Detection Monitoring Equipment.(ODME).
AVBU	the speed of light
AVCH	Lower the viscosity and improve purification.
AVDC	only to certificate holders
AVED	Applying 12 - 15% nitric acid on tank surfaces, either with a brush or spray; then washing off after 10 - 20 minutes using copious amounts of fresh water?
AVFY	At exits and in corridors
AVGT	They can have hold back hooks not subject to control station release providing the emergency plan details a person to close them.
AVGU	jump from a height of not less than 4.5m into the water without damaging the suit or being injured
AVHN	Ship's name, Official number, Length, breadth and draft, type of vessel, type and size of engine, name and address of the registered owner
AVOC	Air in the fuel oil system.
AVSJ	To prevent combustion gases to flow back and enter the burner.
AVXJ	A substance with a viscosity equal to or greater than 25 mPa.s at the unloading temperature.
AWAO	To improve the sealing surface between valve and seat during operation of the engine (compensate for the bending of the valve disc caused by combustion pressure).
AWAW	Salted meat and ham, potato dumplings, mashed swedes, boiled potatoes.
AWMI	Throughput too high.
AWPR	Broken water seal.
AWUU	Any of the mentioned alternatives.
AWWH	He is looking for navigational dangers.
AWXG	To ensure that the proper residuals of treatment chemicals, as specified, are maintained all time.
AWYW	The Master?
AXEV	NCS common channel
AXHH	On the Scene Co-ordinator
AXRH	To make sure gas pressure can enter freely on top of and behind the piston ring
AXSB	All the listed alternatives
AXTU	Slagging.
AXVM	Only when the design temperature is below -55oC and the tank is not independent type C , we must have full side ballast tanks
AXYU	Air draught is given by C on the figure
AYHH	nine digits, beginning by 4
AYOU	 2182 Hz
AYQI	High air/fuel ratio rises the condensation temperature, and thereby reducing the safe limits between normal operation and condensation temperature.
AYRG	Yes, one if the ship is under 500 brt. And two if the ship is over 500 brt.
BABO	Tell the deck officer to hoist the red flag. (letter " B ") day signal, or red signal light in the signal mast during night time
BABS	Checking that life-jackets are correctly donned
BACN	5 compressions after every 1 inflation
BADL	In case of major work the fire main shall be under pressure.
BAEB	Loading cargo "on top" of the oil and cargo residues in the  sloptanks
BAEY	in radiotelex-traffic in the MF/HF bands between ship and shore stations
BAFT	Fluids (liquids).
BAIE	one buoyant line, not less than 50m in length, of sufficient strength to tow a liferaft
BAIF	one set of fishing tackle
BAIG	All ships of 500 tons gross  and upwards
BAIH	Quay is given by A on the figure
BANY	must be replaced before the expiry date is exceeded
BAPV	the use of SART transponders
BAQT	To confirm to public supervisory authority that the requirements for the seafarer's service on board have been checked, are satisfied and that the compliance with the requirements has been duly documented.
BAUN	Semi-refrigerated gas carrier can be discharged by pressurising the cargo tanks or condensate the cargo to shore or another cargo tank or boil of the cargo
BAUP	Latex
BAWI	He will find a lubricating chart in the maintenance manual
BBAU	8 tons.
BBCC	a jack-knife attached by a lanyard
BBDF	Release gripes
BBHF	Permits the passage of vapor but not of flame
BBVQ	 A class fire door self closing
BCAR	Stop operation?
BCCE	Careful ahead manoeuvring
BCET	At the beginning of every watch
BCKQ	Carry out a risk assessment, make use of available equipment, and instruct staff on lifting techniques
BCLO	Isomer compounds is substances with same chemical formula but different characteristic
BCQL	Twistlocks?
BCTN	Milk
BCVP	For at least three years
BCXU	Calculation 3 is correct.
BDNB	He wants the Chief Officer to organise a lifeboat drill
BDPJ	Bringing the engine up to sufficient number of revolutions for combustion to take place and engine to run.
BDRD	All members of the crew
BDRI	Make the tug fast on port shoulder to pull
BDXV	Same as certificate to which it applies
BEJI	Use a water extinguisher to put out the fire
BEJM	Reject the offer?
BELE	Bleed off may be taken from any of the cargo pumps.
BEOP
By muster lists exhibited in conspicuous places
BEXX	Send a distress message and collect survival suits / thermal bags.
BFBF	Rocket parachute flares
BFCW	if the whip-antenna is replaced by an antenna of about the same length as the original one
BFDT	Identify the extent of damage to own vessel and take necessary steps to safeguard the complement and the vessel.
BFEN	Tug towing line is given by D on the figure
BFGX	Too high amplification
BFGY	The Chief Officer wants the 1st Engineer to empty the starboard bilge in hold No. 5
BFHQ	She will turn to port and the speed will drop gradually
BFHW	That the combustion chamber of the boiler is checked being empty for oil and that the pre ventilation function prior to  ignition is functioning.
BFIK	By soft machine scrubbing with red pad and a renewing of polish only where there is heavy traffic (f.i. in the middle of corridors and not the whole floor).
BFIN	don a lifejacket without assistance
BFIR	All the mentioned alternatives.
BFJI	Pre-wash the tanks with cold water first?
BFKF	Ammonium nitrate?
BFNO	an efficient radar reflector (or radar transponder)
BFQW	an EGC-message destined for ships with the same group call number
BFSL	No openings in sides and bottom
BFTH	6 air changes per hour
BFTI	To minimize the scale formation, the Sea Water outlet temperature should never exeed 50 C
BGBB	Fuel with a flash point of 44°C or more
BGDM	They have had problems securing the gangway
BGJK	Lube oil cooler
BHFX	rescue boat
BHIJ	326.6 Mt
BHSE	A signal representing 0 = "low" and 1 = "High"
BHTC	fading
BHTY	5 - 10 Degr. C.
BHUW	Protecting cloths, safety shoes, gloves, goggles, earmuffs.
BHWN	On area A1 this function is based on the use of SART transponders
BIND	Minimum eight crew members.
BINY	be secured in the lifeboat (except boat-hooks) by lashings, storage in lockers, compartments, brackets or similar arrangement
BIOW	100 ohm at 0° C 
BIPR	In case of bursting pipe, to avoid oil spray hitting adjacent high heat surfaces of exhaust pipes etc.
BIUQ	Radiotelephony - Single sideband suppressed carrier
BIWP	lifebuoy
BIYB	That the MARVS is less than 0,7 bar
BJJW	No, the sea water pumps are still running
BJKR	Swelling below the bandage and heavy pain. 
BJPV	Controlled closing of fire doors
BJRE	A deck officer or certificated person shall be placed in charge of each survival craft to be used.
BKGJ	When the design temperature is below -55oC and the tank is not independent type B or C, we must have full secondary barrier
BKGK	40 meters
BKKM	Improve the scaling surface function, increase the service time of the exhaust valve in the engine.
BKNU	245329000
BKQG	They will be closed if the ship get a damage on the ships hull, and taking in water. It will prevent the water to fill the whole deck. In case of fire they can also be used to stop the fire and smoke from diverge.
BKTW	A device which prevents an operation of  equipment to take place, to allow access or maintenance to be carried out
BLAK	Maximum cargo tank pressure on an fully refrigerated gas carrier can be 0,7 bar
BLAR	Channel 16
BLBF	Ionisation.
BLCD	SOLAS
BLDC	Radar transponder
BLDX	a sea-anchor with a hawser of more than 10m in length
BLFH	Atmosphere is not combustible in either situation.
BLGF	To relieve excessive high pressure in the cylinder to protect the engine from being damaged.
BLIR	406,025 et 121,5 MHz
BLWW	Making the grab bucket open and close.
BLXA	Line throwing appliance
BLXW	VHF / W-T  
BMES	Radiotelex and DSC - Frequency shift keying of carrier with error correction
BMIR	In G3E mode - on duplex basis
BMKP	Sufficient amount for 15 hours of operation at full capacity
BMLK	To neutralize the acids occurring in the condensate system.
BMTQ	-   4° C
BMWY	EPIRB
BNEO	Channels 6, 13 & 16
BNKJ	Excessive cooling water velocity
BNLE	Figure 1
BNOQ	Potentiometer, 10 kilo-ohms                                            
BNPF	Increase the dosage of chemicals, and take new test of the water.                               
BNUC	the use of VHF DSC
BNXP	The main purpose with booster pumps is to increase the manifold pressure
BNXR	No, membrane tanks is normally designed for transport of fully refrigerated cargoes
BOGC	weekly
BOGV	Figure 3
BOIO	brass knife
BOIQ	Act according to the check list "during crude oil washing".
BOKC	When a Panama Canal pilot is onboard
BOLT	The method and use of sea-anchors (drogues).
BONM	Survival suit and lifeline
BOTH	Check that the painter is made fast to a secure point and that the sea below is clear
BOTI	a DSC-message for all vessels within certain area marked by areference position, given in the DSC message and the degrees are given in southerly and easterly direction
BOTK	List of Call Signs and Numerical Identities
BOXP	There is 5 special area where it is forbidden to pump out any sludge or oil residues
BPDK	It could poison the fresh water if leakage occurs.
BPEX	Because they expected the harbor pilot to board the ship at 0730.
BQAQ	Stop all cargo operations and close the deck IG line isolating valve
BQAS	The Gulf of Mexico
BQCL	Secure hatches
BQDK	Lubricating oil.
BQFB	MF
BQFY	All the answers are good
BQIE	MCA
BQKT	Yes
BQNG	That the shipowner is a Norwegian subject or fulfils other requirements stated in Norwegian acts
BQQR	A number of lifejackets equal to at least 10% of the total number of passengers and crew to be placed in the vicinity of the muster stations
BQRJ	-79?C
BQYD	Connect bonding cable then connect hose.
BRCF	the use of MF and/or VHF R/T
BRDD	NAVTEX-receiver
BRJT	Bridge is given by A on the figure
BRKR	Upper Flammable Level / Lower Flammable Level of  explosive atmosphere?                                                     
BRKU	Anti-alcohol foam
BRRN	Reduce motor speed by about 10%
BRUR	Do not carry lighters or matches on the tank deck.
BRXD	Separation with correct temperature and low flow rate.
BRXF	Either of the mentioned alternatives.
BRYX	After 20 minutes
BSAQ	distress alerting
BSDA	with weak incoming signals distortion is reduced
BSFK	a liquid that mixes with water
BSHD	Metals 
BSJY	If time permits, send someone to try to find him. Notify the agent. Have the seaman's possessions collected and packed by two crewmembers, with three lists of contents. Notify the company.Sign the seaman off in his absence, detailing reason for him/her no
BSME	Too lean ( less than 2% by volume of hydrocarbons) or over rich ( in excess of 15% by volume of hydrocarbons ).
BSMJ	Both persons in charge
BSNH	Figure 1
BSNI	Figure 1.
BSPO	anti-seasickness medicine and one seasickness bag for each person
BSTU	The Secretary of State responsible for Shipping
BSVJ	L(S) =     4 H
BSVK	The Master?
BSYR	Provisions on maritime inquiry and death and burial.
BTBL	gases, flames, smoke and heat
BTES	It allows the wearer to jump from height of at least 4.5 m into the water without injury and without damaging the life-jacket.
BTHE	The Part Flow System makes it possible to observe the discharge visually for oil content, on older tankers with discharge below the waterline
BTKK	Constructed of non-combustible material
BTNT	Tank top
BTOO	loss of suction
BTPM	Air from stage one goes through discharge valves in stage one and through suction valves into stage two. In stage two it will be compressed to high pressure air.
BTTW	the applicant on board wishes to have a conversation with a person whose name is known
BTVE	9 digits
BUAI	Before the tank is entered, lifeline, rescue harness and compressed air apparatus shall be ready at the relevant hatch.
BUAK	Once a year/18 months
BUCX	30 L/nm
BUDW	Airway  Breathing Circulation 
BUFM	Plan for safety preparedness
BUGD	requesting an "automatic linetest"
BUOO	It confirms that a ship has been "carved" and allows the Ship's Register to be issued
BUOR	16 times 0,17 SDR
BURD	Ensure adequate circulation in all conditions of steaming.
BUWV	322753810
BVES	Two
BVJN	VHF-channel 87
BVJQ	Muster and embarkation stations shall be readily accessible from accommondation and work areas.
BVKI	Liquefied gases is defined as chemicals with vapour pressure above 2,8 bar absolute at 37,8oC
BVQC	10 minutes
BVTJ	Yes, a ship can be detained on hygiene grounds, but it is more likely that after inspection the hygiene officer would call in other inspectors
BWEG	the nature of distress is unknown
BWEI	listen out on VHF channel 16
BWKE	Excessive cooling water velocity
BWKG	As a safety net, for improved cleaning of the fuel oil
BWLW	60?C
BWSO	Either of the mentioned alternatives.
BWVB	All those listed in the other alternatives
BWWT	85 - 90 Centigrades.
BXFY	All personnel onboard (crew and passengers) must be registered to keep a track of number of people onboard.
BXKD	equipping of the survival craft
BXPC
As near as possible to the ship's manifold?
BXUA	Figure 1
BYAU	By use of a float switch or differential pressure in the liquid receiver
BYIN	U.S.A
BYKV	A throughput of at least 400 litters a minute and  a "throw" of 15 metres?
BYKX	Do nothing.
BYKY	On area A4 this function is based on the use of  HF R/T
BYMI	Cinnamon
BYMK	2187.5 and 2182 KHz
BYSG	at sea, outside territorial waters, and in a port or harbour
BYSN	Yes, on a form prescribed or approved by the Norwegian Maritime Directorate
CABB	Viscosity.
CABE	2182KHz
CABT	All of the mentioned actions
CADH	Alarm, st.by start, slowdown. shutdown
CAFE	White or light grey to ensure all minor spills and leakages are noticed and dealt with.
CAFG	Where the ship has passenger spaces below the bulkhead deck
CAGF	Ahead is given by A on the figure
CAGV	Exhaust gas temperatures are higher than normal.
CBAH	As instructed by the helicopter pilot
CBBT	About 80 %
CBEC	Someone of at least school leaving age and less than 18
CBHK	Search and Rescue radar transponder
CBHQ	Maximum 8 hours per day, or 40 hours per week
CBJF	once a month
CBTH	Walk to a smoking area inside the accomodation?
CBUI	Report to the chief officer or chief engineer.
CBYE	12 h
CCCT	In ports only
CCEH	200 cm
CCML	6 times the hose diameter.
CCNF	Leave him in bed or request him to have some fresh air.
CCOE	Broken water seal.
CCOF	Emergency shut down.
CCSF	You set watch on channel 2182 KHz
CDBN	Solid, liquid and gases
CDJY	Provide a replaceable wear surface for the pump housing/impeller.
CDRH	Computer-aided maintenance
CDVT	Air from stage one goes through discharge valves in stage one and through suction valves into stage two. In stage two it will be compressed to high pressure air.
CDWF	A duly completed application with certificate etc. must be made to the public supervisory authorities as an endorsment/ qualification document
CDWK	Automatic gain control
CEBM	Too little gas in the system.
CEHB	AVR and speed governor
CEIB	98 Centigrades.
CEIC	CO2                                                                                  
CEJU	Because they wanted to make sure that the ship could be safely turned.
CEME	Ship owner has Document of Compliance issued, and vessel is assessed and holds all statutory certificates
CEOV	VHF and MF
CEPQ	Because a cook handles food and beverages and could easily be a spreader of viruses and infections.
CETS	For minimum 3 years
CETX	measured by the "dopler" shift in the signals
CFBL	Because he was married.
CFBM	All answers are goods
CFDU	Allow removal of the sensor also when liquid is flowing in the pipe.
CFGH	When manoeuvring?
CFHB	R(L) = R(s)
CFOP	Strainer in operating water low-pressure side is clogged.
CFSA	They will be closed if the ship get a damage on the ships hull, and taking in water. It will prevent the water to fill the whole deck. In case of fire they can also be used to stop the fire and smoke from diverge.
CFWG	A bolt in every hole
CFXD	They can bring any seafarer involved in an incident on the UK coast to court and provide evidence regarding the incident
CFYN	To obtain a proper sealing and correct distance between piston and cover in TDC position
CGAH	1:4
CGAJ	The smallest diameter piston is the stage two piston.
CGDW	F1B
CGER	a manually controlled lamp fitted on the inside
CGON	Report to bridge or duty officer, actuate the fire alarm, call the persons around the fire and join the fire squad
CGUH	Insulated on both sides with approved non-combustible material
CGXS	The clearance between the rocker arm and valve pushrod.
CGXV	He should be aware of the steel thickness of the valve
CHHV	Donning of fire protection clothing
CHMA	Stop discharge, inform USCG and Qualified Individual.
CHNU	A 2 stroke engine has an ignition every time the piston reaches its top position
CHPK	With this type of material the hatches should not be battened down.  The fire can only be extinguished by using large quantities of water. 
CHQA	doing a "linktest"
CHQC	a light plus a whistle
CHRB	Make it possible to retain most of the recovered oil in the primary slop tank, while cleaner part of the water will flow into the secondary slop tank, where it can be re-used as wash-water
CHRU	The speed should be less than 5 knots, normally 3 - 5 knots
CHXS	Safety shoes or safety boots
CHYN	adjust the threshold level for admitting signals and refusing noise
CIAG	All of the mentioned equipment.
CIIO	Chemical, physical or mechanical foams
CIMU	1.25 times the maximum working pressure
CIPM	All alarms are reengaged prior to switching to UMS-mode
CIUK	1 year
CIUL	month
CJLY	the use of SART transponders
CJNM	Great circle
CJNR	the height of the antenna
CJUB	Deck cargo shall not block emergency exits or exits from accommodations or machinery spaces.
CKAU	One minute.
CKAY	0.7 bar?
CKBY	Yes, the turning diameter will increase if I reduce speed
CKFA	Comparing input and output values against a documented standard
CKHN	20 seconds or less
CKHS	75 Kg
CKIH	it allows the wearer to jump from height of at least 4.5 m into the water without injury and without damaging the life-jacket
CKII	48 hours
CKLT	MAYDAY
CKPA	Prevent excessive furnace heat losses
CKPX	In case of a bursting pipe, to avoid oil spray hitting adjacent hot surfaces or coming into machinery air intakes
CKRM	Periods not exceeding 3 months
CKSH	15 compressions followed by 2 full ventilations. 
CKSJ	Diamond and graphite.
CLAV	The water supply hoses contain internal wires that act as conductors
CLIB	Allow for increase in water volume
CLNB	are a fire hazard because they are liable to spontaneous combustion
CLPR	All of these.
CLUS	At least two sets of instruments to detect each type of gas expected to be encountered?   
CLUU	Blow  the boiler and renew water until the PH-value is normal again.
CLWK	40 gr of each
CLYV	The master of a  ship who coordinates on scene search and rescue operations
CMET	kkkk
CMJB	Not more than 10 minutes
CMLL	The Master
CMOA	For all vessels.
CMTS	all sea-areas (A1 to A4)
CMWC	Quay is given by A on the figure
CMWH	Port quarter is given by D on the figure
CNLM	They tend to contain heavy vapours inboard during cargo operations?
CNNX	A sink is always needed irrespective of the type of the dishwashing machine provided.
CNOS	Above the bulkhead deck
CNQG	only be given receipt when the ship is actually able to give assistance
CNQH	watertight, as far as possible,except for drain holes in the container bottom
CNSU	Diesel oil leakage to the lub oil system. 
COHG	 All the mentioned alternatives
COHV	To the Master
COJV	Vitamin C
COKQ	Immediate availability of water for at least one effective jet of water from any hydrant in an interior area
CONY	always passed on to a LUT
COOQ	the volume
COVL	The two gases is Freon 22 and carbon monoxide
COYW	all the answers are good
CPAK	Endeavour to hold the anchored/yawing vessel steady
CPDR	Any of the listed alternatives.
CPEQ	The difference between possible maximum and minimum measurement
CPIY	If any of the main registered particulars e.g. length were changed
CPKJ	ability to make weak stations audible
CPLH	Act 18 June 1971 relating to enrolment of employees on board ships.
CPNV	almost rectilinear
CQDW	The "Abandon ship" signal is not specified, only the general emergency alarm signal is stated
CQHR	The Norwegian Maritime Directorate
CQUI	Once every month
CQXU	Caps and cocks should be closed at all times, to prevent ingress of water into the engine room in case of tank bottom damage.
CQYK	Lenght overall is given by B on the figure
CRBD	all of the alternatives together
CRBQ	Smoke going out the stack
CRCR	is intended for radio traffic onboard of the own ship
CRIL	have permanent boarding arrangements on both sides to enable persons in the water to board the lifeboat
CRQB	Give the coating time to "weather out" the trapped solvents using good ventilation, and recover it's hardness again, prior loading the next cargo?
CRQT	Pressure to electric current converter.                              
CRRP	Check the ballast tanks for oil after the ballast tanks have been filled
CRTJ	Distress traffic, urgency traffic, safety traffic
CRUE	be made of fire-retardant material
CSFC	F1B
CSGX	nine digits, beginning by 6
CSOC	MAYDAY RELAY
CSOE	To avoid the compressor-oil  to disapper from the crankcase during starting.
CTCN	Separation with correct temperature and low flow rate.
CTDH	To prevent serious damages on main components.
CTLR	Use the rudder hard over both sides while reducing engine power, so-called "high frequency rudder cycling"
CTTE	Crankshaft
CUAR	To prevent freon condensing when the compressor is stopped.
CUBK	All the items mentioned
CUCF	Too fast
CUCG	On the fire control plans
CUCJ	R(S) =18 ohm
CUFX	1.15 Ohms
CUYC	Floor space is usually more valuable than height.
CVAP	It should be avoided, unless the tank atmosphere is inerted.
CVNA
All the spaces mentioned
CVOV	A manually operated release system only
CVTQ	At least once a watch
CVTV	Serial adapter
CVXD	It satisfies the SOLAS requirements for ship safety
CVXG	Into the crankcase and mix with the lube oil.
CVXY	The bows of the ships will be pushed away from each other
CVYY	Method to measure alkalinity and acidity.
CWBD	The number of persons should be clearly stated on the outside of the boats bow.
CWNW	To improve the sealing surface between valve and seat during operation of the engine (compensate for the bending of the valve disc caused by combustion pressure)
CWOQ	As low as possible.
CWTR	Fire is easily spread in dust and trash and wet floors may cause different accidents.
CWTT	Radio Regulations
CWVH	Connect to the hydrant before lowering the machine into the tank.
CWWY	MCA, Lloyds Register, Bureau Veritas, Det Norske Veritas, American Bureau of Shipping, Germanischer Lloyd, Registro Italiano Navale
CXDQ	To prevent freon condensing when the compressor is stopped.
CXSS	Pushing on ship's flat side and make fast in the vessel for pulling if needed
CXXR	the identification of the vessel in distress and her position
CYGF	The atmosphere should be gas free and contain at least 21% oxygen. 
CYGG	95 Celsius
CYHA	Gravity disc is too small. Flow rate is too high
CYJI	Lubricate the piston rings.
CYKL	Cover all exposed parts of the body, protect the area, move people  and if possible use a compartment with extraction fans:
CYVA	Floor space is usually more valuable than height.
DABD	the O.O.W deems it necessary
DABI	Mackerel
DADR	Heavy fuel oil leakage to the lub oil system.
DADV	To allow at least 3 hours of operation
DAPI	Seven or more short blasts followed by one long blast
DAQE	2
DAVJ	1250 m3
DAYP	15 minutes
DBBK	1 litre
DBOR	summoning of passengers and crew to muster stations with the alarm required
DBRD	By double blank flanges with a drain between them?
DBSU	Bollard is given by D on the figure
DBUF	10% of the number of persons the liferaft is designed to carry, or two, whichever is the greatest
DBWC	Stop discharge.
DBXA	Stuffing box.
DCAJ	The dispersing additives in lubricating oil, break up the contaminants in even smaller particles and keep them in suspension
DCJM	 Space protected by foam
DCKH	3150 m3 per hour.
DCLC	Portable bridge between ship and shore.
DCQB	Starboard bow is given by A on the figure
DCQC	muster station
DCQD	To keep the valve in correct position and to maintain proper sealing.
DCSL	When you put rudder amidships, she will continue on a straight course
DCSN	Seafarers employed or engaged on board ship on the business of that ship as part of the ship's complement with designated safety or pollution duties 
DCVC	uncompanded channels
DCXP	Open the flue gas isolating valve
DDGB	The installation shall include equipment for radiotelephone communication on distress frequencies in addition to working frequencies
DDIQ	2 sec
DDMT	it has windows to admit sufficient daylight inside the lifeboat with the canopy closed
DDNQ	Use the "cleaning in place" arrangement to open the heat exchanger for visual inspection and manual cleaning.
DDTI	to exclusively receive MSI-reports meant for the NAVAREA where the vessel is
DECL	The diesel speed and excitation current.
DECM	Check the cargo tanks for water prior to loading
DEJE	100 mm/water gauge.
DENE	To isolate the fuel source before extinguishing the flames on a gas fire
DERP	It is both a prevention and protection measure
DEVQ	A carbon dioxide (CO2) system
DFCK	There must always be one man on the ship's manifold, operating the manifold valve in order to avoid to much pressure raise in the tank.
DFDI	By muster lists exhibited in conspicuous places
DFHM	Proportional + integral  (PI)
DFLS	FEC mode
DFMI	Glycerine is compatible with both of the other cargoes.
DFPX	Non-combustible material
DFQS	21% oxygen by volume and 0% hydrocarbon of LEL.
DFSN	Carbon dioxide
DFTX	45% of the total volume of the space
DFXE	Thermocouple sensor
DFXG	Figure 2.
DFYB	25, 45, or 70 mm
DFYE	All the listed alternatives
DFYJ	until - 15°C
DGGM	All the mentioned alternatives.
DGII	Lower lifeboat to water
DGKR	Adjustable wrench
DGLL	Start with intermittent firing, using small firing periods and long intervals gradually building up to longer firing periods and shorter intervals.
DGRI	3 sets
DGRL	At all times
DGRN	A short circuit occurs between earth faults and the ventilation fan fuse blows
DGTC	Conductivity test.
DGTV	Two prolonged blasts on the whistle at intervals of not more than two minutes
DGXC	Clearing escape routes
DGXD	Lower explosive limit.
DGXM	Safety call
DHIB	Reject it?
DHJB	Trip/stop all nonessential loads that are connected to the switchboard
DHKT	summoning of passengers and crew to muster stations with the alarm required
DHNG	1.44 MB
DHPR	Starboard quarter is given by C on the figure
DHUV	a painter attached to the release device and placed at the forward end of the boat
DIEP	Harness with a rope secured to a safe point on the ship.
DIHC	Aft part of the tank-deck
DIKM	To obtain a proper sealing and correct distance between piston and cover in TDC position.
DIKP	1.5°C per hour after the first 0.5h immersion in calm water at a temperature of 5°C
DIKR	A transducer that converts a known electric current to a  pressure proportional to the current.
DJDA	The ship's master
DJDV	The signal out from a thermocouple is mV,and can not be transferred over any longer distance without loss of voltage, giving a very bad accuracy.
DJFM	A thorough ventilation of the combustion chamber before the ignition takes place.
DJGL	1,3 Bar.
DJJP	safety belts to be designed to hold a person of 100 kg securely in place with the lifeboat in a capsized position
DJQG	How to muster at the assigned stations
DKKG	A combination of hydrocarbons.
DKQF	Checking the moorings for tightness/slack.
DKWV	The entering permit shall be based on the check-list for gas freeing and check-list for equipment and preparedness.
DKXP	Survival craft distress pyrotechnic signals
DLCB	Radiotelex and DSC - Frequency shift keying of carrier with error correction
DLDN	A unit composed of trained personnel suitable equipped for expeditious search and rescue operations.
DLGB	FleetNET
DLGY	70
DLJM	Every 5 years
DLNN	The same as suction pressure.
DLVY	Very large crude carrier.
DMDI	A 60
DMFA	On the fire control plans
DMGW	Multistage centrifugal.
DMKV	A receipt issued by the Chief Officer, stating quantity and condition of goods loaded onboard?
DMUE	SART transponder
DMVB	skates and fenders to facilitate launching down the side of a ship
DNJE	8 hours
DNKB	They are liable to spontaneous combustion.
DNLN	It will try to reduce the deviation between set-point and process value
DNNI	We are controlling the process inlet side
DNOC	The main supply valves in the deck storage are closed prior to switching to UMS-mode
DNSL	Weekly
DNSN	2912 hours
DOAB	8364 kHz
DOBR	3
DOBS	Weather on-scene.
DODH	Reduce speed and use soot blowers if some are fitted
DOFY	The location and capacity of all fuel and cargo tanks on the vessel
DOGT	At least four sets
DOHO	Call the bridge and request for position and  permission to discharge overboard through oilywater separating and filtering equipment.
DOKA	one boat-hook
DOOF	15 m
DOOU	immersion suit
DOPY	Yes, all crew must be able to communicate on the language spoken by the majority of the passengers, or demands set by the company.
DOTF	Emergency lighting
DOWR	One for each person on board who is not provided with an immersion suit
DPAO	Sinkage is the change in draft a vessel obtains when moving through the water.
DPEX	always allowed
DPHL	Name of every crew member, reference number, name of last ship, home address, next of kin, date of signing agreement, date of discharge
DPMI	Density, viscosity, flow rate, temperature, gravity disc diameter
DPOW	At all times when identified as a control method with risk assessment
DPWH	Nitro glycerine tablets.
DPYV	when its area is of 4m? or more
DQAI	Radiotelephony - Single sideband suppressed carrier
DQEU	LUT
DQIC	For personnel assigned to shipboard duties.
DQKN	In emergency generators
DQSB	It will move aft as the ship slows down
DQUJ	Stop the separator and drain the water from the tank
DQUN	1 member
DQUP	When the boiler is firing on high rate.
DQVH	4-20mA/3-15 PSI
DQVN	A period not exceeding 48 months
DQWG	Discharge the washing to shore reception facilities only?
DRIU	The temperature is equal to or over the flash point
DRKO	Change the lube oil.
DRKP	8,3 - 9.
DRMB
The appointed lifeboat commander
DRMV	1100
DRVC	the use of HF DSC and INMARSAT C SAFETYNET
DRYM	Any of the others.
DSIQ	Direction B
DSIY	Pilotage is compulsory and the pilot is only the master's advisor
DSPL	Radiotelephony - Single sideband full carrier
DSVC	Ensure all doors are in closed position.
DSYM	7
DTBA	Three years after the last note was made
DTBG	Figure 2
DTEH	To store quantities of oil at working pressure on the discharge side of a pump and smooth out any pressure fluctuations.
DTHW	Fixed known objects on the shore
DTIR	Notify Master, Deck officer and engineer in charge.The loop for this special sensor to be switched off and take normal precautions for hot work.
DTRU	FEC
DTSU	Separation with correct temperature and low flow rate.
DUAG	Pressure-relive valve setting should not be less than 0.2 bar for gravity tanks.
DVGA	Faulty governor.
DVHQ	At least once every month by a responsible officer and once every year by an expert?
DVUW	Three hours
DWBT	Insufficient amount of bowl closing water
DWFA	The three international conventions that cover the shipping trade is SOLAS 74/78, STCW 78/95 and MARPOL 73/78
DWGW	Steel or stainless steel.
DWKU	Use protective equipment where necessary.
DWOF	Capillary tube
DWPW	Yes, all kind of food waste can be dumped overboard
DWRP	Rotterdam, the Netherlands
DWYY	Lower lifeboat to water
DXBP	Fixed CO2 fire-extinguisher system
DXLK	Easy accessible by the gangway
DXND	is within radio traffic range of at least one VHF- coast station where continuous DSC-alerting is available
DXRL	it allows the wearer to jump from any height without injury and without damaging the lifejacket
DXUT	Once every month
DYBF	Remove any oil or scum on water surface
DYCH	10 minutes 
DYHB	S-Band Radar.
DYHH	200 gr
DYIY	To by-pass, adjust and isolate all machinery that is to be worked on under his supervision.
DYLL	 All Stations - This is "SAINT-ROMAIN"
DYOS	unknown
DYSA	The types of compressors are piston, screw or centrifugal type
EAAC	arrangements for providing an adequate view forward, aft, and to both sides
EAHL	20 metres
EAKC	All working spaces accessible by the crew
EATY	From the condenser.
EAUS	A contract between Master/Owner and Shipper for transportation of goods?
EAWN	is fitted with a light and a whistle
EAXB	a possibility to receive MSI
EBAU	It is the number of revolutions, and the one used on the cargo is oil-free
EBAV	We use inert gas to purge out cargo vapour and have a neutral atmosphere in cargo tanks and spaces
EBLR	Have one slack tank as last tank
EBOE	The blower air inlet
EBOX	1) 5 tons  2) 5 tons
EBPS	In case of accidents, it is important that a wide range of personnel must be permitted and trained to operate the pump.
EBRI	Cargo holds and engine rooms
EBWH	Freeboard is given by B on the figure
ECAT	The speed of the shock wave created by the initial combustion
ECHF	Passenger ships, ro-ro's, bulk carriers, ships which may present a special hazard ships which have had several recent deficiencies and ships flying the flag of a state appearing in the 3-year rolling average table of delays and detentions
ECKQ	Sugar lump, sugar drink or something sweet.
ECLL	Safe working load
ECMI	Bi-stable flip-flop
ECOS	+ 4° C
ECSD	The meteorological station connected with the CES used
ECSV	immersion suit
ECTR	Cut it with the safety knife stowed on the exterior of the canopy close to the painter attachment point
EDCE	Making the crane jib move from side to side.
EDFH	must not be passed on
EDHG	No. More readings should be taken and sediments, sludge and residue should be removed at least 10 m from working site.                                                            
EDKO	On the cargo tank area all time?
EDPP	automatically comparing the message earlier received ones
EDRB	Because certain types of dry powder can cause breakdown of a foam blanket
EDWG	Centrifugal force
EDXV	1620 Mt
EEAM	Ensure all doors are in closed position.
EEBG	3 litres
EECD	He is asking about the position of the chain
EECH	Not allow the clothes to be hung anywhere in the unmanned machinery spaces.
EEDP	All the answers are good
EEFI	Merchant Ship Search and Rescue Manual.
EEHC	Go to your lifeboat station (muster station).
EEYR	Raise the feed water temperature.
EFAD	To lubricate and cool the engine.
EFBE	a license
EFFH	also after 1 February 1999
EFHP	No, only those listed in the Seamen's Act as dereliction of duty.
EFHR	The deck officer of the highest rank present
EFOM	To respond to oil pollution and take appropriate action as may be necessary
EFRB	Three months.
EFRC	Stop the bunkering until  safe communications are established
EFVH	geostationary orbits
EGBB	In the muster list.
EGCP	VI
EGHM	The deck log book
EGNI	Risk of deposits on heat transmitting surfaces.
EGNN	all of the above-mentioned
EGOG	In and outlet temperatures, and flow rates for both media
EGSU	the use of VHF DSC
EHEB	Exhaust valve
EHLP	Herring
EHMQ	Daily
EHNJ	4 - 5°  C
EHQX	two boat-hooks
EHVA	Valve in the outlet line partly closed.
EHWT	The use of devices for protection in launching areas
EICL	Make sure that the compartment has been evacuated
EIGQ	2
EIHP	Centrifugal separator.
EIQQ	The way to board, launch and clear the survival craft and rescue boats
EIXM	At all times
EJAA	In suitable lockers easily accessible, yet segregated  from the living spaces themselves?
EJAR	+ 18.5 bar
EJBR	The stevedore superintendent?
EJCH	Turned at intervals of not more than 30 months and renewed every 5 years
EJJC	1 year
EJLQ	As a safety net, for improved cleaning of the fuel oil
EJQO	burn with a bright orange colour
EJYA	Temperature-control
EKAR	Sweep holds clean first and lift out solid residues manually prior washing. After washing again lift out remaining wet residues after carefully stripping out only the accumulated water?
EKCB	Radiotelephony - Frequency modulation
EKEX	Nine digits, beginning with a four (4).
EKLM	4
EKLO	1.5 litre
EKTV	The vessel anchoring assumes responsibility
EKUL	Liquid at high pressure.
EKUQ	Leave the engine room immediately.
EKWG	Line throwing appliance
EKXF	Between 3% and 6%
EKYY	75° C
ELDW	There are three main reliquefaction systems, Direct cooling one to three stage, direct cascade cooling and indirect cooling
ELER	Maximum allowed Oxygen content in the inert gas on gas carriers is 5% by volume.
ELOQ	Leakages from seawater coolers 
ELOW	10 minutes
ELPL	Differentiator                                                                   
ELPO	Anchor watch responsibility rests with both vessels, each with its own watch
ELQP	Because that was the safest passage considering the ship's draft.
ELTY	Milk
ELUK	One fire hose forward and aft of the manifold, and portable fire extinguisher near to ships manifold?
ELVJ	GMDSS
ELXB	the use of HF DSC and INMARSAT C SAFETYNET
EMBD	To remove the oxygen and by that avoid a chemical reaction.
EMIR	With the pointer of the synchronoscope at 0° (12 O'clock) and both synchronizing lamps dark (off)
EMKK	The Flag State language with copies in English or French
EMKL	tools for minor adjustments to the engine
EMLN	preparation and launching of the survival craft
EMMF	Yes, by putting the rudder hard stb. it will shield waterflow to the stb. side of the propeller and vice versa to port, this will effect turning of the ship
EMON	220 liter
EMRE	Lifejacket
ENBF	Obtain permission from charters and note procedures in oil record book and deck log
ENCD	Have the engine ready for immediate manoeuvre and adjust speed for safe navigation
ENCX	12 - 16 times per minute
ENGE	At all times
ENHX	The pressure switch has contact(s) that will change between open and closed position.The pressure transmitter converts a pressure signal into an electric signal.
ENIY	Drainage/waste from toilets/urinals.
ENJG	By visual and audible signal at the control panel and indicating units
ENJT	Every 12 months.
ENLD	500 kHz, 2182 kHz and 156.8 MHz
ENMD	2275300
EOBE	15 percent.
EOBS	3.5 - 3.9 %
EOCW	To avoid unexpected oilspill
EODR	Astern is defined as D on the figure
EOEQ	Periodical survey every 12 months
EONQ	How to recover survival craft and rescue boats including stowage and securing
EORC	98 %
EOXS	All alternatives
EOYL	Secured via a weak link to a secure part of a ship
EPAE
a searchlight which can work continuously  for not less than 3 hours
EPBT	Sugar
EPEH	number of vibrations per unit of time
EPEJ	Passenger ship initial surveys, Initial surveys of a Certificate of Fitness or International Noxious Liquid Substances Certificate and initial surveys for SEC or IOPP, and all radio surveys.
EPFC	TX: 2189.5 kHzRX: 2177.0 kHz
EPIM	location of embarkation ladder
EPUE	Design temperature on the cargo containment system on a LPG/LEG carrier are -103oC
EPWO	Reserve accumulator battery for two hours normal use to be provided
EPXN	Put the plates in water with qualified cleaning chemicals, and use soft brush, or high pressure cleaner with care.
EQAW	Goggles and shield.
EQBV	2
EQLQ	The load that can be safely lifted during normal working conditions.
EQPD	LIC
EQRN	2.0 bar
EQRQ	A ship with a length to beam ratio less than 5.5
EQTB	2 valves
EQTD	Liferafts intended for throw-overboard launching shall be stowed amidships secured to means for transfer to either side
EQYE	warning the passenger
ERAT	Foam.
ERIM	Increase.
ERJE	On the main beam
ERLQ	At least four sets or more depending on the type and the size of the vessel
ERNF	Leather safety boots and gloves
ERXD	 Yes, showing how it has been calculated and with possible deductions.
ERXJ	To ensure that we do not have any water assembly in the cylinders when the compressor start.
ESCJ	Sufficiently manned with officers and crew to permit safe handling of vessel
ESCK	no fault - hard earth - light earth
ESEA	Clean the system and change the oil.
ESFO	The input impedance is made much larger than the output impedance                                                             
ESGN	feet
ESHH	two buoyant rescue quoits with buoyant line
ESIY	Call immediately the person in charge.
ESOT	distress alerting
ESOV	a book of directions for search and rescue at sea
ESPO	at any moment before the ship proceeds to sea
ESUM	All valves on the delivery side and adjust the propellant pressure.
ETBH	Varying the excitation field strength by regulating excitation voltage/current
ETES	When coming up with another vessel from a direction more than 22.5 degrees abaft her beam
ETJY	LEL is lower explosive limit
ETKK	Because if we don`t clean it will influence safety, economy, our own well-being and maintenance.
ETLE	Different products to be placed on separated and labelled shelves.
ETMC	Section 32
ETSY	nine digits, beginning by 3
ETTX	F1B
ETXE	5 V and 12 V
ETYX	Initially rise, then reset to the set value.
EUCH	On area A3 and A4 this function is based on the use of SARSAT COSPAS Epirb
EUDT	Initial and intermediate
EUDV	Once every month
EUTX	Raise the governor speed controller of the incoming alternator and reduce the governor speed controller of the alternator already on the switchboard
EUUN	0.7 bar?
EUUQ	Ohmmeter
EUWE	1
EUXV	He will find new brake bands in the engine store
EVNS	mV. 
EVNT	Reduce the sea echoes.
EVRY	As stated in the COW manual
EVVG	an efficient radar reflector
EWBA	The condition shall be noted and plans for further actions developed.
EWHS	When the tank has been satisfactory cleaned there shall be a 24 hour quarantine. Ventilation to be stopped and gas levels measured every second hour.
EWIQ	24h after their embarkation
EWKF	The process will oscillate and get out of control
EWMY	Shut off the starting air supply and open the indicator cocks
EWPK	Dry running of the pump, high temperature of the contents and various flowrate.
EWPL	70° C
EWRW	30 minutes
EWUJ	exclusively past to a ground-station between 70 degrees N and 70 degrees S
EWUL	lifebuoy with light
EWVA	He shall ensure obedience by the use of force if he finds it necessary, but not use harsher means than the circumstances make necessary.
EXCO	122700
EXDR	the time of transmission
EXEG	 Wheeled fire extinguisher
EXGV	A combination of ullage soundings and readings from the remote gauges
EXHS	Switch the UMS selector switch to manual mode and engage the "dead man alarm"
EXIL	The plan must show where to clean every day and where/when periodically cleaning should be done.
EYCQ	Close them to prevent the spread of fire, and allow the extinguishant to be released without time wasting.
EYFY	That correct temperature and washing products are chosen for the linen to be washed.
EYJD	To connect the ship fire main to the shore lines
EYJG	only with the master
EYKA	Solid combustibles
EYMK	In Part 16.
EYSQ	F1B
FATM	Not to damage the rotor blades
FAUG	Pushing, made fast in the vessel
FAVA	Use the opportunity to plot direction and rate of drift for later use
FBBB	Leave the engine room as quickly as possible, closing all doors behind you.
FBNL	Seven digits beginning with a one (1).
FBSH	Inspect/measure all areas surronding loaded tanks for leakage. Result to be recorded in the deck log book.
FBUX	lifebuoy with light and smoke
FBVA	Muster station 
FCFD	10 000 000 Ohms
FCGX	Bourdon Tube manometer
FCHS	Circuit breaker operating time
FCHU	70 % of MCR
FCIN	The IMO at London and the ITU at Geneva
FCJC	Because we need old ships in good condition to meet the world's demand for transportation.
FCNJ	Act according to instruction given in the fire plan. 
FCQY	TX: 2187.5 kHzRX: 2187.5 kHz
FCWR	The fire is extinguished by avoiding the contact between the fuel vapours and the oxygen
FDAX	 Heat detector
FDBR	200 gr
FDCL	Electric Contact manometer
FDCQ	 Foam release station
FDHM	to neutralize the sulfur and get a lubricating oil film between piston rings and liner
FDOF	nothing or a special characters will be printed
FDYB	Paint store 
FECM	6 knots for 24 hours
FEIA	A hearing shall be held before a committee on board.
FEPX	The ship's cow manual and ejector's performance curves.
FEUP	not less than 400 mm
FEWC	the amount of ionisation
FEWH	25 nautical miles off the coast
FEWL	Tarragon
FFBP	The should be blown completely dry by the use of air or nitrogen and then blanked.
FFFR	121,3 MHz  and/or  243,0 MHz 
FFMF	Interface towards center.
FFRC	Complete 15 compressions at the rate of 80 compressions per minute
FFSG	Keep the floors and decks free from fat and grease.
FFSU	Immediately notify the captain so he can notify the proper authorities, so the pollution can be dealt with by professionals
FFTA	Cross flooding arrangement
FFTU	An explosion-proof, self-contained, battery-fed lamp
FFYR	alerting
FFYS	the ship's radio log
FGBH	Rapid recovery shall be possible with the boat's full complement of persons and equipment.
FGCY	All these methods can be adopted
FGEQ	All the mentioned alternatives
FGKN	To prevent the water from freezing.
FGOP	Rest, Ice, Compression, Elevation.
FGPT	the date when the battery must be replaced
FGRB	PAN PAN (3x)
FGSD	a rustproof graduated drinking vessel
FGVB	Lye, metasilicate and soda ash.
FGVG	Inter-ship channel
FGWA	to both passengers and cargo ships? Yes.
FGXW	Near to the deck, crawl out keeping your face as near to the deck as possible
FHGM	The deck for the lifeboats.
FHIQ	Lights as per rules regulated by the shape and total length of the towing
FHJO	Increased turbocharger revolutions
FHKJ	Load line certificate
FHLB	There must be a complete interchangeability of hose couplings and nozzles
FHUH	Alkaline detergent (strong).
FHVL	Black
FIAI	Yes
FIBF	Ball bearings on the pump shaft, and wear rings on  pump housing or impeller.
FIEJ	Turbocharger
FIIP	List and trim correction tables.
FIJH	He has a special a special role as company agent
FIKI	In the Act relating to the enrolment of employees onboard ships.
FILE	All the items mentioned
FIPC	lifebuoy with light and smoke
FIRA	The engine shall be provided with an electric power starting system with rechargeable energy batteries
FISU	By immersing them in buckets with oil and water.
FIUL	All of the above
FJAH	15 PPM
FJGX	All alternatives
FJHV	The Act relating to holydays and Regulations relating to holydays for employees on ships.
FJPB	First aspect confirm death. Notify company, and make arrangements for notification of next-of-kin.  Arrange to have body moved to freezer area. Notify local agents and British Consul when abroad. Complete Births and Deaths section of Official Log book. Ma
FJPC	No - his certificate is not valid
FKAB	IMO
FKBR	Raise the water level a couple of inches above normal
FKCQ	Romeo, Alpha, Delta, India, Oscar
FKDL	Air leaks on suction side
FKPY	Intermittent signals by the ship's alarm bells.
FKQQ
The name of the person in charge of the transfer operation
FKRO	One bolt in every hole
FKRP	Henry
FKSJ	Prevent manual synchronising outside permitted limits
FKUA	4
FLBS	Poor cylinder condition - blow by -including leaking exhaust valves.
FLCN	Maximum is 30 litre pr nautical mile and total is 1/30000 part of full cargo on the ballast voyage.
FLDH	Yes, all crew must be able to communicate on the language spoken by the majority of the passengers, or demands set by the company.
FLMJ	The foam should be aimed at the bulkhead behind the fire and allowed to spread out slowly over the fire. 
FLPT	Within 24 hrs
FLPV	To avoid damage and miscolouring of different types of fabric when washing.
FMAT	Inhibitor name, concentration of inhibitor, duration of effectiveness of inhibitor, expected duration of sea voyage, temperature limitation qualifying the lifetime of the inhibitor and number of cargo tanks inhibited
FMKT	Dual purpose (jet/spray) type incorporating a shutoff
FMOV	The ITU List of Ship Stations
FNCM	Training in lifeboat handling.
FNEV	 Regulating freon liquid flow to the evaporator.
FNIF	9
FNIY	yes, with the MF/HF-radio telex
FNMI	By reports prepared by the master/employer.
FNPN	3731101234567#
FNYB	It is possible since the ballasted vessel stops faster than the loaded vessel
FOBJ	To avoid the compressor-oil to disappear from the crankcase during starting.
FOEV	May
FOGO	Proves the name of the owners of shares in the ship and nationality
FOJV	Ports in exposed position shall be closed and properly battened before the ship leaves the quay or berth.
FOJW	An unofficial translation of "Den norske skipskontrolls regeler" leaving out some provisions, such as speed limits, relating to local Norwegian waters. (The authorised Norwegian original applies in cases of discrepancies etc.);
FOPP	20 seconds or less
FOUN	Insuline.
FOVI	Lower the load
FOXW	Start engine
FOYQ	Approx. 18 Days
FPJV	Foam.
FPRB	You are running into danger
FPRD	Lack of oxygen?
FPSU	No - their role is purely investigatory to establish the facts -not to apportion blame
FPUN	to stop fuel oil from getting back from the HP fuelpipes between the pump strokes.
FPUO	with the exception of the areas A1 and A2 within the range of a geostationary satellite of Inmarsat in which an uninterupted alerting is possible
FPVH	Manual operated release system only
FPWB	Emergency fire pump?
FPYN	Radiotelephony - Frequency modulation
FQDR	Improve the scaling surface function, increase the service time of the exhaust valve in the engine.
FQEL	Broken water seal.
FQJO	Conductivity test.
FQLG	Figure 4 is correct.
FQMB	Making the crane jib move up and down.
FQQX	direct access to the navigating bridge
FQUL	lifeboat
FQVB	Wait until the coast-station calls again
FQVC	after ga+ the radio telex-command msg+?
FQWV	Radiotelephony - Single sideband suppressed carrier
FQYJ	at least 50 % of N (*)
FRFG	you must check the date that the battery must be replaced
FRGX	thermal protective aids for the number of persons the liferaft is permitted to accommodate
FRGY	Course, speed and risk of collision.
FRKD	Heavy seas from behind.
FRKL	A leak of exhaust gases from boiler or diesel engines.
FROO	14
FRQV	Best use of the survival craft facilities in order to survive.
FRTI	all of the above
FRYG	Take action to start the process to solve the situation, but do it diplomatically.
FSBA	Changing of filter element would not interrupt the engine operation.
FSFA	MAYDAY RELAY (3x)
FSGQ	MF
FSIL	All the mentioned alternatives?
FSPX	It is the seawater temperature and the purity of the vapour that gives the condensation pressure
FSYD	Prevent biological growth
FTAV	Crane No.1
FTAX	Protect the SCR against damage caused by high voltage spikes
FTEC	Emergency generator?
FTFD	always simplex
FTGS	Not less than half the total number of lifebuoys shall be provided with self-ignition lights.
FTLQ	automatically repeated after 3 and a half to 4 and a half minutes
FTYA	Every month
FUBR	RF-Gain
FUKP	Not less than 10000 kJ
FULL	By using a liquid receiver on the vapour line between the cargo tank and the compressor
FULO	The Health & Safety at Work Regulations (1997)
FUOG	Signals for vessels restricted in their ability to manoeuvre
FUPY	Cast off the rope.
FUSE	The team is applying water and the temperature is decreasing
FUVP	A search inside the crankcase for tools and rags.
FUWK	A pharmacy authorised to do so or if no such pharmacy is available, the master and an approved seamen's doctor
FVJY	Pump will overheat
FVOQ	a manual pump for effective bailing
FVYA	On a time sheet arranged by the Norwegian Maritime Directorate
FWEU	To relieve excessive high pressure in the cylinder to protect the engine from being damaged
FWFP	Water extinguisher.
FWHC	Incomer picks up as a generator
FWTR	The master checks all the relevant documentation is valid and in date. He completes the seaman's details in section ALC 1a, ALC 1b or ALC 1c as appropriate. The seaman signs in section a) of the signature of seaman section of the appropriate ALC form.
FWVK	One for each person on board who is not provided with an immersion suit
FWVL	Remove the toggle which will release the painter
FXAI	Ionization type
FXAK	30 minutes
FXCG	The visible smoke that is a result of combustion
FXDX	When you apply the rudder, she will continue to turn when the rudder is put amidship, and may even increase the rate of turn
FXGK	receipt of a distress alert
FXIA	0.2 Bar
FXIY	A SAR coordinating centre
FXTT	Every 12 months
FXYN	For cooling and to maintain correct viscosity on the fuel when injected
FXYP	A vessel, other than a rescue unit, designated to co-ordinate surface search and rescue operations within a specified area.
FYAL	Longer
FYCV	Climatic condition check list.
FYKG	Injection valve opening pressure is too low.
FYNQ	Ensuring that all persons avoid smoking in bed.
FYRU	The gas is harmful when the consentration is 5 parts per million or more. 
FYXS	14 hours a day
FYYN	The Norwegian Consular Court concerned.
GAAK	when technical problems are experienced with the Inmarsat-terminal
GAPO	It is important that the rotation direction is correct to avoid dry running.
GAPQ	Water
GAQH	Once a week.
GAQJ	Keep steady course.
GATR	Differentiating
GATX	a binnacle containing an efficient compass
GBCC	solid, liquids and gases
GBHB	muster station
GBHD	It is visible for a shorter time than a fuel oil spill
GBIW	Stop loading
GBNA	the use of SART transponders
GBOK	A, B, D
GBPL	The vessel's bow is pushed away from the nearest bank
GBQH	Not re-measured, but re-registered
GCCD	Before hot work or welding in tanks is started, a complete set of duly signed check lists and certificates shall be provided.
GCDS	Quantity of ballast discharged from segregated ballast tanks
GCDV	Figure 3.
GCEQ	Three years
GCFL	a MF radio telephony installation
GCGE	Toxic gases
GCLI	8 hours
GCOU	…..
GCRA	he SOLAS convention
GCSV	ESD is Emergency Shut Down and the release buttons are located different places onboard
GDCT	To all seafarers.
GDDY	Pressure diaphragm
GDFK	Turning the plunger piston  according to engine load.
GDHA	Full astern and drop the anchor
GDHX	Sent to RSS within 48 hours of closure
GDJK	Radiotelex and DSC - Frequency shift keying of carrier with error correction
GDNR	Measuring distance from cargo level to ullage point
GDQB	Sufficant, but minimum 3 complete sets.
GDRC	A water pad should be maintained during loading, transit and discharging. In addition a inert gas pad should be maintained during transit.
GDRY	The minimum temperature at which a combustible gives off vapours that may burn in contact with oxygen in air, and at which combustion persists once the source of ignition has been removed
GEDQ	Every three months. Details of test with signatures of Master and witness
GEFB	8 MHz band
GEGA	urgency
GELU	Propylene oxide may not be stowed in a tank adjacent to  butyric acid.
GEPB	1000 000 Hz
GERS	J3E
GESH	The master.
GEYG	Start slowly and closely monitor to ensure that discharging is actually taking place in order to avoid overflow.  When the level is below 98% the tank overfill alarm must be reset.
GFAW	Codes, MSC resolutions etc which are implemented in the regulations and which are expressly mentioned.
GFLQ	Made of material resistant to the different liquids to be stowed and also well ventilated?
GFLW	A relief valve.
GFPU	The wheels of hatchcover No. 7 came out off their tracks
GFPV	In two separate rooms outside the engine room space.
GFPW	16
GFQX	On all international voyages (except on short voyages) all lifejackets shall be fitted with a light and a smoke signal
GFRW	To receive information about ships in the vicinity.
GFSP	Prepare it immediately before serving.
GFUA	The current and wind are holding the vessel back.
GGUQ	semi-duplex
GHAV
Training in lifeboat handling.
GHAX	Sometimes it is necessary to facilitate overhauling.
GHFP	80 % of the Inert gas generator's capacity.
GHFX	Incondensible vapour in the cargo  and shortage  of refrigeration.
GHGM	during manoeuvre and manoeuvre speed condition (arrival and departure)
GHHH	In chapter IV
GHKS	Small.
GHLS	227530000
GHND	They automatically prevent any gap between the ship side and the lifeboat at the first stage of its launching
GHOT	the test function on the SART
GHQV	Qualified Individual
GHUM	Yes.
GHYD	Either of the Sen.Off.Deck if he feels the situation is heading out of control due to bad weather, bad manoeuvring, or for any other reason.
GHYX	Whenever the gangway is rigged.
GIDF	Physically smaller for the same capacity.
GIGG	The International Convention on Standards of Training, Certification and Watchkeeping of Seafarers
GIHI	Safetynet
GIRD	No fixed extinguishing systems are generally required for any other spaces protected according to this method
GITV	To ensure that the proper residuals of treatment chemicals, as specified, are maintained at all times
GJCX	518kHz
GJHG	15 ppm
GJKN	Cooling, smothering and dispersion
GJSR	He is supposed to paint the evaporator and use a brush to apply the paint
GJVG	Carbon monoxide, nitrogen dioxide, nitric oxide, sulfur  dioxide?
GKDT	Piston
GKHF	It is the Certificate of Fitness that is issued in accordance with the IGC code
GKLC	The place of welding-work to be cleaned and all unnecessary objects to be removed.
GKOR	Important due to different material and working conditions
GKPK	As soon as possible determine how the ship is drifting to establish if there is any danger
GKPM	Activate the nearest fire alarm button and advise bridge of the location of the fire.
GKQH	Set the engine to dead slow ahead, and change the course 10 degrees to port
GKRE	Navigational warning.
GKVI	the use of MF and/or VHF R/T
GKXR	a tiller permanently linked to the rudder or removable if the lifeboat has a remote steering mechanism
GKYL	Take a visual search of the sea around the ship
GLIP	A keeps out of the way of B
GLJK	Threshold Limit Value.
GLJL	The pressure drop across the filter.
GLKF	Strain gauge
GLKG	Two sets or more depending on the type and the size of the vessel
GLKH	4
GLLG	5
GLRY	PAN PAN
GLWT	Same number as beds in the cabin
GLYL	Crosshead
GMHS	Get out of the engine room as soon as possible. 
GMIR	All the mentioned alternatives.
GMJM	Correct water level is obtained by refilling the cooling system, and the entire system is checked for leakages
GMLA	AND
GMOE	They reduce the surface tension of water
GMOK	Collect rain water
GMQY	lifebuoy with line
GMUY	Yes
GMVY	1.5 times designed working pressure, but not more than two-fifts of it`s bursting pressure.
GNDL	All the mentioned alternatives.
GNEL	the use of VHF DSC
GNGS	As per Builders' specification?
GNHN	12th day, 1310 hours UTC
GNXL	No, as only the output from the barrier is intrinsically safe this is not allowed.
GOCO	Notify as soon as you have knowledge of any spill, or  threat of a spill
GOYB	Make sure your vessel + crew are safe and then offer your assistance to the other vessel
GPAT	It is centrifugal pumps that is normally used on gas carriers
GPGQ	Crew accommodation and provisions and water must be inspected on a weekly basis
GPLP	Gas levels measured in tanks where work is to be carried out.
GPMK	Lubricating oil pressure is too low.
GPPA	10000 ppm.
GPPO	By double blank flanges with a drain between them?
GPPW	Any of the alternatives.
GPQR	Connect the firelines ship/shore
GPRM	8 MHz
GQAU	That all the valves on the delivery side are open before starting.
GQJB	A vessel of more than 50m in length engaged in pushing a barge/barges ahead
GQPU	Venting of the tank must be carried out after cargo discharge to ensure removal of any cargo  which may have been absorbed into the coating system.
GQQR	Find out from officers and crew who have been in connection with the collision, what they have seen, so that detailed and complete description of the sequence of events can be entered in the log-book.
GQSB	16
GQTU	We are allowed to gas up LPG on inert gas if the charterer do not instruct the vessel to use nitrogen
GRDU	Correct donning of life-jackets.
GRHB	the closed-type feed-water system
GRLM	Personnel working in regulated areas must use respirators
GRPI	Can identify small targets
GRPO	telephone signals in the same frequency band are generally weaker than DSC signals
GRTS	Bowl opens unintentionally during operation.
GRWD	Not necessary, he shall use all available resources. He should resist the temtation to step in and do it all by himself
GSCW	38205
GSCY	I am in distress and require assistance
GSDT	The master.
GSES	30 m
GSFP	maximum permitted height of stowage above waterline
GSQL	completely watertight
GSWB	position of the aerial
GSWF	Oil Transfer Procedure  manual
GSXA	Separation of water and oil.
GTDU	Norwegian law unless otherwise provided in or pursuant to a statue?
GTGB	30 minutes
GTJJ	Yes, you must attend to a course held by certified personnel, and then be certified by national authorities (NMD, USCG, etc)
GTJL	The company has to ensure that an agreement is always confirmed  in writing
GTQE	4 times the outer diameter of the lifebuoy
GTRA	Intrinsically safe.
GTSU	No, glass bottles can not be dumped overboard
GTTS	Contain any oil-spill onboard the ship
GTVX	Blow  the boiler and renew water until the PH-value is normal again.
GTWA	0,2 Bar
GTWW	Overhaul the compressor unit.
GUGU	We are allowed to gas up LPG on inert gas if the charterer do not instruct the vessel to use nitrogen
GUNK	90 air-changes.
GUNQ	The gudgeon pin, big end-, or main bearing clearances is too large.
GUNS	Air, Breathing, Circulation.
GUON	Portable bridge between ship and shore.
GUPA	As specified in the vessel' s Planned Maintenance System,       (Ref. Makers Instruction).
GVGW	Dry ice
GVIO	Push the hook through the skin until the barb protrudes, then cut the hook between the barb and the skin and gently  withdraw the hook.
GVIP	Charterers requirement in this example.
GVKX	30 minutes
GVRS	shut off the oil flow if the flames goes out
GVVC	is fixed by manufacturer
GVWW	give relevant instructions and warnings
GVYK	BLEVE
GWDJ	By control of liquid flow
GWGP	In a secure and sheltered position and protected from damage by fire or explosion
GWID	EPIRB
GWKU	Remove the toggle which will release the painter
GWMN	Sierra, Charlie, Hotel, India, Papa
GWNI	A glogged bilge strainer
GXAX	Yes it is.
GXFW	one daylight signalling mirror
GXLQ	The inlet- and exhaust valve tappet clearance is off adjustment.
GXNG	Information about the ships fire preparedness do we find in the alarm instruction
GXRD	Approximately 5 metres
GXXF	7
GXYD	The fishing vessel keeps out of the way of the power driven vessel restricted in her ability to manoeuvre
GYAW	We can trim the ship by stern as much as possible. This will most likely change the direction and rate of drift
GYBP	Throttling the delivery valve, adjust the RPM, by-pass.
GYLM	Monkey wrench
GYMI	They have responsibility for setting, monitoring and enforcing standards of safety and pollution prevention on vessels flying the countries flag
GYQI	300 PPM.
GYVK	Gas may enter, but even if an explosion takes place the fittings  is so strong that the explosion will be contained within it and will not be blow out?
GYVO	Loss of alkalinity, corrosion of boiler metal surfaces, and loss of phosphate reserve in the boiler.
GYVQ	One prolonged, one short, one prolonged and one short blast
GYVS	Camshaft
HACL	Equipment for detecting flammable vapours.
HADH	To minimise oil losses and prevent the sludge getting too hard
HAEF	Seawater
HAFF	Check in appendix 2 of MGN 1
HAJA	That a secondary auxiliary set is switched to automatic standby mode
HANH	On the motherboard
HANI	Stop the engine immediately and keep the luboil pump  running for at least 20 minutes before opening the crankcase?
HAPC	It shall be cleaned daily and oiled and inspected regularly.
HAQP	By pumping test of each bilge before loading?
HARO	22 A                                                                                  
HARQ	Radiotelephony - Single sideband full carrier
HAUF	This is firezones which can be divided from eachother with firedoors. If a fire start in one zone, all firedoors in front and aft of the fire will be closed from the bridge to stop the smoke and fire from spreading.
HAWM	Once every month
HAYE	Alkaline cleaner.
HAYG	on board communications (intra-ship traffic)
HBGO	Passenger ships carrying more than 36 passengers
HBJX	Alarm the rescue centre and commence searching for any survivors
HBOC	Figure 1
HBQV
Yes, if the seafrers demands it 
HCAT	A sticking start air valve.
HCBI	A fixed sprinkler system at the cargo manifold
HCBO	All of the mentioned
HCCJ	12MHz
HCMG	Part ALC 1d of the crew agreement, giving details of specific terms and conditions for seafarers
HCQM	The emergency generators
HDAT	Increased.
HDBM	Wash thoroughly and hang up for drying.
HDCJ	 one whistle or equivalent
HDFT	Section 3.
HDJV	It could be any of the alternatives listed.
HDKP	Not less than 10000 kJ
HDOT	38
HDPT	Every three months
HDQQ	Rescue boat
HDSW	1st February 1999
HDTU	Smoke and increased pressure in the crankcase of the engine.
HDVM	Type of oil or gas chemicals having been carried in the actual tank and the adjacent tanks.
HDXC	Leave a "cushion"of water in the sloptank, to minimize the risk of polluting the sea
HDXU	So that no part of any corridor is more than 20m away from any manually operated call point
HDYY	It will always be a deviation between the set-point and the process value
HEBH	all alternatives
HEOT	Applying 12 - 15% nitric acid on tank surfaces, either with a brush or spray; then washing off after 10 - 20 minutes using copious amounts of fresh water?
HEVD	Figure 2 is correct.
HEWF	Removing trash, dusting and light cleaning in cabins, messrooms and WC.
HFLB	On the fire control plans
HFLG	Full power on the forward tug, reduce on the aft tug while checking the gyro
HFMT	the painter
HFNQ	The master.
HFPI	At least one 
HFQD	the use of HF DSC and SARSAT COSPAS Epirbs
HFQI	Secure hatches
HFRA	Fasten seat belts
HFSQ	It keeps the boat alongside the embarkation deck so that the tricing pennants can be released
HFXU	Hydrochloric acid and citric acid.
HFXV	This is not correct, inter-ship has to be intra-ship
HFYQ	assembling passengers at muster station
HGCY	Serious emergency - all vessels to stop or divert according to instructions
HGDT	Inerted to less than 8% oxygen(IMO).
HGEO	Not at temperatures used for pre-heating
HGGE	Stop bunkering, and establish facts, before bunkering is resumed
HGGY	Open the tank, provide adequate ventilation/lighting, test oxygen content, have someone standing by with rescue equipment, complete a tank entry permit then commence work.
HGHB	Cooling water spaces insufficiently vented.
HGHY	The change needed in the input signal to produce a change in the output signal.
HGKK	At least one hose for each 30 meter length of ship plus one spare
HGLB	Leather safety boots and gloves
HGNW	Marine Officers of the MCA
HGOM	The ITU List of Ship Stations
HHBW	The pump is not primed.
HHCO	Yes, the ship usually steers better if trimmed by the stern
HHDN	Pork
HHFA	2
HHIJ	Centre line is given by A on the figure
HHLE	That the wires are just above the water line at all times
HHNL	the time in minutes, or parts of it, when the landline was used
HHNN	The master, and any person who does not form part of the crew e.g. riding squad
HHUD	Maintain the specified boiling temperature
HHWS	3 sets
HHYM	Ch.70
HIBY	 1. Switch off the transmitter - 2. Switch equipment on - 3. Make broadcast on channel 16 "Mayday all stations…" and cancel the false distress alert.
HIFC	3   -   30 MHz
HIHW	Yes, by "distress priority" one always is assigned a channel
HINF	The fixed fire fighting medium in engine room, pump room etc. is Carbon Dioxide CO2, Halon or foam
HIWP	It is an automatic system for plotting vessels for rescue purposes
HIXI	Just in forepart of the rudder square (figure 3)
HIXJ	in presence of atmospheric or interfering signals automatically adjust itself
HJCN	Ships fitted with free-fall life-boats may carry thermal protective aids instead of immersion suits
HJLS	Re-pack the stuffing box loosely with the correct size packing at the earliest opportunity.
HJMN	 reduce the "noise" in the background
HJMQ	Safetynet
HJNL	Pressure relief valve.
HJPY	98 Centigrades
HJSI	To prevent contamination of the cargo.
HJVM	RSS, HM Coastguard, Marine Officers, Enforcement Unit, Channel Surveillance Unit, MPCU
HKDC	4  Rocket parachute flares / 6 hand flares / 2 buoyant smoke signals
HKLJ	+ 85 ° C
HKMF	be as small and of as little mass as possible
HKNF	Check linearity
HKSD	6
HKTA	Special section for Births and Deaths and also to be included in narrative section
HKUV	lifebuoy with light
HKXE	Yes
	
HKYX	The seafarers shall have available for their use the Seamen's and NIS-acts with regulations, together with all relevant CWA`s/CBA`s.
HLFN	Inverting amplifier                                                           
HLIX	In stairways, corridors and escape routes
HLJS	Higher measuring accuracy.
HLNC	All the mentioned alternatives 
HLOW	search and rescue at sea
HLQN	instruction in the use of radio life-saving appliances
HLRC	a person who holds a "certificate of proficiency in survival craft"
HLVJ	Flat file
HLWF	Space thoroughly ventilated, Oxygen and gas readings taken, communication set up, permit to work completed, Crewmember standing by, with rescue gear.
HLXE	He wants the heating coils inspected
HMBI	Exhaust leakage
HMEV	Assorted canapes.
HMGD	On area A3 this function is based on the use of INMARSAT A, B or C
HMGN	a ship idendity number
HMLF	All preventive methods to avoid spreading of bacteria and fungus.
HMPK	To protect both owners and charterers
HMSW	Safety purpose?
HMTS	When the container also contains water
HMYN	All the actions listed in the other alternatives
HNAL	30 minutes
HNCT	Depth is given by B on the figure
HNCU	Fully slacken and remove top ones first, then middle, then bottom.
HNLE	Opening water function missing.
HNVG	Scavenge box fire
HNVI	Channels 6, 13 & 16
HNWY	It should be about 20%
HOCT	COTP-zones may have additional rules and regulations
HOLA	A throughput of at least 400 litters a minute and  a "throw" of 15 metres?
HOLX	Water extinguisher.
HOQE	4.5 bar
HORY	- 43° C
HOTH	Adiabatic.
HOUE	Yes, you must attend to a course held by certified personnel, and then be certified by national authorities (NMD, USCG, etc)
HOWT	Water-tube boilers are more efficient and contains less water. They suffer from major damages when run dry during operation.
HOYJ	All launching appliances shall be capable of recovering survival crafts and rescue boats with their crew
HPDQ	4.25% of the volume of the room
HPDU	Aft breast line is defined as B on the figure
HPGW	Plate
HPHR	Zener diode                                                                      
HPHU	5 seconds
HPLE	When you need to protect your eyes.
HPMA	40 ohm
HPMR	10 %
HPPB	The smallest diameter piston is the stage two piston.
HPPC	Deballasting and loading simultaneously.
HPTH	To maintain a record of all British ships and British certificates
HPVB	Regularly check your pressure gauge and note how much air you used to reach your work area. Start to return when you have this amount left plus a reasonable reserve
HPVX	Immersion suit
HQAX	1 m depth per minute
HQEF	Figure 1                                                                       
HQGU	continuously after having been immersed for a period of 10 seconds under 100mm of water
HQHT	Shut off the starting air supply and open the indicator cocks
HQIS	Not more than 13,5 litres and not less than 9 litres
HQJG	Avoid spilling water and fat on the floors.
HQLU	Forward spring is given by D on the figure
HQQS	To do a full calibration.
HQQW	the degree of priority
HQQY	8 MHz band
HQXO	Bow/stem is given by B on the figure
HQXQ	Outside the coloured zone.
HRCT	Equal power on both tugs while checking the gyro
HREE	No. 1 diesel and No. 2 diesel
HREY	He is to check the heater for the hydraulic oil
HRJV	Radiotelephony - Single sideband full carrier
HSTT	11 %
HSUT	 Use the "cleaning in place" arrangement or open the heat exchanger for visual inspection and manual cleaning.
HSXB	Cargo ships of less than 500 tons gross
HSYU	You cannot survive in H.E. foam as the oxygen content is reduced.
HTAQ	3 cm radar
HTAU	4  Rocket parachute flares / 6 hand flares / 2 buoyant smoke signals
HTPS	Raise the load
HTPX	Loose tight clothing, ask all unnecessary bystanders to leave and carefully place something soft under the head. If casualty is unconscious, place the person in Recovery position.             
HTQN	Air in the cooling water system.
HTVI	In tanks not adjacent to the ship's shell plating having heating coils?
HTYW	Forward spring is given by D on the figure
HUHC	Expands
HUIB	They shall be carried in cargo tanks independent of the ships hull structure?
HUPO	Singapore
HUSV	Foam.
HUTX	Duration of public correspondence communications
HVER	Each lifeboat shall be launched with its assigned crew, and manoeuvred in the water at least once every three months during an abandon ship drill
HVGC
Williamson Turn
HVGD	Answering Pendant
HVGH	He is asking about the position of the chain
HVJO	Chemical powder is the main medium for tank deck fire fighting on gas and chemical carriers
HVKH	Yes, neutral atmosphere in hold space on all gas carriers exempt from those who have independent type C tanks
HVQG	One month
HWBC	Too low suction pressure.
HWCB	2 lines of position.
HWDR	2
HWHD	To cool, remove sulphur dioxide and particulate soot from the flue gas? 
HWKI	substitutes for key persons who may become disabled
HWQG	Stand on dry insulating material and pull the person away with isulating material.
HXBC	Lower lifeboat to water
HXCQ	an area within the radiotelephone coverage of at least one VHF coast station in which continuous DSC alerting is available
HXGD	VHF-equipment
HXGI	rescue boat
HXHS	For at least three years
HXIM	When temporary bulkheads (bins) are used on deck, openings shall be arranged as to prevent water accumulating.
HXKF	A thorough ventilation of the combustion chamber before the ignition takes place
HXMV	The temperature must at all times be 10 degrees Centigrade above the oil's pour point temperature.
HXNP	have at least two entrances
HXUC	Figure 1
HXVA	That the watch keeping personnel shall be ready for starting or manoeuvring the main engine.
HXWA	Not less than 10000 kJ
HYDL	4,50 m
HYEK	too much combustion air
HYRP	Close the valves on both the Acetylene and the Oxygen bottles.
HYSN	West cardinal buoy
HYTJ	Both STCW and Class rules
HYVW	NAND
IAFK	muster station
IAKJ	Check if fuel injection is too early or fuel pump lead too large
IAKL	150 tons
IAQA	one first-aid outfit in a waterproof case
IATQ	A wire for pulling burning ships off the pier
IAUG	safety call
IBFF	25 % more than the wire's
IBHY	a given number of buoyant oars provided with thole pins or crutches attached by lanyards
IBOK	64
IBOM	It is incumbent on the shipowners and the master to ensure that the requirements are complied with and documented.
IBPY	Evacuation slide
ICAA	The hydraulic pump is usually used for tightening the G-nuts
ICHS	Shut off the oil flow if the flames goes out
ICHU	Radiotelephony - Single sideband suppressed carrier
ICIK	The use of engines and accessories
ICWU	 Remote controlled fire pumps
ICYJ	Windlass is given by B on the figure
IDCO	The fuel oil filters or pipes are clogged.
IDDM	Amount of superheat in the vapor leaving the coil
IDEA	of being deployed by one person
IDIL	Bollard is given by D on the figure
IDIN	Warm clothes, blankets and lifevests.
IDQV	The method of donning life-jackets.
IDRK	Stuck grease was blocking the grease pipe
IDUT	Starboard quarter is given by C on the figure
IDVS	At least two
IDYB	Amplitude of output signal divided by amplitude of input signal
IEOE	Class B fire
IEOX	J2B/F1B
IERT	Reduce to slow or less in due time before entering
IEXH	 424432010 or 424432020
IFAS	Airway  Breathing Circulation 
IFFT	G3E
IFJV	2 separate compartments
IFJW	The uppermost deck to which transverse bulkheads are carried
IFLU	Two tongue-type/hinged bowstoppers with separate closed fairleads - Capacity 200 tons
IFMN	A compilation of Norwegian laws and regulations concerning the safety of ships and crew.
IFMO	MARPOL 73/78.
IFRI	out of order
IGCA	To prevent electrostatic generation
IGDX	You should have reduced your speed to the minimum on which the vessel can be kept on course
IGES	Nervous tension,allergy, or none obvious cause.
IGFO	Rotary positive displacement (mono type).
IGGI	Overboard discharge is stopped.
IGRD	IMO divides cargo tanks on gas carriers into 4 groups: Integral tanks, Membrane tanks, Semi-membrane tanks and independent tanks
IGWC	No spark or flame is required to ignite gas or vapor
IHAH	activate the fire alarm
IHAO	Two
IHBJ	Notify Master, Deck officer and Engineer in charge.The loop for this special sensor to be switched off and take normal precautions for hot work.
IHCB	Start air supply
IHCD	Powder
IHCU	To secure/lash containers?
IHCX	This call was sent by a coast station
IHHG	5 sets of Firemen's outfits
IHSR	Fully charged bottles with a total free air capacity of at least 6000 liters for each breathing apparatus.
IHTT	Closed loop feed back system
IHUR	Pressure indicator, installed on panel/console                 
IHXA	Ahead is given by A on the figure
IHXT	Ensure a flow of steam through the superheater when raising steam pressure after shut down
IIBD	A person may serve on board as from the 17th. calendar year
IIES	Don't let the ship turn to port
IIGG	If the back pressure when discharging is so high that one pump is not able to deliver any cargo.
IIHB	It is the SOLAS conventions that take care of the human safety at sea
IIHE	Presentation flange.
IIOS	Both STCW and Class rules
IIPJ	Monthly 
IIQH	Regularly check your pressure gauge and note how much air you used to reach your work area.  Start to return when you have this amount left plus a reasonable reserve.
IITK	Stern line is given by A on the figure
IIYU	 1. Switch off the transmitter - 2. Switch equipment on - 3. Make broadcast on 2182 kHz "Mayday all stations…" and cancel the false distress alert.
IJEM	Reduced.
IJEO	Start with intermittent firing, using small firing periods and long intervals gradually building up to longer firing periods and shorter intervals.
IJIP	Chemical powder is the main medium for tank deck fire fighting on gas and chemical carriers
IJNO	J3E
IJOI	In permanently exhibited fire control plans
IJRT	anti-seasickness medicine and one seasickness bag for each person
IJRV	Height is given by D on the figure
IJST	one knife of the non-folding type having a buoyant handle and a lanyard
IJVB	the curvature of the surface of the earth
IJWV	Reduce speed and, if possible, keep the fire zone to the leeward of the ship
IKAB	All the mentioned alternatives
IKCT	0,56 m3/kg
IKIN	Tanks adjacent to the tank where work is to be carried out shall be cleaned and free of gas.
IKKD	To avoid build-up of static electricity, which may cause explosion
IKLV	Full power on the aft tug, reduce on the forward while checking the gyro
IKLX	Clogged air inlet filter.
IKNO	to wear a lifejacket inside
IKSJ	Hatch openings in weather deck to be closed and battened down before loading of deck cargo.
IKTI	Yes 
ILDJ	Prior to every plant start-up, following an 8 hour stop
ILED	1530 C
ILEH	Every second hour.
ILFC	It will destroy the properties of the lube oil and lead to serious damage in our engine.
ILMM	the "Abandon ship" signal is not specified, only the general emergency alarm signal is stated
ILOD	The light from lanterns and signals must not be obstructed.
ILOI	trying to ignite burner from hot brickwork
ILRP	The Norwegian Consular Court at the nearest competent Norwegian Foreign Service Station.
ILTE	In SOLAS chapter II-2, rule 17 and in the IGC code
ILTH	5 times the maximum pressure the hose will be subjected during cargo transfer.
IMBR	A Norwegian Maritime Investigator
IMGM	1 VHF RT + DSC+ DSC watch receiver - 1 or 2 SART - 1 NAVTEX and/or 1 EGC receiver and/or 1 HF NBDP watch receiver - 2 or 3 VHF portable - 1 EPIRB - 1 MF RT + DSC+ DSC watch receiver - 1 HF RT + DSC+ DSC watch receiver
IMJB	A suitable composition of water and detergent.
IMJD	15 and 17
IMNG	Stripping pump.
INEX	lifebuoy with line
INKV	CES two digits code    #    00    Country code    Area code    Subscriber code    #
INRG	No ventilation should be done?
INSB	Able to effect a complete change of air of the space being ventilated 16 times an hour?   
INUQ	Centrifugal pump
IOAU	Acts.
IOBI	request for a collect call
IOQF	No
IOQH	Yes.
IPEP	Proximity switch
IPFK	Maximum allowable working pressure
IPGK	Class A
IPJW	All the listed alternatives
IPLJ	Opened after rough weather or before loading/discharging or transferring cargo to check for liquid accumulation and contents drained into a drip pan.
IPPP	watertight receptacles containing 1.5l of fresh water for each person (may be partially replaced by a desalting apparatus)
IQBD	Figure 3.
IQEQ	Discharge the slop tank completely and refill it from another tank from which the bottom 1m ullage has already been discharged
IQGE	Ventilate the holds as well as possible
IQGK	The user should be warned that the product contains fluids that may irritate and itch skin.
IQHC	Washing and polishing floors, chemical cleaning of furniture and carpets in cabin and other common rooms.
IQHE	Need more space than normal
IQLG	recommended at the beginning and at the end of the message-transport to exchanges 'answer back' s'
IQMB	 Released blocking function in remote starting system.
IQOS	to have a telephone conversation with a person whose name is known
IQPN
Any of the listed alternatives.
IQTT	The human body absorb toxicants through respiration, skin and the aliment channel
IQXU	Monthly
IRAJ	4 mA.
IRHV	there is never a direct connection with the shore-subscriber
IRIT	1300210
IRVA	not more than 800 mm
IRWV	The extinguishing agent
ISIJ	1.495 kg/l
ISPY	Measurement of differential pressure
ISRV	Figure 2.
ISSQ	High block coefficient vessel
ISUD	12 mm,  16 mm and 19 mm
ISVS	Special area is certain areas like Red Sea,  Black Sea, Baltic Sea, Mediterranean, Gulf area, Antartic area.
ISVY	68 - 79°C
ISXN	A1
ITAY	Safety Radio
ITCP	To purge a tank means that we change atmosphere in the tank e.g. change cargo vapour with inert gas.
ITEE	In suitable lockers easily accessible, yet segregated  from the living spaces themselves?
ITKE	evacuation slide
ITNO	IMDG - CODE
ITOJ	The 0-voltage must always be grounded.
ITOL	Small changes in temperature can cause large movement of the interface
ITPC	A visual and audible alarm signal at the control panel
ITRO	Start water-spray
ITRV	All of the listed alternatives.
ITWS	liferaft
IUBR	No. More readings should be taken and sediments, sludge and residue should be removed at least 10 m from working site.                                                            
IUBW	Glycerine is compatible with both of the other cargoes.
IUED	In any port in a country which is a member of one of the port state control regimes currently in operation, other than the UK
IUHP	I require assistance
IUIH	Cargo ships of less than 500 tons gross shall have the batteries located in the upper part of the ship
IUJJ	121.5/406MHz
IURP	Operate valves gradually
IUTX	Call the nearest coast station and inform it that a false distress alert has been transmited
IUWK	32
IVAV	Minimize corrosion, prevent deposits and scaling, and control of biological growths.
IVDF	60 %
IVGQ	Head line is given by B on the figure
IVHF	To ensure that we do not have any water assembly in the cylinders when the compressor start.
IVHI	handrails for persons moving about the exterior of the lifeboat
IVIF	NO. 1,2,3 and 4
IVKX	On the bridge
IVMO	always with the coast-station
IVNJ	a personal call
IVPP	To prove that oil has been pumped overboard according to regulations
IVRK	a mock search and rescue of passengers trapped in their staterooms
IVSE	How to don lifejackets, immersion suits and anti-exposure suits, as appropriate
IVWK	60 bar
IVXI	Directional control valve.
IWDX	Every motorized survival craft shall have a certificated engineer assigned
IWES	The tug's bow against my stern, made fast with lines. By moving the tug to either side of my stern, this will help to steer the ship (figure 4).
IWGN	Safety equipment to be made good in a given time period; Safety equipment to be made good at next port; Safety equipment to be made good before sailing; Vessel to be detained  until all safety gear brought up to a minimum standard
IWHE	The route to musterstation, how to put on lifejacket and different emergency signals used onboard the ship.
IWIF	3 litre
IWNB	To prevent the steam and water in the boiler from discharging out by the feed line, if a feed line fracture or a joint in the line blows.
IWOD	Broken water seal.
IWQN	Separation of two insoluble liquids with different densities, and at the same time removing of solids.
IWUO	Correct flow, pressure and temperature. ( Viscosity)
IWVQ	Chemically dose and fill up.
IWWK	To prevent the suction line from draining and keeping the pump primed.
IXBH	rescue boat
IXHF	States of matter means that a substance can exist either as solid, liquid or vapour state
IXIY	30 minutes
IXTV	First Zero adjustment and the Span adjustment. Then Zero  should be rechecked. 
IXUQ	Water extinguisher
IYBF	The meaning of MARVS is Maximum Allowable Relief Valve Setting
IYEL	3 cm
IYES	The latest IMO gas code is IGC code International Code for the Construction and Equipment of ships carrying liquefied gases in bulk
IYJN	Contact the issuing authority via the company office
IYLF	The alternators output itself via the automatic voltage regulator
IYNT	2 sec
IYPK	Non-inverting amplifier                                                   
IYQF	1000 A
IYRC	Will relay a message concerning an important navigation -or meteorological warning
IYRE	All of the mentioned reasons.
IYTO	100% of the ships complement on each side
IYUJ	the use of SART transponders
IYVI	Reduce speed and use soot blowers if some are fitted
IYYL	A unit which automatically releases the liferaft/lifeboat at a depth of approx 4 metres.
JAFM	Where the mooring lines lead.
JAHH	Warm nutritious drinks.
JAID	Boarding, launching and clearing of survival crafts (lifeboat/liferafts) and rescue crafts (MOB-boats).
JAJB	A resistance guide stating which chemicals are compatible with the coating.
JAKR	Salt
JAKS	Zero
JALM	Capable  of immediate operation at all times
JALP	40 - 60 %.
JAQO	the sea area of the vessel
JAXC	STCW means Seafarers' Training, Certification and Watch keeping
JAXE	Carbon atom has 6 protons and electrons
JBCE	To avoid liquid coming back to the compressor during start  up.
JBEN	The condition shall be noted and plans for further actions developed.
JBEU	The container, the extinguishing agent, the impulsion system
JBGH	That the main propulsion unit controls are attended under standby condition.
JBKS	By help of the Headword Register, the Chronological Register, the table of contents, the tables of contents in the respective provisions, the Preface, etc.
JBLI	channel 06
JBMD	Through stapled-in supplements in the quarterly NMD magazine "Navigare" and Ships Documents.
JCAG	Annually.
JCAI	The turbine rotor is not balanced.
JCFG	Remove the load from the alternator to be stopped
JCFL	Regulations concerning the registration of hours worked and the format and keeping of time sheets.
JCNS	Aft is defined as A on the figure
JCQI	Rectification would be required before sailing
JCVE	Inspectors from the International Maritime Organization (IMO)
JCXX	518kHz
JCYL	Normally use it, as free or dissolved chlorine is not aggressive towards stainless steel?
JDDS	Connecting rod
JDOT	A code issued by IMO for use onboard vessels carrying packaged dangerous goods?
JDPL	2500  mm wg?
JDQF	A period not exceeding 12 months
JDRW	It shall be cleaned daily and oiled and inspected regularly.
JDRX	The master.
JDTO	S band radar
JDUG	About 20 %
JEWX	Water in a cylinder.
JFDH	Until all crew members and passengers have reported to their respective muster stations.
JFFD	The side from the wind.
JFFG	25 miles
JFJN	The main supply valves in the deck storage are closed prior to switching to UMS-mode
JFPI	To complete a voyage (max 5 months) or at a surveyor's discretion (max 1 month)
JFRS	there is never on-line connection with the shore-subscriber
JFSQ	36715
JFVX	An injury, other than a major injury, when the injured person is incapacitated for more than 3 consecutive days
JGAE	The aircraft is directing a vessel towards an aircraft or vessel in distress
JGBT	Radar transponder
JGGR	Permission must be obtained from Chief Officer?
JGMM	We can, reduce discharge rate, pump hot vapour into the cargo tank or pump some liquid back to the cargo tank
JGNK	DSC-symbol is sent twice and checked extra by Error Check Character
JGRM	STCW 95
JGSJ	A, B, C, D
JGYG	sunspots
JHBM	on the number of kilobits of information transmitted per block of 256 bits
JHBO	Dual purpose (jet/spray) type incorporating shutoff
JHHH	LUT before the satellite is actually seen by this ground station
JHKS	Line-throwing appliance
JHND	Complete 15 compressions at the rate of 80 compressions per minute
JHQR	Water in one or more cylinders.
JHRM	The quality of the Crude Oil Washing performed during the last discharging
JHUY	Any one involved in the operation
JHVV	Survival craft distress pyrotechnic signals
JHYC	Follow your track and reduce the speed to keep your vessel in line. Overtake the other vessels after the strait is passed.
JHYU	an atomization of the fuel injected into the combustion chamber.
JICN	Safety of ship and crew
JICP	It is higher pressure on one side of the seat than on the other side, and it is shut manually or by change of pressure on the seat
JIEU	FEC
JIKQ	Fluids (liquids).
JIQO	Freeboard is given by B on the figure
JIRL	the amplitude of the carrier-wave changes
JIUS	Marine Officers of the MCA
JIXC	Increase scavenging air temperature to above dew point
JIXI	vessel
JJEP	Dynamic pressure pump (or roto-dynamic pump).
JJGL	it's canopy has viewing ports in all directions
JJLF	1 VHF RT + DSC+ DSC watch receiver - 1 or 2 SART - 1 NAVTEX or 1 EGC receiver - 2 or 3 VHF portable - 1 EPIRB - 1 MF RT + DSC+ DSC watch receiver
JKAN	 Gas detector
JKDV
Steam at high velocities may generate static electricity  which might cause incentive sparks?
JKEW	Twistlocks and rods with turnbuckles?
JKGC	master
JKGH	Oil pressure is greater than the water pressure.
JKHA	Vitamin A
JKHB	For all vessels.
JKRE	By repeating the order
JLBA	High density, sub - micron particles.
JLBI	portable fire-extinguishing equipment suitable for oil fires
JLCB	Ensure the valves are of the correct discharge capacity for the boiler.
JLCY	urgency signal
JLES	Figure 3.
JLQD	The use of the ship's line throwing apparatus
JLRA	The floor of the raft has a second layer which can be inflated to help insulation, in addition to the thermal protective aids (10% of complement, minimum 2)
JLSV	reporting to stations and preparing for the duties described in the muster list
JMHV	5 years
JMLY	1 Smoking in bed. 2 Covering of electric fires with blankets.  3 Overloading electric plugs.
JMMT	Raise the fire alarm.
JMUH	Check fuel injector valve, fuel injection timing, fuel pump suction valve and fuel pump lead
JMUI	Quadrupled
JMVB	The Norwegian Maritime Directorate
JMYM	Double check valve.
JNDM	capable to determine the position of the EPIRB
JNIS	CES two digits code    #    00    873    SES INMARSAT code    #
JNOB	10 k ohm
JNPC	ICE-method.
JNTH	Alarm instruction.
JNTN	1 VHF RT + DSC+ DSC watch receiver - 1 or 2 SART - 1 NAVTEX or 1 EGC receiver- 2 or 3 VHF portable - 1 EPIRB
JNUC	It should be protected by a fixed fire fighting system i.e. sprinkler system.
JNUH	a food ration for each person
JNXO	one copy of the prescribed life-saving signals
JOCU	1% to 10%
JOKT	Clean the heat transfer surface
JOPB	Either Ore or Oil.
JORR	go to simplex telephony
JOSN	Sea Area A4.
JPGR	So that neither the rescue boat nor its launching arrangements will interfere with any survival craft at any other launching station
JPJV	Several control-valves are connected to the same controller
JPKQ	Reduced.
JPOX	70
JPPA	A balanced assessment between keeping a visual lookout and monitoring the radar
JPTG	The function of the ESD is to close loading valves, switch of power to cargo compressors and pumps
JPYF	 Area protected by halon
JQBS	To maintain the required pressure and flow to the machine in use.
JQCH	He wants the OS to show him where the switch that changes between automatic, manual, and emergency steering is
JQFQ	He wants the Chief Officer to organise a lifeboat drill
JQKS	the amplitude is modulated
JQLJ	Merchant Shipping Act 1995 and Merchant Shipping (Registration of Ships) Regs 1993
JQLN	Before leaving the port
JQMN	frequency
JQQS	At least two sets of instruments to detect each type of gas expected to be encountered?   
JQWN	 Fire main with fire valves
JQXA	Lowers oxygen content in the tank
JQYB	Class C fire 
JQYS	To have a hot-work permit
JRCD	an area excluding sea area A1 within the radiotelephone coverage of at least one MF coast station in which continuous DSC alerting is available
JRDY	1
JRHG	150 mtr
JRHI	the height of the aerial
JRLN	That the watch keeping personnel shall be ready for starting or manoeuvring the main engine.
JRUR	Vessel not under command and not making way
JRUT	Close the valves on both the Acetylene and the Oxygen bottles.
JSAJ	Receiving in mode J3E
JSBE	He shall arrange for proper, including medical, care.
JSFO	The supervisor's field is the work situation, the commitee's the total environment, also spare time
JSGE	To allow at least 3 hours of operation
JSIB	To bring the remaininig oil to the stripping suction
JSMW	By control of liquid flow
JSNV	You did not maintain a proper lookout by all available means
JSOP	Difficulty in breathing in and the casualty may be unable to speak.
JSWF	The water to  be drained periodically and scuppers to be closed in between. Oily water to be transferred to slop tanks or other suitable receptacle?
JTBC	Class A
JTIQ	The closed-type feed-water system
JTJS	along the curvature of the earth
JTLD	Start an additional auxiliary engine
JTPI	Vitamin C
JTQE	up to 150 persons
JTRF	sufficient buoyant oars or paddles provided with thole pins or crutches
JTXR	The General Civil Penalty Code § 315 .
JUEN	If you are taking bunker on the port side of the vessel, check that the starboard manifold is closed and blanked off
JUEQ	Cast off the rope.
JUES	to control the weardown of the main bearings.
JUHY	17284.0 kHz
JUIQ	The performance of the engine is reduced noticeably.
JUIS	No, the most effective rudder angle is about 25 to 30 degrees, this is because the rudder is "stalling" at 35 degrees angle
JUMT	You have a cracked liner, or cover.
JUPC	He wants two spring lines, four stern lines and no breasts
JUSP	Yes, cleaning is maintenance and contributes to keep expenses down.
JVBE	The chain is slack, dirty turbocharger or glogged turbocharger filter.
JVDO	Immediately reduce on the suction valve, and watch the Open more on the suction valve gauge.
JVIQ	action to be taken by crew and passengers
JVPG	The MS and FV (Health & Safety at Work) Regulations 1997 (The HSW Regulations)
JVPH	Connections on manifoilds and jumpers should be protected with spray shields to guard against spray.
JWAG	To fill up the lines slowly.
JWHU	a coast-station or coastguard-station
JWHW	G.Area
JWIN	Total pressure head
JWLW	Correct flow, pressure and temperature. ( Viscosity)
JWOJ	Position A.
JWUC	Keeping the lube oil in a state of low viscosity for a long period in the centrifuge bowl.
JWWL	a thermic detector
JWWN	Vitamin B
JWXG	Potatoes. 
JWXH	By permanently exhibited damage control plans
JWXI	For as long as people are working in the tank.
JWXR	All those listed in the other alternatives
JXNL	13.0 mm?       
JXQR	Rocket parachute flares
JXTB	Leave him in bed or request him to have some fresh air.
JXXF	Radiotelephony - Single sideband full carrier
JYCG	Start the fire pump
JYJE	Rudder hard to port, full astern. After you gain some sternway, rudder hard to starboard and full ahead
JYKY	Channel 16 plus another one
JYLQ	74 m2
JYLR	On the ship fire plan
JYLS	a radar reflector or a radar transponder
JYMM	None of the answers is good
JYNF	The control system is depending on the best possible process signal
JYNH	All these requirements apply
JYOE	1,0 Bar
JYQQ	Up to 90 C
JYQS	Outside the space which is to be protected
JYWL	6 - 25 watt
JYYX	A letter  "Exemption from the nationality requirement for foreign shipmasters"
KACN	A chemical tanker intended to transport cargoes mentioned in IBC/BCH chapter 17 with appreciably severe environmental and safety hazards which require significant preventive measures to preclude an escape of such cargo.
KAJE	Grind the valve against the valve seat to obtain a uniform sealing surface.
KANK	given by the EPIRB itself
KAVO	1301
KAVW	Not less than 10000 kJ
KBCO	16
KBCP	Air from stage one goes through discharge valves in stage one and through suction valves into stage two. In stage two it will be compressed to high pressure air.
KBEA	CBTs cargo tanks are also used for ballast, SBTs are not.
KBEX	Important due to different material and working conditions.
KBGS	Remove the cartridge and weigh it to check that it has the full weight stamped on it
KBXK	Your position, name, call sign and speed
KBYD	Membrane tanks are not self-supporting
KCCQ	the structure dimensions and the material of the coax cable
KCQT	Stop the purifier immediately, and make sure the oil is being feed to the bowl.                                   
KCRF	At exits and in corridors
KCRJ	To keep the lifeboat in an accurate position close to the vessel
KCSI	- 33° C
KDOB	She will most likely change heading to starboard
KDOW	Release gripes
KDSY	Seven short blasts followed by one prolonged blast
KDYY	The Norwegian Maritime Directorate determines the basic safety manning after an evaluation which includes, inter alia, job specifications and qualification requirements.
KEAK	F1B
KEAO	100% of the complement if it can be readily launched on either side of the ship. If it cannot be readily launched on either side, 100% must be provided on each side
KECH	Cold work permit +  Permit for entry .
KEGJ	GOV (gross observed volume).
KEGO	Vessel engaged in dredging or underwater operations, indicating that you should pass on the dredgers port side
KEJU	It is necessary to have a pilot ladder rigged and reaching from deck to the waterline, next to the pilot hoist.
KEKK	Give starboard rudder in order to balance the force of the bank effect and rudder effect
KEKN	Fasten seat belts
KEKU	2 entrances among which one is fitted with a semi-rigid boarding ramp
KELH	Stainless steel?
KELO	Order the dock man to shut down.
KEMH
SOLAS B PACK
KENW	Nine.
KEPR	Intra-ship traffic
KESU	2 compartments
KEUN	Any of the others.
KEVJ	Under the forecastle.
KFAI	Reduce the service interval
KFBJ	Hertz
KFCD	1000-2000 PPM Nitrate.
KFGL	FIC
KFHC	The vessel?
KFMA	Eggs
KFMF	Risk involves both identification of the occurrence and the likelihood that it will happen
KFMY	Center, alternately towards each end
KFQH	In a clarifier solids are removed from oil, whereas in a purifier solids and water are removed from oil
KFQI	Restriction in the usage of combustible materials
KFTT	The edge on the plunger which opens for the return line
KGBF	Vegetable oil and cooking oil
KGJR	The ISM Code is an international management code for the safe operation and for pollution prevention (Indian Safety Management (ISM) Code).
KGQE	If the work could result in a serious injury, the work should be stopped immediately, and the master informed, then improved control methods put in place- otherwise personnel involved informed and alternative work methods employed
KGTH	 Primary means of escape
KGTP	through hops between the ionised layers and the earth
KGYJ	Every 12 month
KHBC	Norwegian Seamen's Act, NIS Act
KHHS	The illumination in launching areas
KHJK	In the cargo tank there is a float on 99% filling that will give an alarm then close the loading valve to the tank when liquid reach the float
KHPI	15 ppm
KHPK	Do a complete sounding of all bunker tanks
KHRP	 International shore connection
KHRV	22777.0 kHz
KHSQ	High air pressure in water seal
KHTO	Accommodation
KHVA	Reduce main engine setting to stop
KHWQ	Water in the lubricating oil during service
KHWS	enhance the safety of lives at sea
KHWX	It should be possible to inert and maintain a O2 content of less than 2 %.
KICL	At least two sets of instruments to detect each type of gas expected to be encountered?   
KIKI	No, the tanker should show the normal navigation lights only
KILB	Injection valve has too high opening pressure.
KILD	As shown in figure 1.
KIMW	Rocket parachute flares
KIOJ	above the equator
KIQX	Organise a lookout system. Join up with other survival craft if possible. Stream the sea anchor
KIXP	Control by the master/employer and public supervisory authority that the requirements of law or agreement concerning the employee's service on board are satisfied.
KJFY	Loss of supply to one of the bearings.
KJIF	Maintain sufficient intact stability
KJIN	English or French
KJJK	it will have sufficient built in buoyancy to avoid the use of a lifejacket
KJPW	it can be dropped from a height of maximum 18 metres
KJSK	Each crew member signs in part b of the applicable crew agreement and the master or deputy signs in part c below the signature of the seamen. The discharge book is signed by the master and given to the seaman. An entry is made in the official log book ind
KJXL	Add some m? of cold water, preferably freshwater into the tank at high speed without pumping out in order to avoid heat reaction.
KJXP	Activate the nearest fire alarm button and advise bridge of the location of the fire.
KKDD	6 and 7 litres
KKEX	The water will explode into steam causing hot fat to be thrown far away thus possibly causing severe burns or fire.
KKFP	Within 68 ?C to 79 ?C
KKFS	High water level in the water seal
KKHQ	7
KKID	Rump.
KKNI	Strong acidic solution.
KKXI	Ropes made of natural fibres, such as manila or cotton with non-metallic, non-conductive equipment at the lower end?
KLAP	To secure the rope.
KLAT	Series of short blasts
KLDY	At intervals not exceeding 9 steps.
KLJY	Clogged turbocharger filters.
KLOY	 All of the answers are good
KLSC	In tanks not adjacent to the ship's shell plating having heating coils?
KMAT	Radiotelephony - Phase modulation
KMGN	Outside the colored zone.
KMJW	Gear pump
KMJY	Gravity disc is too small. Flow rate is too high
KMOT	 CO2 horn
KMRE	To measure the distance from the deck or tank cover measuring point to the liquid level in a tank.
KMTS	Distribution and weight of the containers?
KMVP	After it has been laid down
KMWH	The International Management Code for the Safe Operation of Ships and for Pollution Prevention
KNDQ	They must ensure that workers are provided with suitable protective clothing where it is needed
KNER	Inform passengers at frequent intervals over the public announcment system about the situation and how they shall act. Use as many of the ships officers and crew among the passengers to assist.
KNLD	For safety reasons, otherwise seawater could enter the engine room.
KNME	be automatically activated when floating in water
KNNW	Cover the spillage with a layer of foam.
KNOQ	Independent tank type A need secondary barrier
KNPO	180 kg
KNSC	Preparation of survival crafts' Emergency Position Indicating Radio Beacons (EPIRRB).
KNTU	length of painter
KOHT	Best use of the survival craft facilities in order to survive
KOHY	Not less than 5 min after starting from cold with the lifeboat out of the water
KOIR	To prevent the alternator from "motoring" by being supplied  power from other parallel alternator
KOLC	A relief valve.
KOLE	0600 - 1700 hrs
KONU	an operational compass provided with a binnacle
KOQG	Yes, if the ship, for example, is not in a seaworthy condition for the voyage and the master fails to take steps to remedy the defects
KOWW	Warm clothes, blankets and lifejackets
KPCA	Onboard training and instruction shall be given in addition to regular abandon ship drills
KPCW	Detergent.
KPEP	muster station
KPFD	Exhaust gas temperatures are higher than normal
KPGF	slow to get slow cooling.
KQAX	 Vessel aground
KQBB	To meet the requirements of goods to be transported
KQBV	FR
KQBY	To be sure that we do not have water collected in the cylinders.
KQCA	Provide clear warning that persons must not smoke in bed
KQCR	Survival craft portable radio
KQDQ	radio log or ship's log
KQEI	Name and Port of registry of your vessel.
KQIN	The deck cargo shall be stowed so that navigation and manoeuvring is not hampered.
KQNQ	Stop all cargo operations and close the deck IG line isolating valve
KQSM	Carry out procedures to instructions for cold work including filling in forms and having them signed.
KQUB	G =  I / R                                                                                                                                                                     
KQWV	Resistance, 3300 ohms                                                     
KRBW	People, officers and crew
KRDL	In a room especially meant for cleaning products.
KRDM	Gooseneck vent on main deck
KRDN	VHF channel 06 or 08
KRFV	Warning signs that indicate lack of oxygen inside
KRKE	The atmosphere should be gas free and contain at least 21% oxygen. 
KRMO	5 years
KRVT	FR01
KSGK	32
KSOC	+/- 0.06 bar  
KSPR	The aircraft wishes to inform or instruct survivors
KSTC	To remove solids, water and sludge.
KSWJ	be of sufficient strength to permit to pull the painter from the container and the inflation of the liferaft
KSXF	Charlie, Hotel, Alfa, November, November, Echo, Lima
KSXK	go to your muster station
KTIH	Situation Report.
KTIK	Over a wide range of temperature variations.
KTJF	they must not be used for any purpose
KTLP	Monitor the tank pressure closely and if necessary have the watchman to give the valve a little help to let the pressure out.
KTND	not less than 40% of total capacity of main pumps, but in any case not less than 25 m3/h 
KTNG	Transmission of ship to shore distress alerts
KTSB	Normal temperature of the lub oil after the cooler is approx. 45 C.
KTXA	Place the heel of one hand, two finger breadths above the bottom of breastbone. Cover the hand with the heel of the other hand.
KUCD	All the listed alternatives
KUGH	Until all crew members and passengers have reported to their respective muster stations
KUGI	Fouling of the hull
KULO	SOLAS
KUPP	give one of Inmarsat's "special accesscodes"
KVCA	Once every month
KVCC	Posted on the notice board on board.
KVES	be repeated after 3 and a half to 4 and a half minutes
KVPM	Excessive heating caused by over tightening of the gland packing.
KVQD	When the capacity requirement is higher than the performance of one centrifugal pump.
KVRB	A dry certificate has to be issued.
KVRE	Compressor discharge pressure
KVRG	Between 7 and 9.
KVUM	Increase safety for all ships in the area
KVUR	Amplitude modulation (AM)
KVVK	At all times
KVVL	R1 / R2  =  R3 / R4
KVXA	+75 C to +80 C
KVXC	Complete interchangeability of hose couplings and nozzles
KVXU	A rapid ringing of the bell forward followed by the gong aft for about 5 seconds at intervals of not more than 1 minute
KVYO	Crude oil washing.
KWCB	Regularly check the gyro against the magnetic compass
KWPJ	As soon as possible but not later than 2 weeks after he joins the ship
KWPM	Yes, must be cooled to 25° C.
KXLB	Human error
KYBY
they are fixed-temperature detectors
KYGT	Figure 2.
KYTH	By all the other mentioned alternatives.
KYUC	As an able seaman
KYVX	Opening water function missing.
LAAH	Letter M plus two other letters.
LAOL	To assist in the efficient and safe watchkeeping.
LARA	Breadth is given by B on the figure
LASX	Forcastle head, manifolds, maindeck?
LAYN	All of the items in the other alternatives should be done.
LAYU	Sufficient fuel to run at 6 knots for a period of at least 24 hours
LBGG	The use of the ship's line throwing apparatus.
LBGX	coax cable
LBSN	Increase the dosage of chemicals, and take new test of the water.      
LBVB	At least once a month if circumstances permit it
LBVY	The smallest diameter piston is the stage two piston.
LBWB	Allowance must be made for a running-in period with reduced speed and careful temperature monitoring.        
LBYM	urgency signal
LCFH	85 - 90  Centigrades.
LCGW	They must be fabricated of non-combustible material
LCMO	All of the mentioned alternatives.
LCPA	12.000 hours
LCQU	The General Civil Penalties Code § 315 .
LCQV	Start air supply
LCRT	The rotor blades are damaged or the blades are not properly cleaned
LDEA	The method of release from launching appliances.
LDGV	in a continuous way so that the powder spray is in the same direction as the one of the flame
LDHS	a.  blue  b.  gray   c.  orange                                             
LDIQ	Thick paper (old charts).
LDKV	A vessel engaged in fishing other than trawling, making way, with gear extending more than 150m from the vessel
LDLP	Double shut-off valves or by clearly identifiable blanks.
LDLS	Zero-Point
LDLY	Potato flour
LDOK	He wants the OS to show him where the switch that changes between automatic, manual, and emergency steering is
LDPC	one copy of the prescribed life-saving signals
LDPW	a means for collecting rain water
LEDM	OBQ (on board quantity).
LEKY	Radar transponder 
LEMO	listen out on VHF channel 16
LEQT	Yes, to avoid cold cargo to came in contact with the ship construction
LETE	TLV is threshold limit value and the unit is parts pr million ppm
LFAT	Governor droop settings on each prime mover
LFAV	During work in tanks, the gas concentration shall be checked every second hour
LFDG	Keep the manifoild closed and not let any cargo reach the cargo tanks, then call Chief officer/Captain.
LFTT	When an accident nearly occurs in connection with the operation of a ship
LFXF	3 phase excitation winding/rectifier bank/main field winding
LFYY	Formula 4 
LGGI	A ship's classification society recognized by the Norwegian Maritime Directorate.
LGHG	assigned frequency
LGSE	Decrease the speed as much as practicable
LGWL	Wire connected to chain through center lead or anchor chain
LHEQ	4
LHFO	Care, wages, free passage home
LHIW	Within 24 hrs.
LHND	CO2 plant.
LHSA	Separation of two insoluble liquids with different densities, and at the same time removal of solids.
LICU	Flash point
LICX	Keep the floors and decks free from fat and grease.
LIDV	Astern is defined as D on the figure
LIFP	 Flame detector
LIGK	Weekly
LIMC	Because the ship is leaving after sunset the following day
LINN	Neutral cleaner.
LIQF	Radiotelex and DSC - Frequency shift keying of carrier with error correction
LIQG	Slower
LIRE	Radiotelephony - Frequency modulation
LISN	Seaman's Act Section 5.
LISS	must also be kept after the implementation of GMDSS
LISU	directions for search operations
LIVF	cannot be charged
LIYJ	Use a rope ladder close to the raft to climb down and board
LJBE	A zener barrier is a unit made to obtain intrinsically safety in installations for instrumentation in hazardous areas.
LJEQ	125 %
LJIO	Relatively non linear characteristic
LJKN	one waterproof electric torch suitable for Morse signalling
LJLY	The vessel becomes sluggish in responding to the rudder
LJWW	Do not use loose garments, belts, ties or scarfs near winches and moving machinery.
LKCQ	Nine digits, beginning with a three (3).
LKDM	Sufficient foam concentrate shall be supplied to ensure at least one hour of foam generation
LKDO	Immediately reduce on the suction valve, and watch the gauge.
LKEJ	the use of SART transponders
LKHU	always sent twice
LKHX	Organize a lookout system and join up with other survival craft if possible. You should also stream the sea anchor
LKJO	as a fax
LKVE	 Area protected by sprinkler 
LKYH	In a pressure transmitter.
LLIP	Go to your lifeboat station
LLTF	Hand or body heat the affected parts skin-to-skin (e.g. frozen hand in persons opposite armpit...)
LLUA	Move the load in the direction of the signal man's hand.
LLUC	on the basis of a six second minimum charge with six second incremental steps
LLVU	Lubricating oil temperature is too high.
LLVW	Stow the product adjacent to a cargo which have a heating around the requested temperature for the isocyanate.
LLXP	0.2 A
LMCM	at least 15 % of N (*)
LMPX	Switch the UMS selector switch to manual mode and engage the "dead man alarm"
LMQS	Securite  Securite (3 times)
LMSK	Position A.
LMTI	A non-emulsifying agent with self splitting emulsifiers.
LMXF	everybody can read along
LNAV	In case of an emergency situation, the car deck can be difficulty to find the way around, and cars can shift position caused by ships movement.
LNDE	Everyone who may be in charge of life-saving equipment
LNEE	No, the vessel must wait his return or his replacement
LNGQ	the height of the layers of ionisation
LNKR	The water can be applied in a fine spray starting from the front in a sweeping motion
LNKX	Set the engine to dead slow ahead, and change the course 10 degrees to port
LNOD	Too long I-time
LOFV	clean the dust filter of the fan regularly
LOGQ	two buoyant rescue quoits
LOIY	to enhance the safety of lives at sea
LOKP	A large vessel overtaking a small vessel with little difference in speed between the two vessels
LOLK	Knowing exactly how the equipments are working.
LOPPD	lifebuoy with light and smoke
LOSI	In and outlet temperatures, and flow rates for both media
LOXC	Unsaturated hydrocarbons are colourless liquids with a sweetish odour and they are chemically reactive
LPFX	Windlass is given by B on the figure
LPHX	once a month
LPJV	Yes
LPOU	The employer must write an up-to-date policy statement and bring this to the notice of all on board
LPXX	Powder
LPYS	J3E
LQBJ	 a sea-anchor fitted with a shock-resistant hawser
LQFL	14 hours per day
LQGH	0
LQGJ	gooseneck vent on main deck
LQLH	Less than 12 to 1
LQRD	Shut down of inert gas blower
LQSV	Raise the boom, lower the load.
LQUE	Pork
LQWD	Figure 3.
LQXX	Open for the steam first to avoid freezing of condensate inside the heater.
LRBA	The best use of all survival craft facilities in order to survive
LRDS	The purpose of the IGC code is to provide an international standard for safe carriage of liquefied gases in bulk
LRIU	A person taking cargo samples must wear protective clothing.
LRNW	J3E
LROO	Gently flood the casualty's ear with terpid water so that the insect will float out.
LROQ	Check if any internal or hull leakages
LRSW	18,8 mA.                                                                          
LRSY	pH value 7.5
LRUI	a food ration for each person
LRWC	Indonesian waters
LRXW	Kg
LSCP	Seven (7).
LSDR	All of the alternatives together.
LSFC	Making the grab bucket/hook move up and down.
LSJL	Ore Bulk Oil.
LSRS	Acknowledgement request
LSSR	Wire for pulling burning ships off the pier
LSWV	Brass knife
LTCP	8,3 - 9.
LTGA	Isolated danger
LTIN	Broken water seal.
LTNI	A1
LTNL	406,025 et 121,5 MHz
LTQR	the length of the ship
LTXR	Yes, at the first port after his birthday, he would  sign off from the ALC1c and re-sign on in the ALC 1a section
LUAE	No, despite the fact that he promised to carry out several duties.
LUAT	The slave controller shall be in remote mode
LUDJ	Start engine
LUDO	To provide continuous digital selective calling coverage.
LUFB	According to the nomograms You select a gravity disc with larger hole diameter.
LUMK	Unannounced drills at any time
LUMM	Ball and butterfly valves are generally utilised on loading lines on gas carriers
LURR	622753420
LVDJ	Tanker vessels carrying oil
LVEH	Any of the others.
LVFA	muster and embarkation stations shall be readily accessible from accommodation and work areas
LVLW	Combustion suppression
LVMK
Warm nutritious drinks.
LVRO	Checking the operation of watertight doors, fire doors, fire dampers and relevant communication equipment
LVSL	Black
LVUY	38237
LVVO	Because the Captain expects fog early in the morning
LVVQ	5 l /m?/ min
LVXI	all the answers are correct
LVYA	PI-controller
LVYC	The ship is loaded in such a manner that adequate stability is achieved in all loading condition.
LWAA	ARQ followed by the coast-station's ID-number
LWBS	Lower lifeboat to water
LWDJ	The IGC code primarily deals with gas carriers design and equipment
LWKS	Check own vessel for any loss of life, danger of explosion and offer your assistance to the other vessel
LWND	2
LWPS	request of an "automatic telex test"
LWUP	Vessel "A", merchant vessel
LWXH	only send a positive delivery notification (PDN) to the sender if the sender requested, so in the send menu
LXHE	HM Coastguard
LXIT	A lamp, (0-50 mA) and a mA-meter in series.
LXNG	It must be constructed of approved non-combustible materials
LXSX	Enclosed Space Entry Permit and Cold Work Permit
LXTX	sky wave
LYIU	EPIRB
LYIV	No
LYKN	A remedy to which the mooring lines are made fast.
LYKO	Breadth is given by B on the figure
LYMA	Safetynet
MAAW	12 mA
MAFP	Echo, India, Golf, Hotel, Tango
MAFQ	Victor, Oscar, Lima, Uniform, Mike, Echo
MAJW	Atmospheric line
MAML	Secure hatches
MAOX	Powder.
MAUQ	4 kg
MBAT	the use of VHF DSC
MBER	Scavenge ports dirty.
MBFP	All alternatives
MBGK	Provide a replaceable wear surface for the pump housing/impeller.
MBJW	It adheres to the boiler tubes and reduce the heat transfer. It combines with solids to produce sticky deposits.
MBMG	+ 18.5 bar
MBOQ	To check condensate returns for oil.
MBRG	All answers are good
MBTS	The asphalt unlike sulphur is a viscous product and therefore does not transmit its heat easily to the steel bulkheads, allowing the steel to stay cooler than the cargo?
MBUO	Every person other than the Captain and the members of the crew or other persons employed or engaged onboard the ship in the business of that ship.
MBVJ	Remove the cartridge and weigh it as it has the full and empty weights stamped on it.
MBWH	a device to secure a painter near its bow with an inside release device that can be operated under tension
MBXC	2187,5 kHz
MCEM	Indefinite
MCEP	All of the mentioned alternatives.
MCIV	When anything unusual happens, and 30 minutes before the pilot station
MCKN	6
MCMC	Mackerel fillet
MCXS	not possible
MCYQ	Give relevant instructions and warnings.
MDDX	Physical checking the ramp/cargo holds/hoistable decks and see that everything are in order and the ship's gear correctly located?
MDHW	16 hours
MDIW	the operating certificates of the radio-operators must be shown
MDJK	28,0 tons
MDLC	To prevent the environment to be polluted if there is a leak on a cargo tank
MDNT	Start water-spray
MDNV	INMARSAT-A.
MDQG	Yes, provided it appears, amongst others, the wages and overtimepay and that it is subject to Norwegian laws and courts, but may be brought before a court in the employee's country of residence
MECU	They are to let go on the stern lines
MECX	Soft cloth on wide applier with handle.
MEDS	Make sure that the compartment has been evacuated
MEFG	Automatically, when the temperature is within a range from 68°C to 79 °C
MEIV	will immediately be detected within the coverage-area by the satellite's concerned
MEJJ	the use of MF DSC
MELX	ground wave
MEMY	Use a rope ladder close to the raft to climb down and board
MEPK	A bolt in every hole
MEWT	Broken water seal, oil outside the top disc.
MFBY	Make fast on the vessel's shoulder to push and pull
MFDO	5 miles
MFDQ	identify yourself with your call sign and /or ships name
MFNP	According to the IGC code liquefied gas is chemical with vapour pressure exceeding 2.8 bar absolute at 37,8oC
MGAY	all alternatives
MGCN	200 meters
MGCS	Hot work permit + Permit for entry.
MGPW	2,5 kg
MGVT	Every two years
MHHP	Do not use dangerous liquid detergents in closed spaces.
MHJG	Not permissible any where.
MHKY	ensure a flow of steam through the superheater when raising steam pressure after shut down
MHLN	Every three months, at least once a year 
MHMP	Prevent contamination if leaks are developed
MHNE	100 Tons
MHNK	Recirc. full open, fresh air intake closed.
MHNM	In ports only
MHPB	The welder shall have been instructed in the use of the ship's welding plant
MHRO	Segregate the oil in a separate tank for continuous purifying.
MIFX	9 GHz
MIIB	22 m.
MIJD	Lifeboat 
MIJF	must be replaced before the expiry date is exceeded
MIJY	MAYDAY RELAY (3x)
MILK	The boundary between oils and water?
MIOE	Fuel oil quality
MIQL	To reduce the general risk of fire in an unmanned engine  room.
MIQO	davit launched liferaft
MITU	Not allow the clothes to be hung anywhere in the unmanned machinery spaces.
MIWH	Legs bent, back straight, using leg muscles to lift
MJDT	Keep the keys with the Duty Officer/Electrician and call one of them when "Bypassing" is required.
MJKM	Vessel Response Plan
MJKW	a one-sided transmission meant for one vessel
MJPN	FEC
MJPV	Opacity, amount and colour
MJXV	 Fire station
MKAJ	Regulations of 11 Dec. 1981 concerning medical supplies etc on board ship  
MKAU	NOR
MKCF	the use of SART transponders
MKGM	to inform the NCS that one is available for messages offered
MKMI	Lack of oxygen?
MKNC	Department of Environment, Transport and Regions (DETR)
MKRE	If packing fails the pump can be kept running by tightening the glands, but if a mechanical seal fails it must be renewed to stop the leakage
MKTY	With both vessels underway, fig. 1
MKUM	the number of persons should be clearly stated on the outside of the boats bow
MKXA	Be checked at regular intervals for gas which might be released perhaps from sludge deposits; and if such gas found, the tank to be re-gas freed?
MLKK	The Certificate of Competency (or equivalent), the seaman's discharge book, the medical certificate and additional qualifications for specific types of ship e.g. tanker, high speed craft
MLRU	Increased velocity and decreased waterpressure around the ship's hull
MLRW	Connecting rod
MMCW	5 compressions after every 1 inflation
MMGB	39
MMMU	All the listed alternatives
MMMX	Temp sensitive semi-conductor
MMPK	Adjustment of Zero-point and span
MNGY	(Y)
MNHS	Negative
MNIN	Leave the engine room as quickly as possible, closing all doors behind you.
MNNO	By spring.
MNOM	A1,A2,A3 and A4
MNQU	1 meter
MNXM	Enough capacity to secure a certain draft.
MNYK	Sitting on a chair, leaning forward, with two fingers pressing the nose together.
MOBB	Closing must be possible from outside the spaces being ventilated
MOCN	Liver
MODM	Pushed by sufficient force to accurately check the correct opening pressure
MOGR	When he is properly relieved.
MOMN	to prevent contact with earth
MOQU	All passengers that will require some form for assistance in case of evacuation, etc. must be registered, so there can be sent crew to assist them if needed.
MOSN	seven digits, beginning by 1
MPAB	Panama lead is given by C on the figure
MPAV	MAYDAY RELAY (3x)
MPTB	A change in the viscosity of the mixture.
MPUV	60 Ah
MPYB	Peaches
MPYD	Before leaving the port
MPYH	He wants the OS to train as helmsman today, because they are sailing in open waters and there is not much traffic in the area
MPYI	Ensuring that all persons avoid smoking in bed.
MQBS	To make a copy of the NIS act and the CBA accessible to the crew if referred to in a contract
MQFA	Near to the deck, crawl out keeping your face as near to the deck as possible.
MQIM	Outside the coloured zone.
MQPV	Natural bends at intervals?
MREW	No
MRJA	As and when the manoeuvring vessel instructs them to do so.
MRJS	a remotely operated steering arrangement
MRNI	Removal of excess oxygen in the feed water.
MRTW	17.
MRWE	Checking the moorings for tightness/slack.
MRXG	to keep a listening watch on two channels more or less simultaneously
MSCB	Suspend all cargo transfer operations and close vents valves from the cargo system.
MSCD	Check the surface of the sliprings, polish if necessary and bed in the brushes
MSHH	Make sure that the compartment has been evacuated
MSHI	No need of any signal
MSIC
Use the intercom to inform crew and passengers of the reason for the alarm.
MSID	The vessel's cow manual.
MSLO	Once every month
MSMI	the floor of the raft has a second layer which can be inflated to help insulation, in addition to the thermal protective aids (10% of complement, minimum 2)
MSPP	VHF-channel 13 in the areas where the master deems it necessary
MSQK	The Seaworthiness Act.
MSSY	AF-gain
MSVK	A whistle and a light
MSXD	The sea chest valve.
MTBD	Undue overspeeding.
MTDB	Increase in draft to the point on your ship which is closest to the bottom
MTDD	Fuel injector
MTDT	Start engine
MTDW	To remove solids, water and sludge.
MTMD	the MMSI
MTNX	Operating instructions for life-saving appliances.
MTQH	During embarking and disembarking the driving ramp shall be securely locked to the recess of the ferry.
MTTQ	All of these.
MULC	Information about muster station on boarding card, poster in cabins, safety video running continuous.
MUNT	a class B fire
MUPE	Broken water seal, oil outside the top disc.
MUSR	Until all crew members and passengers have reported to their respective muster stations
MUUI	G3E
MUWW	A junction between two dissimilar metals generates a small voltage.
MVDM	a collect call
MVGA	Sodium hydrosulphite ,  potassium hydroxide, magnesium
MVGB	All the answers are good
MVJI	Polymerisation take place when a single molecule react with another molecule of the same substance to form a dimer
MVNV	30 minutes.
MVPG	8 %
MVPI	All the other alternatives
MVQI	Carry out a right or left hand search and proceed carefully  feeling the area in front with the foot and using the back of the free hand to check the area in front. 
MVSL	Relatively wide range of temperature measurement
MVST	4
MVTM	has a lateral field of vision of at least 120°
MVVV	The stern will "back" into the wind
MVYL	It is recommended, especially when dishes are heavily soiled.
MVYO	simplex
MWAH	Water Pump Pliers
MWIT	Frequency
MWLB	A zener barrier. (Positive)
MWOJ	covers the whole body with the exception of the head and hands and possibly feet
MWVC	the way in which radio waves travel are propagated
MXEE	Close the ventilation system and other openings to the hold in order to choke the fire
MXFW	Hold
MXGR	The oil relief valve on the cylinder block or the safety valve in the oil pump is sticking.
MXGV	The foam should be directed towards the bulkhead behind the fire and allowed to spread out slowly over the fire
MXIK	Lower lifeboat to water
MXIO	Always use correct working techniques for all cleaning duties.
MXKY	Dismantle the exchanger  and check or  renew the rubber packings.
MXLY	4,5 V                                                                                 
MXOG	Master's record and Documentation file.
MXSP	RF-gain
MXTI	the hydrostatic release unit
MYBP	Pan Pan   (3 times)
MYBQ	 A class division
MYBR	Total pressure head
MYDH	7
MYDJ	where reliable radio communication can be established with the use of a DSC on the MF frequency of 2187.5 kHz with one or more coast stations
MYGV	It's a cargo tank where all piping or venting piping are seperated and in not connected to other systems.
MYGW	Raise the fire alarm.
MYJB	controlling the movements of passengers.
MYNK	In J3E mode - on simplex basis
MYPX	The Norwegian Maritime Directorate
MYUS	You will be able to smell the presence of the actual gas if the consentration is 5 parts per million or more. 
MYYD	4
NADK	The cargo vapour is normally condensed against freon in a cascade cooling plant
NAJH	Body temperature below 35C / Heat the body
NAJJ	Separation of water and oil.
NASM	increasing with poorer cooling of the air in the air cooler.
NAUC	To fill up the lines slowly.
NAWY	so that neither craft nor stowage arrangement interfere with the general operation of the ship
NBCP	Cargo heater, cargo condenser, freon condenser, vaporiser, super heater, oil coolers, intermediate cooler
NBEB	Allyl alcohol is incompatible with propanolamine but both are compatible with benzene.
NBFY	It would be determined by risk assessment, but at very least would comprise safety line and harness, lifebuoy standing by, safety hat, boiler suit safety boots.
NBOJ	Flames are usually higher than the diameter of the fire
NBQX	Forces which bends the vessel up and down in the fore-aft direction (hogg/sagg).   fore-and-aft direction (hogg/sagg).
NBRR	If during a Port state or Flag state visit, or whilst carrying out a safety survey or in the event of an accident or incident and it is discovered that essential safety gear is inoperative or missing.
NBSF	the use of MF and/or VHF R/T
NBTI	Pivot point
NCDF	Clean the heat transfer surface
NCKV	Calculate the time of the sunset and then take the bearing
NCMM	less than 20m
NCMO	B keeps clear of A
NCNE	I(2) = 4 A
NCOG	four rocket parachute flares
NCOX	OR
NCTB	EPIRB 
NCUS	seven or more short blasts followed by one long blast
NDBP	The signs use black lettering on a white background
NDFR	Ventilate excessively?
NDGM	To ensure that we do not have any water assembly in the cylinders when the compressor start.
NDKP	- 38 V                                                                               
NDKR	Coal?  
NDLP	use of communication equipment
NDLR	sea-charts and navigating equipment
NDMF	Informal warning(s), Formal warning(s), Dismissal,
NDOY	Reduce the RPM to reduce the scavenge air temperature
NEAR	is important
NEAW	Secure hatches
NECK	Aft spring is defined as A on the figure
NEEW	an immersion suit or an anti-exposure suit
NEGL	As with no. 2
NEJV	at least 200 % N (lifeboat capacity: 100 % N; liferaft capacity: 100 % N) (*)
NELP	That the CBA expressly states that it applies to NIS ships and is subject to Norwegian laws and courts of law unless courts of another country is explicity mentioned.
NEQI	He would be signed in form ALC 1c
NFBH	Letter b.
NFDV	LF-gain
NFFQ	Searchlight to be provided at the launching station
NFGJ	Lower lifeboat to water
NFPJ	Lub oil cooler is clogged.
NFTP	None of the other alternatives
NFTW	Hold space is the space enclosed by the ship's structure in which a cargo containment system is situated
NFUP	either 10% of the number of persons the liferaft is permitted to accommodate or 2 whichever is the greater
NFVF	He wants the anchor secured thoroughly
NFVG	Check for proper air vent of the exchanger.
NFVL	Stop the engine and look for a fuel or water leak.
NGAH	The use of drogues
NGFM	Both local, remote from bridge and one emergency remote control station
NGOL	Rapid recovery shall be possible with the boat's full complement of persons and equipment
NGPG	The interface moves outwards
NGPM	either automatically on immersion or by a single manual motion or by mouth
NGQJ	A ship with a long, slim hull
NGST	Proportional increase  - higher temperature - more volume.
NGWA	always
NGXP	Each lifeboat shall be launched with its assigned crew, and manoeuvred in the water at least once every three months during an abandon ship drill.
NGXU	They may not carry cargo between Norwegian ports.
NHGF	Decrease.
NHLF	Any one of The Norwegian Maritime Directorate or the shipowner or the master.
NHPH	Should be informative for both operational parties?
NHUH	A continuous DSC watch on Channel 70.
NHUI	smoke going out the stack
NIAX	Blow down boiler and check condenser for leakage.
NIBB	A responsible Officer
NIBX	Hypothermia
NIDO	Inform the stevedore superintendent, the chief officer, and write a damage report?
NIDQ	S O S (Telegraphy)  /   MAYDAY  (Telephony)
NIDR	Clean the system and change the oil.
NIDT	The person who is designated in the muster list
NIGD	Co-ordinator Surface Search
NIHX	Greasy sludge from the compressor sticking between the fins in the air coolers, necessitating extra cleaning of these.
NIIL	No, drifting in ballast condition may be quite different
NIMS	lifebuoy with light
NING	All vessels carrying more than 10 000 gallons of oil , irrespective whether as cargo or bunker
NIUB	He will find new brake bands in the engine store
NJAV	All the mentioned alternatives.
NJBT	Segregated ballast tanker.
NJBY	12 h
NJOJ	10 minutes
NJWV	Sensitivity
NJXQ	Short circuit protection.
NKEH	Call the engineer on watch
NKJG	All answers are good
NKMQ	All work
NKPW	Reduce mechanical wear on the internal parts caused by vibration
NKSP	Improve material of intake air filters
NKVO	By have him demonstrate his ability
NKVW	IMO Solid Bulk Cargoes Code?
NLAA	the coast-station
NLCN
climb up and down vertical ladders from the survival craft embarkation point to the water
NLIE	 Foam installation
NLKW	Fire alarm bell
NLMM	A buoy or a lighthouse which is activated by a ship's radar, this is indicated by a marker on the radar
NMAS	It means that the product is included in the code because of it`s safety hazards.
NMBQ	Tell the jettyman to stop loading immediately.
NMKT	16 mA
NMRJ	a non-skid finish on all surfaces on which persons might walk
NMTV	3% of the total cargo volume.
NNDD	the speed of the vessel
NNEO	The engine officer in charge of bunkering on the receiving vessel
NNFL	Leaking injection valve.
NNFN	The position ensures that an open airway is maintained.
NNFR	2182 kHz.
NNJV	Yearly
NNOO	Lifebuoy with light and smoke
NNPO	not be sent by VHF-installation
NNPQ	Keep your working area clean and tidy.
NNSX	Piston rod
NNTP	ensuring that passengers and crew are made aware of the order to abandon ship
NNTR	The hydraulic pump is usually used for tightening the G-nuts
NNVH	Not specified exactly, but recommends at periods between 4 and 6 weeks
NOAH	Stand on dry insulating material and pull the person away with isolating material.
NOGG	Near to the entrance to the space
NOIP	1
NOIR	Enhanced Group Call
NOOL	Drill press
NOTM	 Area protected by CO2
NOYM	The P & I Club's nearest representative.
NPLF	Nylon.
NPQE	In the SOLAS convention and its annex
NPRT	 A class fire door
NPST	they always have access to the radio-equipment on board
NPVG	Mask, bottle, frame, medium pressure valve and low pressure valve
NPVV	Not to damage the rotor blades.
NPVY	Integral tanks are normally not allowed on gas carriers if the cargo to be carryed have boiling point less than -10oC at atmospheric pressure
NPWY	13 - 14° C 
NQAF	starting and operating the lifeboat engine
NQHW	 Smoke detector
NQKI	Likely cause a sudden or violent list due to the very large free surface in the broad beamed holds?
NQMS	They have had problems securing the gangway
NQQE	15 ppm
NQRT	Cargo ships below 300 tons gross
NQVA	how the order to abandon ship will be given
NQVW	Identification of the ship.
NRCQ	Powder.
NRCW	Everyone
NRDN	Annually or more frequently due to new methods being employed or following an accident
NRLY	15 PPM
NRMV	3,5?
NRMW	Aft is defined as A on the figure
NRNJ	Must not exceed 8% by volume.
NRNL	hatches positioned so as to allow launching and recovery operations to be performed without any occupant having to leave the enclosure
NRWS	All ships that are covered by the IMO safety conventions
NRWV	14
NSAY	Gear pump
NSDK	There isn't longtitudal bulkhead in membrane tanks
NSGS	Not recommended at all.
NSJD	Forward is given by C on the figure
NSNF	Lifejacket
NSOF	be sent by an MF-installation on the DSC-distress frequency
NSRP	3 min
NSRR	The FW-HT is circulated in a closed system, cooling cylinder jackets on Main Engine and aux. Engines
NTAR	Both systems use same chart datum
NTBL	Air suppression
NTBS	Open, when pressure in the boiler is in excess of normal working pressure.
NTCQ	By inhaling, skin penetrating, skin absorbing and swallowing
NTDJ	None of the above
NTFU	To avoid backflow of gas to the engine?
NTJA	F1B
NTJV	half of the total number of lifebuoys provided on board
NTJX	routine
NTRG	So neither the rescue boat nor its launching arrangements will interfere with any survival craft at any other launching station.
NTVN	He must sign on in section ALC 1c of the crew agreement, and his hours of work would be carefully monitored and would involve risk assessments being carried out to ensure that he can carry out the tasks given him
NTWM	Maintain the specified boiling temperature
NTXB	Direction B
NUIA	25 %
NUSE	T T T (Telegraphy) / SECURITE (Telephony)
NUTE	Into the crankcase and mix with the lube oil.
NUUX	Square System
NUVL	7m
NVAO	Every port
NVAQ	Details of ship, the date of first entry, and list of Masters
NVEO	Inerted to less than 8% oxygen(IMO).
NVKL	G3E
NVKP	Line fuses and overcurrent relays
NVQH	Shear forces and bending moments.
NVRF	To do a full calibration.
NVSA	By immersing them in buckets with oil and water.
NVSX	Your ship will sheer to starboard rather quickly with the possible consequence of grounding
NWDX	The frequency of the incoming alternator is the same as that of the main switchboard
NWFJ	The infrared radiation and ultraviolet radiation given off by flames
NWHD	Bimetallic strips need time to cool down
NWJN	Because you may cut your fingers.
NWKI	The  surveyor is checking that the emergency exits are properly marked, free from obstacles and that the closing devices are easy operable.
NWLI	Midships is given by B on the figure
NWNS	Upper.
NWRF	6
NWSS	date of replacement of the battery
NXCC	The signal which is stated in the muster list
NXCD	All mentioned functions
NXEM	All combustible materials
NXFE	None
NXTS	On the cargo tank area all time?
NYAJ	For safety reasons, to ensure that all explosive atmosphere inside the boiler is removed.
NYBB	a disc aerial is used
NYBH	Somewhere aft of the center of gravity, but it is impossible to pin-point the exact location
NYFJ	Dismantle the exchanger and check or renew the rubber packings.
NYFL	Purging inertgas, purging air, inspect, purging inertgas?
NYSN	Correct donning of life-jackets
NYWA	Information related to fire fighting equipment, release systems etc. do we find in ship fire plan.
NYWT	Pump out a small quantity from each tank at the first opportunity , to avoid having an overflow to deck when you put heating to the tank
OAES	An abbreviation of American Petroleum Institute.
OAQC	Hot work
OATS	200 nm and capacity for evacuating more then 15 persons.
OBCW	Fire extinguishers equipped for powder or CO2 only.
OBEQ	2
OBJN	The load connected to the switchboard
OBLY	Only if approved by the Flag State
OBNS	At the deck level and near the bulwark top level.
OBNV	Wrong installation will result in a major deviation in measurement
OBPJ	38237
OBRV	All the mentioned alternatives.
OBYL	Embarkation ladder
OCEG	Central cooling system
OCJJ	check that we have an open discharge line all the way to the pressure bottle.
OCKG	a manually controlled lamp fitted on the outside
OCSM	two minutes
OCSO	J3E
OCYK	Metals 
ODAG	Any of the mentioned extinguishers 
ODBF	Wire for pulling burning ships off the pier
ODEH	All the answers are good
ODFH	access hatches which can be closed watertight
ODMV	The method of launching from within the survival craft
ODNH	make contact with an RCC
ODTM	2 - 3 %
OEEI	westerly and northerly direction
OEQU	Fasten seat belts
OEUA	It is more easy to give correct pressure to the fractured/injured area, and the control of swelling and bleeding is more easy to observe.
OEVU	Procedures according to instructions for hot and cold work should be carried out and necessary forms filled in
OEVV	Bearing damage.
OEWT	Abeam is defined as A on the figure
OEXO	When the machinery spaces are in the manned condition.
OEXP	have self-bailing arrangements
OFBQ	1,200 litres of free air
OFGT	Aft spring is defined as A on the figure
OFHS	Class B fire
OFLW	Starting and operating radio life-saving appliances
OFPV	Can not produce enough energy to ignite a gas (explode)?
OFQT	Seelonce Distress
OFSJ	Pick up for tachometer is wrongly adjusted.
OFXF	med +
OGEA	No
OGEV	Outside the space which is to be protected
OGHH	To neutralize the acids occurring in the condensate system.
OGLP	To get rid of sludge in the water chamber.
OGNG	mayday (1x), call-sign of ship in distress (3x) / this is / own call-sign (3x) / received mayday
OGNH	There are three types of independent tanks, type A, B and C
OGPR	All the mentioned alternatives ?
OGQP	Pushed by sufficient force to accurately check the correct adjusting pressure.
OGXE	blending LF & HF signals
OHCB	Heat the ballbearing in oil, and put it on the shaft.
OHDB	 PAN-PAN
OHDY	In the Flag State official language with copies in English or French
OHEU	100 - 300 PPM CaCO3.
OHFV	Parallel System
OHGM	Painted red/yellow/red with the red bands 0.1 meter (0.33 feet) wide, and the middle yellow band 0.8 meter (2.64 feet) wide; and  Labelled ''VAPOR'' in black letters at least 50 millimetres (2 inches) high.
OHNX	three tin-openers and a pair of scissors
OHQF
A pharmacy authorised or accepted by the Norwegian Board of Health or, if no such pharnacy is available, the master and a doctor approved by a Norwegian Consulate shall perform inspection once every 12 months.
OHQH	To clarify circumstances and causes of an occurrence with particular reference to the seaworthiness of the ship and safety at sea.
OHSY	1,0 - 1,5 watt
OHTW	30   -   300 MHz
OIBJ	2 miles
OIDU	The performance of the engine is reduced noticeably
OIDW	Constant flow, clean probes and temperature below 60 Degr.C.
OIEQ	No
OIPL	21 %
OIXQ	Triac                                                                                 
OJEL	1906 hours UTC on the 17th of the month
OJEM	No he is exempt from signing
OJFG	Alkaline detergent (strong).
OJHX	month
OJLA	All of the mentioned alternatives.
OJRA	10 Mohm
OJRC	5 %
OJXP	C
OKBI	41
OKKG	on ships on short international voyages, each lifeboat shall be launched and manouvered in the water at least every six months
OKMB	Bringing the engine up to sufficient number of revolutions for combustion to take place and engine to run
OKUF	Search the engine room, make sure all personnel is out. -Stop ventilation. -Close for all air access. -Upon approval of the Master, release the halon/CO2.
OKWV	a testing program built in for this purpose
OLBD	Stop the washing process and not resume until the oxygen content in the tank is below 8%.
OLHT	Every three months.
OLKG	Anchor ball
OLLX	ionisation layers
OLNU	Prevents the backflow of inert gasses into nonhazardous areas
OLTI	fitted with water pockets of a highly visible colour and so designed as to fill to at least 60% of their capacity within 25 seconds of deployement
OLXQ	The Act relating to hours of work and the Seamen's Act
OMCP	The tank shall be mechanically ventilated as long as there are people inside it.
OMDJ	The camshaft rotates with half the RPM of the crankshaft on a 4 stroke engine.
OMGR	2
OMHQ	Blow the bunker hose to avoid oil spill when the hose is disconnected
OMIP	TC
OMXQ	Only Merchant Shipping Notices (MSNs)
ONDK	Not less than 20 changes per hour.
ONFS	To make sure the job is done under controlled conditions
ONGT	FLEETNET
ONHN	The percentage of the L.E.L. in the ambient air
ONJG	Close the valves on both bottles, first the acetylene and then the oxygen bottle
ONKB	Inmarsat-C equipment
ONPW	How to release from launching appliances
ONQR	Safety shoes or safety boots
ONUY	No it is not
OOAU	Power dissipation capability
OOAW	By giving the vessel a starboard turn
OOHJ	Ask your superior for advice before attempting to operate it.
OOKQ	The master and the shipowner are responsible for the adequate manning of the ship.
OOMJ	Goggles and shield.
OOSW	Give information on survival craft capacity
OOYE	Investigating accidents/incidents and making reports
OPNU	All the mentioned alternatives.
OPPO	The vessel will roll violently?
OPQN	The thermostat has one or more contacts (open or closed) depending on the temperature/setting. The temperature transmitter converts a temperature signal to an electric signal.
OPRI	4 Rocket parachute / 6 hand flares / 2 buoyant smoke.
OPSV	Government Authorities of the Flag State
OPWD	One hose for each fire hydrant
OPWI	Oregano
OQHJ	Frequency
OQIC	Every three months
OQJQ	heat the feed-water
OQKO	Fuel injection advanced too far due to incorrect preinjection angle.
OQLL	Notify the engine room of the procedure.
OQOS	1 metre
OQPL	be provided with a painter system with a breaking strength of not more than 2.2 kN
OQUS	30 litres pr. nautical mile
ORDD	Cut it with the knife contained in the equipment locker
OREP	Smoking is only permitted in designated places.
ORFJ	Fat fish
ORHE	To relief pressure in a crankcase explosion
ORIW	C(S) =  4 µF
ORMA	70
OROR	TX: 2177.0 kHzRX: 2177.0 kHz
ORXC	1250 m3
OSAI	Immediately stop the discharging.
OSAK	 Portable fire extinguisher
OSDQ	Personnel authorized by the master?
OSDY	The primary controller in a cascade control system
OSER	Yes.
OSFJ	two sea-anchors, one being spare
OSFK	Strong alkaline solution.
OSIO	F1B
OSNR	Read off  the compass and keep her steady on the course
OSPJ	Yes, in ship of 76 m in length and longer, a double bottom shall be fitted midship, and extend to the fore and after peak bulkheads, or as near as practicable.
OSTK	Just prior to reaching the water, the lanyard should be pulled. This sets the hook which will automatically release once the raft is waterborne
OTAE	Mechanical and chemical.
OTDK	Release gripes 
OTFG	In the SOLAS convention.
OTGX	a coax cable of proper impedance
OTQA	Higher temperature leads to lower literweight.
OTTM	20ppm
OTUG	Discharge the washing to shore reception facilities only?
OTUI	Increase dosage.
OTYF	The bow may be sucked against, and the stern may be pushed away from the other ship as you pass
OUDL	pressed in during speaking only to work semi-duplex
OUMN	It is easier to damage a centrifugal pump than a piston pump if they run dry.
OUOE	Transistor                                                                         
OUOJ	Inmarsat -B and -M
OURT	Each vessel vapor connection flange must have a permanently attached 0.5 inch diameter stud at least 1.0 inch long projecting outward from the flange face. The stud must be located at the top of the flange, midway between bolt holes, and in line with the bolt hole pattern.
OVDG	3
OVHR	Pale or grey.
OVKD	The officer in charge at the barge or the foreman in charge if it is at a shore facility
OVKW	Reactive load (kVAR)
OVKY	Fuel oil with poor combustion properties.
OVLW	A variable electric signal.
OVQS	2182 kHz/VHF channel 16
OVRL	Copy of crew agreement posted in a conspicuous place giving details of relevant information and contractual clauses as per ALC 1d
OVRM	One
OVSH	On the fire control plan
OVUT	Neutral to alkaline solution.
OVUY	the calling station
OVVR	On ILO 22
OWAU	Cotton
OWBR	Secure all burners
OWDI	Survival craft distress pyrotechnic signals
OWFT	water
OWFX	A vessel may proceed only when it has received specific orders to do so
OWGL	Grapes
OWGN	It is how many degrees a ship continues to turn after you apply counter-rudder
OWLM	A garage tweendeck on a passenger ferry 
OWLQ	41821
OWOE	Too much combustion air
OWQM	Most attacks take place in territorial waters
OWRH	2000
OXAN	3 long blasts repeatedly
OXAS	To avoid the compressor-oil  to disappear from the crankcase during starting.
OXET	December
OXFU	Direction-finders to be installed on, or as near the navigating bridge as possible
OXKW	you must call on another working channel
OXLR	That the strainer needs cleaning.
OXYX	To maximize discharge outturn?
OYAM	3 meters
OYMC	It`s a product added into a cargo in order to keep the cargo stable. This cargo should never be blanked with nitrogen because the inhibitor needs oxygen to be effctive.
OYTW	Match the size and capacity of the ship's loading line, venting system and static generation hazard limitation, if any?
OYTX	From the water space.
OYXH	It will give full back flow at the time the pump stops.
OYYQ	10 000 kJ/person
PANF	Use water extinguisher to put out the fire.
PAOY	He is to help the other crew members and fetch more Vaseline from the storage room if they run short
PAQS	Consult with the instruction manual for the equipment in question for correct values.
PAQV	All of the mentioned equipment.
PAUY	the use of SART transponders
PBHG	60 minutes
PBIF	A unit subordinate to a rescue co-ordinating centre
PBKR	The slave controller receives the set-point from the output signal of the master controller
PBKT	Navigate the vessel on ground as soon as possible
PBQI	6
PBRK	give a bright red light during the entire emission time
PBTW	equally spaced, not less than 300 mm or more than 380 mm
PBVP	Any of the others.
PCCF	The diameter will be the same whatever initial speed we have when starting the turn
PCHA	Passenger ships carrying more than 36 passengers
PCHF	Fats
PCHH	Transducer
PCIV	Distress call
PCJS	The floor surface becomes cleaner.
PCJU	85% of the gas can be discharged into the space within two minutes
PCOU	Seek advice from your superior before attempting to operate it.
PCVI	Class C fire 
PDJX	3
PDPR	Weekly
PETM	20 - 100 meters.
PETN	remove any oil or scum on water surface
PEUL	Fuel oil pipes or filters are clogged.
PEVX	Nothing for the first 24 hours, then 1/2 litre per day (more in the tropics)
PEWY	instructions for immediate action
PFDR	Place sterile dressing over the burn and secure with a bandage.
PFDT	Primary and secondary slop tank.
PFKA	At the gangway.
PFKF
Safety purpose?
PFNQ	the old mariphone must be checked out and the new one must be checked in
PFNU	Near to the deck, crawl out keeping your face as near to the deck as possible
PFOM	Never.
PFPG	Pork
PFRD	To take part in public traffic
PGFF	Blow down boiler and reduce dosage.
PGHS	Dispersement of chemicals?                                            
PGHU	As the second course.
PGII	instructions or diagrams printed on its casing by the manufacturer
PGIK	Ventilation must be capable of being stopped from an easily accessible position outside the space being served
PGKC	Stop the engine before meeting, and apply engine during meeting
PGNP	0
PGSL	 Injection pump failure.
PGXN	Remaining on board.
PGXQ	To get rid of sludge in the water chamber.
PHEI	Silverside
PHFB	To maintain a tank at atmospheric or overpressure.
PHGS	Greasy sludge from the compressor sticking between the fins in the air coolers, necessitating extra cleaning of these.
PHLT	to deliver a message by telephone via a modem on the computer of the subscriber
PHOE	Kkkk
PHPE	not allowing undue ingress of water after a jump from a height of not less than 4,5 m into the water
PIAV	Ethylene is the gas produced by most fruits and vegetables during the ripening process
PIBQ	in urgent cases
PIIA	It is double acting oil free piston compressors
PITC	Total content of organic and inorganic acids in the oil.
PIUV	may only be present at the place, as indicated in the license
PIWK	An efficient engine room watch with the main engine on standby be maintained.
PJCN	Yes, if an employment agreement refers to the collective wage agreement
PJEU	TX: 8415.0 kHzRX: 8436.5 kHz
PJKV	Section on Births and Deaths to be completed, and entries made in Official Log Book detailing circumstances of the death and actions taken on board. Deceased is signed off the crew agreement in his absence
PJQQ	+  85° C
PJRQ	Pre-wash the tanks with cold water first?
PJSY	Owner or master
PJTD	Unloaded.
PJTT	Exhaust gas boiler fouled.
PJUX	The nearest coastal radio station
PKFN	Maximum filling limit of cargo tanks on gas carriers is 98% if the liquid temperature is equal to safety valve reference temperature
PKKU	Feed the pump from the sea water inlet pipe.
PKPS	To get the oil into the cylinder when the piston is in the right position.
PKRF	From the stripping pump's delivery side directly to the manifold's presentation flange.
PKSA	Start air supply
PKUQ	a number which indicates the nationality of the ship
PKUT	background noise in receiving a weak FM-signal
PLDX	To ensure that the proper residuals of treatment chemicals, as specified, are maintained all time.
PLEV	Transfer heat from one fluid to another
PLMY	1 entrance fitted with a semi-rigid boarding ramp
PLOS	a 10 cm radar.
PLOX	MMSI-number
PLRF	No.
PLVK	Comply with all the requirements listed here
PMBF	Milk
PMCW	They have to bunker fuel oil and diesel oil
PMCX	Evaluation of the situation, rescue and life-saving, confinement of fire, extinction, then feed back on the emergency
PMCY	No.2 generator trips on reverse power
PMFR	Salted and dried rack of mutton, mashed swedes, boiled potatoes.
PMOS	atmospheric line
PNAE	8 %
PNAF	To single up to one line and spring forward
PNBY	All personnel onboard (crew and passengers) must be registered to keep a track of number of people onboard.
PNON	6
PNUJ	Lifeboats shall be stowed attached to launching appliances.
PNWR	The name of the person responsible for the oil discharge
PNYN	be given no receipt  indubitably too distant from the distress-case
POAD	Measure the amount of explosive gases in % of LEL.
POAH	By showing the ship's register
PODI	Every report or message must be logged including time and date
PODJ	Wilful misconduct, gross negligence and violation of Federal Safety
POEH	a one-sided transmission
POJH	Class B fire
POLB	Organize a lookout system and join up with other survival craft if possible. You should also stream the sea anchor
POLU	The water will explode into steam causing hot fat to be thrown far away thus possibly causing severe burns or fire.
POPC	The method and use of sea-anchors (drogues)
POSK	Bulkheads constructed of approved non-combustible materials but do not meet any of the requirements relative to smoke and flame nor limitations relative to temperature rise.
POSP	Every fifth year with a periodical survey every 12. month.
POUC	Start with intermittent firing, using small firing periods and long intervals gradually building up to longer firing periods and shorter intervals.
POVA	To monitor the cable/wires for break.
POVX	Due to temperature expansion.
POWT	lifejacket
PPNJ	In stairways, corridors and escape routes
PPNK	A will take 1/3 of the extra load. B will take 2/3 of the extra load
PPOI	0
PPTF	All ships covered by Chapter IV of SOLAS I.e. all cargo ships of 300GRT and above and all passenger ships on International voyages
PPYD	to ask for 'maritime inquiries
PQBN	Using nets
PQFE	By turning up the rope on the bitts, fig. 1
PQFU	 B class fire door self closing
PQIJ	This is the best place to land
PQNK	immersion suits for the number of persons the boat is permitted to accommodate
PQOV	lifeboat
PQPC	Owners submits delivery certificate and proof of eligibility, RSS send Carving note, vessel is "Carved", completed carving note returned to RSS, RSS issue Register
PRBR	Orifice plate
PRDJ	The dedicated heavy weather ballast tank
PRDY	The Chief Officer wants the 1st Engineer to empty the starboard bilge in hold No. 5
PREC	Calcium
PREE	not always radiotelex
PRHG	Pressure
PRJE	ensuring that a supply of blankets is taken to the survival craft
PROF	The national DSC-call frequencies of the coast-station concerned
PRQS	Protective clothing, safety shoes, gloves, goggles, earmuffs.
PRRL	Conduction, convection and radiation
PSEX	Water extinguisher.
PSIB	the frequency actually used by transmitter and receiver
PSNB	Overboard discharge is stopped.
PSUV	The Chief Officer
PSXB	Rocket parachute flares
PSYS	Use of breathing apparatus
PTDV	high/low power
PTEU	frequency modulation is often applied in the maritime VHF-range (band)
PTFK	Protect against corrosion
PTIX	Only one type of launching and recovery arrangements shall be used for similar survival crafts onboard the ship
PTNV	422753810
PTQH	5:20 pm (17:20)
PTQI	An area of defined dimensions within which search and rescue services are provided
PTRD	Metals 
PTTS	Dirty scavenging air cooler on the air side.
PTUO	Ship's captain
PTWE	R(Pt100) = R1 - R2
PUBC	The shipping company and the master
PUHC	Stop the purifier immediately. Check the bowl for heavy side,   deposits, bearings, housing, and the spindle for damage.
PUPO	11 00
PUQJ	Report it immediately to the chief engineer
PUSR	Throw a lifebuoy over board and report to the bridge immediately.
PUUL	Urgent call
PVGY	Enables sludge to be discharged directly to shore tanks
PVHA	 Manually operated call point
PVIR	Reduce speed temporarily and increase cylinder oil consumption.
PVSS	At the first occurrence he would be given an informal warning, if the offence occurs again, this may lead to a formal warning
PWDQ	+2 bar
PWEN	on the basis of a three minute minimum charge with one minute incremental steps
PWKH	can not be adjusted, this is set by the manufacturer
PWOI	the captain
PWPD	Neutral cleaners.
PWUB	When we have a higher cargo tank pressure than the corresponded in the table, it means that we have inert or nitrogen left in the tank or the cargo itself is not clean
PWVY	Because the manometer units change with the atmospheric pressure and all values start at vacuum
PWXQ	Information about muster station on boarding card, poster in cabins, safety video running continuous.
PWYO	To secure the rope
PXDL	Upper explosive limit.
PXHP	56 hors
PXKF	Wearing and fastening of lifejackets and associated equipment
PXNM	Gives reference number as per crew agreement, and name of each crew member on board
PXNO	Melting heat.
PXTG	5 seconds
PXXG	Use the winch. Forerunner and wire stopper to pick up the slack and stop the wire. One man operating each. Make the forerunner fast on the bit, releasing the eye of wire and the stopper, lower the wire easy by forerunner
PYHM	When the boiler is firing on high rate.
PYHO	Closing of watertight doors, fire doors, valves, scuppers, sidescuttles, skylights.
PYIH	6
PYIK	Increased.
PYKD
To deal with emergencies and safety of the ship
PYKE	Emergency shut down.
PYPA	Every four months
PYQV	One prolonged blast followed by two short blasts at intervals of not more than two minutes
PYRQ	Stripping pump.
PYTF	To prevent serious damages on main components.
PYUA	Maintain a safe distance, apply the extinguishing agent to the base of the flames with the wind behind us
PYWM	A vessel engaged in fishing other than trawling not making way through the water
QABD	permit the wearer to swim a short distance through the water and board a survival craft
QAJN	Cast steel, Iron, Brass & Bronze.
QAKI	At least one
QALV	Natural bends at intervals?
QAMT	He wants the anchor secured thoroughly
QAPI	Carry out a right or left hand search and proceed carefully, feeling the area in front with the foot and using the back of the free hand to check the area around. 
QAUC	the water level
QBDI	5
QBEJ	Mutual agreement between participating vessels
QBEL	37 m2
QBGU	Drain the water into the sloptank
QBHO	The chemicals make it difficult to remove the oil from  the water
QBIM	I can find out from sea trials or test on my own
QBVS	One self-contained air breathing apparatus (Not using stored oxygen), protective clothing, boots, gloves and tight-fitting goggles, fire and chemical resistance lifeline and explosion-proof lamp.
QBVV	He is supposed to paint the evaporator and use a brush to apply the paint
QCCO	Oil Detection Monitoring Equipment.
QCDH	Figure 3
QCNI	always simplex
QCQP	Stop operation?
QDBP	Every 5th year?
QDFT	liferaft
QDGL	polar
QDID	100% of the complement if it can be readily launched on either side of the ship. If it cannot be readily launched on either side, 100% must be provided on each side
QDND	All bolts to be in position and tightened?
QDRM	The person in charge must report the spill to the US Coast Guard
QDSH	the transmitting antenna has broken down
QDUW	Stiffening of the thin metal sheet.
QDXJ	He is to help the other crew members and fetch more Vaseline from the storage room if they run short
QEAB	an urgent call
QEAU	 Clogged exhaust gas system.
QEID	Once every month
QEMG	Stop bunkering
QEMI	Make it possible to drain to shore the remaining cargo in the ship's lines and pumps, after the discharging is completed
QERF	Electrodes
QERG	Switch over to the other pump and inform the CE of the noise immediately.
QESD	one waterproof electric torch suitable for Morse signalling
QFBP	The ship's safety plan.
QFHG	The respiratory organs.
QFJV	Start engine
QFNX	Self contained breathing apparatus in addition to normal safety equipment.
QFPK	SARSAT-COSPAS EPIRBS
QFRB	ITU
QFRG	received messages which aren't intended for own ship are not used
QFUQ	1 minute
QGBC	Place sterile dressing over the burn and secure with a bandage.
QGEN	1 - 2 years.
QGER	Departure and arrival ballast tanks plus 25% of remaining cargo tanks for sludge control.
QGEW	Two prolonged blasts followed by one short blast
QGHC	The sea-trial tests may tell me, or else I can do a test myself to find out
QGIV	All the answers are good
QGPJ	All pipelines or components which may be isolated in a liquid-full condition should be provided with relief valve
QGPL	Liquefied gases is mostly a mixture of hydro carbons
QGPP	In such locations that no point in the engine room is more than 10 m walking distance from an extinguisher
QGSA	have a sufficient length of non-combustible line behind the rocket
QGTO	instruction in the use of radio life-saving appliances
QGTQ	Pressure/vacuum valve.
QGXX	Yes
QHEK	SECURITE
QHHU	watertight receptacles containing 3l of fresh water for each person (may be partially replaced by a desalting apparatus)
QHKJ	7,5  kN
QHQI	Pump will overheat
QHRY	Position A
QHUG	All the mentioned alternatives.
QHYQ	Two vessels engaged in pair trawling
QIAE	Insert a blank flange on the line between the slop tanks and the rest of the cargo compartments?
QIFA	Norwegian laws unless explicitly otherwise provided in or pursuant to a statute
QIGW	until it is manually turned off or is temporary interrupted by a message on the public address system
QIOL	MGN's; MSN's and Statutory Instruments
QIVI	either a manual system or a power starting system with two independent rechargeable energy sources
QIXR	Near the entrance to that space
QJGW	Absolute pressure is atmospheric pressure added with manometer pressure, to be used in technical tables
QJLX	The shore-side of the cargo manifold valves, port and starboard side
QJMW	Plugging the scuppers
QJOF	Radar transponder
QJOH	Making the complete crane move port and starboard.
QJTG	Packages of 500 g each
QKCU	Raise the feed water temperature.
QKGW	By reducing your speed until vessel "D" is cleared
QKHP	The deck for the lifeboats.
QKHR	the adjustment of the cam/camshaft of the engine.
QKLO	Air filter to turbocharger fouled or damaged.
QKLW	the build-in test facilities in the modem
QKMN	Start engine
QKRO	He would inform master that ship was unseaworthy, and that the emergency fire pump must be rectified before the ship can sail or the Safety Equipment certificate can be endorsed
QKVR	lifebuoy with line
QLFS	Regulations of the light on the PPI.
QLHH	All of these mentioned must be provided
QLKA	For cooling and to maintain correct viscosity on the fuel when injected.
QLMO	In the main section VI,  letter F.
QLRK	be able to identify oneself
QLTD	operation of davits used for launching liferafts
QMBL	Warm nutritious drinks.
QMBN	He wants all the lashings tightened and two extra chains fastened to each container
QMFV	125 pct?
QMKY	5 °
QMWE	release the liferaft at a depth of not more than 4 metros
QMWG	To check out if the rules of ISGOTT Chapter 10 is followed.
QMXA	He is worried that oil will run through the outlets and into the sea
QMYC	Horizontal
QNGM	 Injection valve opening pressure is too high.
QNVJ	Notify Chief Engineer, find cause of leakage, remedy the leakage and then immediately start to clean the bilges
QNVP	10% of the number of persons the liferaft is designed to carry, or two, whichever is the greatest
QNXY	must be replaced when the seal is broken
QOCD	At least every three months
QOCF	3
QONU	Keep the floors and decks free from fat and grease.
QORA	A
QOSA	Call immediately the person in charge.
QOSC	3 years.
QOTU	Pump the oil to the incinerator tank.
QOUP	The Master
QPBC	To avoid backflow of gas to the engine?
QPIQ	Standard Marine Navigational Vocabulary.
QPJL	Inner diameter of impeller is bigger due to cavitations, or outer diameter reduced by erosion.
QPKF	Cold drinks and salt.
QPMT	Figure C
QPMY	Use a rope ladder close to the raft to climb down and board
QPPH	IMO Grain Rules?
QPPI	Figure 4
QPYR	1 N/mm2
QQBE	He shall have all the knowledge as listed in the other alternatives
QQCV	a whistle and a light
QQEL	Survival craft portable radio
QQFI	highest possible frequency that will be reflected by the ionosphere
QQFL	Every time the machine has been used.
QRAA	Construction of all internal bulkheads of class "A" divisions
QRBC	16 or 22 MHz-band
QRKE	The methods of retrieval
QRUF	Gas concentration measuring and examination in connection with cleaning and gas freeing shall be carried out by  the safety  delegate.
QRVV	to jump from a height of 4.5m into the water without being injured or damaging the suit
QRXO	98 %
QSBA	GEC-Marconi
QSBU	above water escape for its occupants after automatically positioned in damaged condition
QSQU	That no solid beam of fuel shall be present
QSRN	A heavily leaking starting air valve  can cause an explosion in the starting air pipe system.
QSRP	Body temperature below 35C / Heat the body
QSRS	At three levels for at least two places in the tank.
QSUB	Line throwing appliance
QSXM	15 kg/cm?
QSXN	Inform RDR by mail of the sale of the mariphone
QSXP	it stops the spreading of smoke and flames during one hour
QSYH	Engage the turning gear on the engine.
QTBT	be prepared and approved by the Administration before the ship proceeds to sea
QTDK	Absorption drier gives the lowest dew point down to -60oC
QTFE	Clearing escape routes
QTHR	Camshaft
QTLR	F1B
QTOF	Vitamin E
QTSJ	Draught is given by D on the figure
QTYE	the radiotelephony distress fequency in the band in which the DSC distress alert was received
QUEX	all the answers are good
QUEY	Dibromomethane.
QULK	8
QULS
In the meat freezer
QUNH	Embarkation ladder
QUNI	To assist in dealing with crew, cargo or ship regards whilst in a foreign port
QUOY	Because serious structural damage and overflow can be caused by the creation of pressure in the tanks during this operations. 
QUQP	That there is great concern and interest regarding the safety at sea
QUUQ	List of Call Signs and Numerical Identities
QUUS	LES
QVCN	Wait for a resuscitator to be brought from the ship's first aid locker and use it?
QVEY	Alkalinity of the lubricating oil.
QVFT	10 ampere during 20 hours
QVFU	3 White star rockets
QVLG	has inherent buoyancy of at least 70N
QVRB	The Maritime Act
QVSY	24 houres
QWBM	Lube oil cooler.
QWBO	Increase in condenser pressure.
QWEQ	All ships.
QWFO	All of the mentioned alternatives.
QWJQ	reporting to stations and preparing for the duties described in the muster list
QXAK	Extinguishing attempt is started immediately
QXFN	Heat exchangers that are utilised for cargo handling must be designed and tested to tolerate the products the carrier is registered to transport
QXGH	The ship's fire plan.
QXGL	Normal jacket water temperature after the cooler is approx. 80 C
QXIB	One in which the atmosphere may have a deficiency of oxygen or may have a toxic gas
QXLI	If the seaman brings a case of unfair dismissal against the Master/Company, it serves to ensure that  all details have been recorded and is admissible as evidence
QXMC	General emergency alarm to be tested daily
QXXB	Within coverage of the INMARSAT system.
QYAI	The use of helicopter rescue gear
QYAM	30 metres
QYBG	indicate on what frequency communication will be continued
QYMA	 Secondary means of escape
QYNU	Prevent air accumulation in the cooling water system
QYOS	Throttling of delivery valve
QYQB	1000ppm
QYRW	Your assistance is no longer required
QYUD	Helmet, safety shoes, gloves and protecting cloths.
RABL	 Push button for fire alarm
RAGG	Line throwing appliance
RAHA	Renew lub oil in the system.
RAHB	Near the entrance to that space
RAKK	Rescue Co-ordination Centre
RALO	with the exception of the A1 and A2 area, within the coverage of an Inmarsat satellite'in which continuous alerting is possible
RAMF	Four (4) days.
RARA	By a telecom report followed by a report on a personal injury report form
RARC	Information regarding maximum deck cargo permitted shall be available.
RARK	The confined space always has six sides
RAVI	Rescue boats shall be stowed attached to launching appliances
RBCW	The master or his qualified representative must be on the bridge at all times
RBDT	Must be capable of being stopped from an easily accessible position outside the space being served
RCCV	The Chief Engineer
RCFG	Yes
RCLB	Report to bridge or duty officer, actuate the fire alarm, call the persons around the fire and join the fire squad
RCLC	smothering and cooling
RCLY	All the mentioned alternatives ?
RCOH	No, if this is done the lifetime of the inhibitor will be reduced.
RCTK	Prevent damage to sensitive electronic components from high voltage tester
RCWF	3
RCWR	The main diesel generator or shaft generator.
RCXT	Boneless beef entrecote
RDBW	International Oil Pollution Prevention Certificate, UK Oil Pollution Prevention Certificate, Safety Construction Certificate  of Fitness.
RDFA	Throughput too high.
RDFC	Changing of filter element would not interrupt the engine operation.
RDPC	The apparatus shall be capable of being operated on VHF channel 16
RDRP	579.2 kW
RDSN	White flour
RDSP	To reduce the free surface "sloshing" on the cargo
RDWQ	F1B
RENR	Fully knowledgeable of the content.
REOI	The current and wind are holding the vessel back
RFBU	G3E
RFFV	Alkaline.
RFGW	Longer
RFHP	Overheating of the piston, and oil coke deposits in the cooling chambers.
RFJB	Dismantle the rotor and assemble the sealing plate
RFJD	Vessel steering a few degrees off weather / sea (approx 30 degree)
RFKY	Arrange ment for rowing
RFPA	the distance travelled by a radio vibration in a period
RGAY	Suction valve open, delivery valve closed
RGBR	Better linearity and increased accuracy
RGCL	B-15
RGCP	Once every month.
RGEC	0 - 7
RGFD	To the satisfaction of the administration
RGFU	In all professions you have to learn before you can manage a job.
RGGR	the use of MF and/or VHF R/T
RGMJ	ensuring that every passenger is provided with an immersion suit or a thermal protective aid
RGQQ	Harness with a rope secured to a safe point on the ship.
RGVO	Outside the colored zone.
RGVQ	The product is both flammable and toxic.
RGYC	Telephone
RHCF	The Very High Frequency (VHF) band.
RHFP	send a DSC distress alert relay
RHGO	A vessel is aground
RHKU	We mean maximum allowed relieve valve setting
RHWK	The difference between maximum and minimum measurement that gives a standard output signal
RHWP	No, the turning diameter will be increased in shallow water
RHXD	Start air supply
RHYX	By audible and visual signals at the control panel
RIFO	In a secure and sheltered position and protected from damage by fire or explosion.
RIGH	C
RIHE	Means of access, working environment, working conditions and general compliance with regulations
RIIT	+2 bar
RIOP	Good radio communication facilities (preferable 2182 kHz and/or 156.8 MHz (channel 16) radiotelephony and 500 kHz radiotelegraphy)
RIPO	In conjunction with the senior watchkeeper and electrician, isolate valves, electrical supply, automatics and post  'Do not operate' signs before commencing work.
RIRG	A described UMS-mode check shall always be carried out prior to leaving the engine room, irrespective of the time he will be absent.
RIRJ	Vessel with a high block coefficient
RITQ	At all times
RIUL	Either Oil fitting equipment , or Oily-water separating equipment , or combination of both.
RIVP	the use of MF DSC
RIWF	child's lifejacket
RJHC	Ch.13
RJWB	Woodward regulator will regulate very slowly
RKFK	Report to and discuss with the Master.
RKHY	While at sea the installation shall be maintained in a satisfactory condition
RKIR	About 10 %
RKIX	Within range of VHF coast radio stations.
RKJP	Waterline corresponding to deepest allowed draft permitted by subdivision requirements
RKKC	immersion suit
RKLD	PAN PAN
RKMT	The diffuser ring is damaged.
RKMV	No, high-level alarms should be a separate system.
RKOI	00 followed by an MID-number and a station number
RKPG	NAVTEX and EGC-receiver
RKPK	Promptly locate the fire and raise the alarm
RKPM	Yes, one if the ship is under 500 brt. And two if the ship is over 500 brt.
RKRA	A surveyor from one of the 6 societies authorised by the MCA
RKSY	Put the rudder about half way to port to slow down the turning rate
RKWT	Not at temperatures used for pre-heating
RKWU	Foam is the main medium for tank deck fire fighting on oil tankers
RLAM	Checking that lifejackets are correctly donned
RLDL	No, when the speed exceeds 5 knots we have not much help in a tug
RLEI	1.5 litre
RLFI	Because you may cut your fingers.
RLMB	100% of the ship's complement on each side
RLPJ	Cold drinks and salt.
RLPK	Class A
RLVB	Use of dedicated, clean dry transfer equipment, ie. buckets, tubing and pumps
RLVD	All of the mentioned alternatives.
RLYO	Cast steel, Iron, Brass & Bronze.
RMHT	SEC On tankers over 10 years old
RMIN	Where possible the master shall provide such service. Cost and other circumstances may be taken into consideration.
RMNJ	20 minutes if there is inert gas; 30 minutes if there is not
RMPC	Fluorine and/or bromine
RMTF	Close the valves on both bottles, first the acetylene and then the oxygen bottle
RMTH	85 - 90  Centigrades.
RMUB	Instruction for emergency repair of fire-fighting equipment
RMUI	At room temperature.
RMUY	Vapour at low pressure.
RMXG	The anchor to be all way in the hawsepipe and secured by brake on winch and wire/chain stopper
RMXL	Means shall be available to prevent any discharge of water on to survival craft during abandonment
RNCS	until all crew members and passengers have reported to their respective muster stations
RNEG	the height
RNFB	Verify that the sefarer has been given his rights according to law or agreement, make entries in the sea service book or record of service, have a report on seamen sent to the Maritime Employer/Employee Register.
RNFT	reporting to stations and preparing for the duties described in the muster list
RNFX	Scrubber.
RNOD	Integrator                                                                          
RNOE	 Fire alarm panel
RNOG	The method of release from launching appliances
RNPW	Inform the bridge about the reason for blackout, and expected time to restart.
RNSP	Fast FWD and AFT in center lead to pull the vessel out from the jetty and make it in position for voyage
RNTY	No. 2
RNUD	child's lifejacket
ROML	21% oxygen by volume and 0% hydrocarbon of LEL.
RONJ	50 enclosed spaces
ROSD	instructions on how to survive
ROVT	All over the world
RPBK	He must instigate an investigation. He must inform the complainants of his findings and make recommendations as may be necessary
RPHF
The controller will not react on a process change in a specific range
RPIE	To avoid an explosion in case of oil have been leaking into the boiler furnace.
RPIG	He is to notify the Chief Officer
RPJS	To know specificly where to clean every day/week/month.
RPLM	Latex?
RPSC	Sierra, Hotel, India, Papa
RPUA	ensuring that passengers and crew are made aware of the order to abandon ship
RPUT	Broken water seal.
RQDA	When anything unusual happens, and 30 minutes before the pilot station
RQDD	+/- 50° C
RQDE	a MF/HF-antenna
RQKV	a 50 Ohm resistance coax cable
RQRK	No, they are not compatible.
RREN	evacuation slide
RRLK	Abeam is defined as A on the figure
RRRD	At the gangway.
RRRG	Plan for safety preparedness
RRWD	Using sinking agents
RRYQ	 Yes
RSFL	Collect rain water
RSHB	The vessel is proceeding at 7 knots or more, is more than 12 miles off land and is in a water depth of 25 metres or more.
RSSX	Stop the engine immediately and keep the lube oil pump running for at least 20 minutes before opening the crankcase
RTLE	After use
RTMY	Radiation burns.
RTOK	Both master and shipping company.
RTPF	Ask your superior for advise before attempting to operate it.
RTQE	Extinguishing attempt is started immediately
RTTQ	Inform the master
RUEJ	Check for proper air vent of the exchanger.
RUQY	Inter-ship channel
RUTJ	Bowl opens unintentionally during operation.
RUYL	Disposed of in an ashtray and ensuring that it is extinguished.
RVAV	F1B
RVBW	Yes, freon reacts with open flame to a poisonous gas (Fosgen).
RVED	Closing must be possible from outside the spaces being ventilated
RVGU	Start engine
RVHM	Forward is given by C on the figure
RVYE	Making the complete crane move fore and aft.
RWGN	per minute or parts of it
RWGX	To prevent forming a potential flammable gas cloud
RWKT	Yes, transit passage through US waters to a non US port
RWUV	He should take the padlock inside the room.
RWWQ	It depends on the installation
RXCL	Put the rudder 10 degrees to starboard
RXFR	liferaft
RXKT	This is firezones which can be divided from eachother with firedoors. If a fire start in one zone, all firedoors in front and aft of the fire will be closed from the bridge to stop the smoke and fire from spreading.
RXOA	every week
RXRE	Give a kick ahead
RXRM	First wash and then rinse with fresh water from hose.
RXRO	Activate bridge watchkeeping receivers and attract the attention of the person on watch.
RXRQ	Stop pumps  -  report  -  clean up?
RXTB	one buoyant rescue quoit, attached to not less than 30m of buoyant line
RXTW	Because these metals have a very low thermal expantion coefficient and do not burst of extreme low temperatures
RXWG	Increased turbocharger revolutions.
RYDF	5 %
RYJV	Legs bent, back straight, using leg muscles to lift
RYML	Activate the nearest fire alarm button and advise bridge of the location of the fire
RYMM	A calculation example showing the use of  "KG"  limitation curves.
RYNA	a searchlight which can work continuously for not less than 3hours
RYOR	Dirty scavenging air cooler on the air side
RYOX	All of these.
RYUT	the height of the aerial
RYWE	The use of all survival equipment
RYYY	4,50 m
SAGM	Disposed of in an ashtray, ensuring that it is extinguished
SAGQ	the frequency chosen
SAHK	The ship's safety plan
SAHL	Stern line is given by A on the figure
SAHM	To avoid liquid coming back to the compressor during start up.
SAHN	Separation of two insoluble liquids with different densities, and at the same time removing of solids.
SAMO	Yes, if engaged by the owner.
SAOD	20 Nautical Miles
SAPX	The employer.
SBBT	The boiler be allowed to cool down by its own after shut down. Then pump the water out.
SBCL	Figure 1.
SBCM	In J3E mode - on simplex basis
SBGQ	Impossible to say
SBMI	STCW deals with minimum recommendation of education for seafarers and minimum standards for training centre and schools
SBVR	only necessary radio conversations are made in a concise and businesslike way
SBVS	Due to suction, the two ships will be sucked together
SBXE	Sitting on a chair, leaning forward, with two fingers pressing the nose together
SBXF	The governor
SBXY	Swing the load in the direction of the signal man's face
SCBL	Class1
SCCH	Every 6 months
SCDY	13
SCJU	Turbocharger
SCPN	1000 000 000 Hz
SCQR	Activate the alarm, evacuate the area and seal the place, then activate the extinction system
SCUT	The regulations are a part of the Norwegian Ship Control Legislation regulations, concerning production and serving of foodstuffs.
SCXB	Sound the fire alarm signal
SDDX	Reduced heat capacity of the heater
SDOU	Wire takes 95 % of the extra load. Rope takes 5 % of the extra load
SDPN	SOLAS
SDPO	3.5 to 4.5 mtrs.
SDSA	Air, Breathing, Circulation.
SDUS	2 on new-builds only. Old ships have to comply by August -95
SDYS	Lima, Oscar, Bravo, India, Tango, Hotel
SEBC	The shore-side of the cargo manifold valves, port and starboard side
SELB	Small diameter line.
SELD	Change operation to the third generator set, preparing the original set for  repair of the failure and switching to manual mode until repair is carried out.
SEQK	one waterproof electric torch suitable for Morse signalling
SERD	perform all duties associated with abandonment, assist others and operate a rescue boat
SEYS	Separation of solid contaminants from a liquid.
SFGC	one daylight signalling mirror with instructions
SFGF	OR gate
SFIO	100/amplification
SGBA	He wants the OS to train as helmsman today, because they are sailing in open waters and there is not much traffic in the area
SGBB	Central gas extinguishing system and/or waterfog.
SGIK	should exceed 1,5 % of the lifeboat length when loaded with 50 % of the number of persons the lifeboat is permitted to accommodate, these persons being seated to one side of the centreline
SGPK	Wrong, if the valve is wrongly set
SGWS	Oil Transfer Procedures Manual
SGYJ	windows on both sides which can be closed watertight and opened for ventilation
SGYN	Worn scrapper and piston rings.
SHDI	Yes, within thirty (30) minutes
SHEL	Muster station 
SHFF	Foam.
SHHQ	By carrying out a risk assessment
SHNN	1
SHRS	Check list for periodic inspections
SHSJ	Sound the fire alarm signal and send the seaman on watch down to inspect and report the situation
SIAX	the choice of the inmarsat-region
SIIH	To take reasonable care of himself and fellow workers and co-operate with any person with any statutory duty imposed upon him in relating to Health & Safety
SINL	Survival craft portable radio
SIOB	Above 200 deg C
SIUA	Check the position only
SIWL	to guarantee reception of NAVTEX-reports
SIXI	2187,5 kHz
SJHN	5 minutes
SJIH	call the engineer on watch
SJIJ	Survival craft distress pyrotechnic signals
SJKT	Pick up a life jacket
SJLS	None of the alternatives.
SJLU	check that we have an open discharge line all the way to the pressure bottle.
SJOB	They must be fabricated of non-combustible material
SJOG	Public Correspondence Station.
SJTA	lifebuoy with light
SJUT	Lifeboat 
SKCL	518KHZ
SKDI	Lube oil cooler
SKFS	It shall be properly stored and prepared for another meal.
SKFX	All of the alternatives
SKGN	Where the sills of the sidescuttles are below the margin line
SKHD	Dismantle the rotor and assemble the sealing plate.
SKKP	Cause oxidation which increase viscosity.
SKLS	a survival manual
SKPM	SES or an EGC receiver
SLCC	Yes, the lift force will be dramatically reduced
SLGH	Any ship of 500 gross tonnage and upwards
SLGL	a call for account of the receiver
SLGM	1300210
SLHF	Close them to prevent the spread of fire, and allow the extinguishant to be released without time wasting.
SLHH	Within  200 nm of US waters including Guam, Hawaii, Alaska and San Juan
SLKR	Low-pressure switch is jammed closed
SLYO	The exhaust gas receiver
SMBG	send a PDN, if the message has arrived in the mailbox
SMFK	Life saving
SMHG	Both the suction and spill valves are controlled
SMKM	Code of Safe Working Practice for Merchant Seamen (COSWP)
SMPN	He is informed by the ship/agent, relays information to the RSS, arranges completion of documentation and may assist with having the deceased returned to home country
SMSW	To keep the oil protective film between moving metal  surfaces .            
SMUI	Proceed at highest speed to the distress source position.
SMUN	Exhaust gas leaking into the oil chamber.
SMWG	Class A bulkhead
SMXY	Under keel clearance is given by C on the figure
SNUK	evacuation slide
SNXR	use the intercom to inform crew and passengers of the reason for the alarm
SOAH	F1B
SOKG	The water level is between the water cock connection of the boiler, and the bottom of the gauge glass. It is safe to put feed water into the boiler.
SOKH
Maritime investigators, The Telecommunications Administration, the Electrical Inspectorate, and other public institutions, Det norske Veritas and other approved survey institutions, other private institutions of foreign countries, the authorities of foreign countries
SOMW	All officers who takes part in the operation, preferably also the deck hands.
SOON	Heating coils are to be pressure tested, preferable by the heating medium. Test to be recorded.
SOSQ	It is a public record and is admissible in a UK court of law
SOWV	21% oxygen by volume and 0% hydrocarbon of LEL.
SPAG	the weak link
SPBW	100 dB
SPEH	Completely loose its share of the load causing the auxiliary engine to speed up
SPFC	Resistance sensor, Pt100
SPGA	11 shackles
SPHQ	A certificate with information regarding the inhibitor added such as type, oxygen dependence, date added, duration of effectiveness,  max adjecent temperature, lifetime and other limitations.
SPLA	an area within the radiotelephone coverage of at least one VHF coast station in which continuous DSC alerting is available
SPVV	Organic chemistry are substances that contain of hydrocarbons
SPWU	Yes, on all ships that comply with MARPOL 73/78 annex 1 must have oil record book onboard
SPYJ	The Master
SQHQ	ALC 6
SQJK	The Norwegian Maritime Directorate.
SQSQ	By asking different crew members specific questions relating to the familiarization training
SQUE	Inverter                                                                             
SQYA	Grind the valve against the valve seat to obtain a uniform sealing surface
SRAU	have a floor capable of being sufficiently insulated against cold by means of inflated compartments, or by equally efficient means not dependant on inflation
SRBP	V(2) =   50 V
SRBU	Acid detergent.
SRCN	1 litre
SREE	15 June 1987.
SROD	In any country by an MCA Marine Officer
SRPA	2 men 
SRRN	Foam
SRSF	Stern is given by C on the figure
SRTC	Restrictions regarding length and breadth exists. Draft restrictions vary with seasonal changes.
SRTH	All the measurements mentioned must be performed.
SRVV	Port quarter is given by D on the figure
SRXH	Sidereal hour angle
SSGN	It keeps the boat alongside the embarkation deck so that the tracing pennants can be released
SSHM	A unit which automatically releases the liferaft/lifeboat at a depth of approx 4 metres.
SSMG	Measuring distance from cargo level to ullage point
SSOA	Posted or available where it can be easily seen and used by crew-members engaged in the discharge  operation.
SSOY	The ship would be due to sail
SSPQ	5mg/m3
SSPX	Chief cook and second cook work together to select provisions for officers and crew, discussing needs and quantities, if necessary.
SSSK	12.000 hours.
SSWK	The flue gas plant
STBN	All of the mentioned equipment.
STJU	sufficient number of pumps and bailers
STMG	1.25 times?
STQJ	2 digit code telex services
STQL	Digital Selective Call
STRE	To minimise oil losses and prevent the sludge getting too hard
STUQ	Charge air pressure is too low.
STYA	When it is fitted with a guard or similar device which prevents foreseeable contact between a person, his clothing or items held in his hands, whilst it is in operation
SUCA	Large fenders meant for floating between vessels and absorbing considerable impact. Example of fender size: L - 4.5 m. Dia. - 3.3 m.
SUFL	Start water-spray
SUFQ	By use of cable stopper backed up by brake with chain slightly slack between stopper and winch
SUKO	not less than 3 metres
SUPJ	The pressure control valve will automatically close, the ventilation valve will open
SUSU	Manning of fire parties assigned to deal with fires.
SVAP	Sector System
SVBG	Of low expansion, viscous and solid, easily contaminated by hydrocarbons
SVEQ	2187,5 khz
SVIW	Every three months
SVSR	4.5 bar
SVUP	Voltmeter and synchroscope
SVYO	Any remaining grinding paste will corrode on the metal surface and after some time the needle will be damaged
SWAI	child's lifejacket
SWCT	Lower than or equal to 61?C 
SWIT	A product with flashpoint below 60 ° C.
SWMR	Conductivity test.
SWQC	He wants the heating coils inspected
SWQI	Figure 1
SWRC	Right if the immersion depth is smaller than 100mm 
SWRP	To bring the remaininig oil to the stripping suction
SWRV	When the lifeboat is flooded
SWVX	Broken water seal, oil outside the top disc.
SWYL	Yes
SXAI	soot would be swept toward the uptakes
SXAJ	SOLAS
SXHQ	Small changes in temperature can cause large movement of the interface
SXJJ	Figure 1.
SXPA	He wants two spring lines, four stern lines and no breasts
SXRU	He should take the padlock inside the room.
SXRV	The number of persons should be clearly stated on the outside of the boats bow
SXTE	The heading will most likely change by a large amount
SXTH	the use of HF DSC and SARSAT COSPAS Epirbs
SYAD	To remove solids, water and sludge.
SYAI	Gate valves, globe valves and butterfly valves.
SYIE	By audible and visual signals at the control panel,  distinct from the fire signal
SYIP	Ensuring that all persons avoid smoking in bed.
SYNP	Fasten seat belts
SYPG	the testing function of the device
SYPY	Continue with manual operated engine room until the maintenance work is finished
SYSO	10 kN
SYWS	By control of liquid flow
SYXR	For safety reasons, to ensure that all explosive atmosphere inside the boiler is removed.
SYYL	Reject the offer?
TAFD	- 20°  C
TAGC	The location of the beacon is determined by Doppler shift measurement
TAHA	one (two for a 13 person accommodation) buoyant bailer
TAIP	5 years
TAKH	A tankerman certificate
TAKJ	On all short international voyages, muster of passengers shall take place as soon as possible after departure
TALF	TX: 2177.0 kHzRX: 2177.0 kHz
TAQH	To ensure safe and efficient operation.
TASR	This tank must be inerted if carrying a flammable product (Flash Point<60°C).  
TAVB	Reject it?
TAXN	Put on your life jacket.
TBAY	a buoyant bailer and two buckets
TBGU	That the Seamen's Act applies in full
TBSL	That all vessel's water tight ramps and doors are locked and secured at sea.
TBUY	After the separator shell has warmed up. 
TBVW	Greater than the pressure in the lubricating system.
TBXU	A period not exceeding 24 months
TCFW	To control the tank atmosphere by introducing the required inert gas.
TCGV	12 - 16 times per minute
TCQW	Put the rudder full starboard.
TCQX	To the master according to his instructions
TCUD	Every 5th year.
TCYE	406.0 MHz Cospas-Sarsat EPIRB
TDJH	Prior to sailing
TDKX	100 Tons.
TDPX	Same powers as Marine officers in that they can detain a vessel, conduct an inquiry into an incident/accident and start legal proceedings against the persons involved
TDVP	Its always possible to put the turning unit in a fixed position, so the MF distress frequencies can still be used
TDVR	alerting
TDWO	The confined space always has six sides
TEDC	Midships is given by B on the figure
TEEY	Drill press
TEFQ	Operate valves gradually
TEFS	All of the mentioned alternatives.
TEIE	The buoy may not be in its charted position
TEJW	Draught is given by D on the figure
TETA	at the beginning of every watch
TFDX	Enclosed Space Entry Permit and Cold Work Permit.
TFGO	Llebuoy with light and smoke
TFKV	TX: 2187.5 kHzRX: 2187.5 kHz
TGBK	10 minutes
TGER	That the CBA expressly states that it applies to NIS ships and is subject to Norwegian laws and courts of law unless courts of another country is explicitly mentioned.
TGHE	The relevant regulations'  Section 8.
TGNC	General Mundial Distress and Safety System.
TGWD	all the answers are correct
TGXW	Close the ventilation system and other openings to the hold in order to choke the fire
THAN	always immediately detected by the satellites concerned
THBE	to regulate the light
THOS	EPIRB
THQB	Means shall be available to prevent any discharge of water on to survival crafts during abandonment.
THXS	The use of onboard communication systems
THXV	in ASCII
TIFE	120 mm above the water (in calm water)
TIJL	If we have a sudden drop in pressure after the valve is supposed to be closed, this is caused by a leak
TIKJ	Bad management and poorly maintained old ships over several years have proven to be fatal
TIMW	The side from the wind.
TIPH	As stated by shipper?
TIQA	one whistle or equivalent
TITO	13
TIXV	IX
TJCM	Heating of the feed-water
TJEO	Discharge to a shore facility only
TJJI	have self-bailing arrangements
TJKB	Distress relay call
TJQW	Fire control plans.
TKAB	for radiotelex-traffic in the MF/HF bands between ship and shore stations
TKBU	In stairways and corridors
TKED	International Maritime Organization (IMO)
TKFX	to enhance the safety of lives at sea
TKGC	access hatches capable of being opened and closed from both sides
TKGR
Increase cylinder oil consumption, determine fuel quality and readjust the fuel oil purifiers
TKLD	Once a month
TKRN	Dry extinguishing remedy.
TKTI	Within 24 hours, or within 14 days in relation to serious injuries
TLDL	6
TLEF	Yes if the cargo compartment is designed for temperature down to -48oC
TLKF	Table 11 and 13.
TLNN	The ITU List of Coast Stations
TLPT	CT2, WT2 port, WT2 starboard.
TLPV	4000m3/h at 120 meter liquid column. (delivery head).
TLRO	Remove any contaminated clothing and flood the affected area with slowly running water.  Make sure that the  contaminated water drains away freely and safely.  
TLRP	According to the specific eductor`s performance curve.
TLTI	Place the heel of one hand, two finger breadths above the bottom of breastbone. Cover the hand with the heel of the other hand.
TMEE	It depends on the installation
TMFC	It is important that the rotation direction is correct to avoid dry running.
TMMM	Distribution and weight of the containers?
TMQK	Total weight in tons of cargo, equipment, complement, stores and supplies on summer freeboard in saltwater
TMRE	Tins of 850 g each
TMSD	Fatty fish
TNAU	 Wood
TNBS	Cut it with the safety knife stowed on the exterior of the canopy close to the painter attachment point
TNJV	continuously after having been immersed for a period of 10 seconds under 100mm of water
TNLK	Because the Captain expects fog early in the morning
TNLM	Behind one`s back and over one of the shoulders.
TNOD	No
TNOX	Development of nitrous gases?
TNPO	an area excluding sea areas A1 and A2 within the radiotelephone coverage of at least one Inmarsat geostationary satellite in which continuous alerting is available
TOCE	The main supply line to be blanked off prior to the work.
TOHK	They are not normally used for pumping oil
TOIX	Blocked condenser.
TOPM	8
TORA	The master shall notify next of kin/  Norwegian Consulate - arrange for burial/ repatriation of coffin/ashes - and maritime inquiry
TOTU	centre, alternately towards each end
TOVL	Checking that lifejackets are correctly donned.
TPCA	Start air supply
TPDU	Zero-point is accurate, but 100% input is not giving 100% output
TPDV	Able to effect a complete change of air of the space being ventilated 16 times an hour?   
TPEO	1 to 2%
TPGI	Increase the jacket cooling water temperature to avoid the sulfur dew point
TPHC	a first-aid outfit in a waterproof case
TPLC	200 meters
TPLE	One for each person on board who is not provided with an immersion suit
TPNT	The Norwegian Consulate
TPXQ	Incomplete combustion owing to wrong mixture of air and oil.
TQCW	2 men 
TQLY	Make it possible to drain to shore the remaining cargo in the ship's lines and pumps, after the discharging is completed
TQTJ	Heat level rises
TQWY	Wear protective goggles, gloves, coverall, footwear and mask.
TRAE	The seaman signs in section b) of the appropriate ALC form (ALC1a, ALC 1b or ALC 1c as appropriate), the Master signs below in section c) of the crew agreement. Completes the relevant information in the seaman's discharge book, signs in the appropriate co
TRAF	Notify the Master, Deck officer on duty and the Engineer on duty, the loop for this special sensor to be switched off and take normal precautions for hot work
TRFB	60 minutes
TRQA	Weight of the ship including fixed and permanent equipment, less cargo, complement, passengers, stores and supplies
TSEM	Close all air ventilators and other openings to the hold in question
TSJG	The pressure drop across the filter.
TSKA	Because the ship is leaving after sunset the following day
TSKB	received messages, which aren't intended for own ship are not passed on
TSLU	To enhance safety in general
TSLV	24 hours
TSMU	All of the alternatives together.
TTBT	Excessive heating caused by over tightening of the gland packing.
TTGT	He has disengaged the windlass and put the brake on
TTGW	Stop the purifier immediately. Check the bowl for heavy side, deposits, bearings, housing, and the spindle for damage.
TTHL	0,75 candelas (about 0,6 mile range at normal meteorological sight), 8 hours
TTQU	Keep the floors and decks free from fat and grease.
TUBR	Broken water seal, oil outside the top disc.
TUBT	Ensuring that all persons avoid smoking in bed.
TUEB	Forecastle is given by B on the figure
TUFA	All the mentioned alternatives
TUKT	It is a gas containing insufficient oxygen to support combustion of hydrocarbons
TUNG	QI is an authorised individual, situated in the US, and contracted by the owner  or operator of the vessel
TUSK	When the machinery spaces are in the manned condition.
TVHI	to have the correct position in case of accidents
TVSI	the time of day in relation to propagation
TVTB	Stop all F.O. transfers immediately, and inform the CE.
TVTC	the day/night situation
TVWK	He wants all the lashings tightened and two extra chains fastened to each container
TVWN	120° C
TVXB	All these actions are required
TVYV	Helps keep accommodation floors clean longer.
TWIY	8 minutes
TWND	In case of an overfilling.
TWOB	30 litters per nautical mile
TWPS	Propeller disengaged and ahead or astern propulsion
TWRH	In main vertical zones
TWRI	Keep a low pressure in the tanks at all times at sea and in port (periods of gas-freeing excepted)
TWSG	six hand flares
TWSY	a license must be issued
TWTQ	9 mtrs
TWVL	to enhance safety
TXIB	Level in the tank to be reduced as much as possible to reduce/stop any further oil spill.
TXJY	All cargo tanks, pump rooms and cofferdams shall be examined by two type approved explosimeters.
TXKL	If the face mask has a leak toxic fumes/smoke would still not enter the mask
TXLI	Disposed of in an ashtray and ensuring that it is extinguished.
TXMD	 1200 litres
TXNC	geostationary
TXTT	2187,5 khz
TXUR	The main difference is that deep well pumps are connected to the motor with a long shaft and submerged pumps have both pump and motor submerged down in the tank
TYDR	That they are kept under constant surveillance.
TYEQ	1m/s
TYFI	Raise the boom.
TYHB	CT2, WT2 port, WT2 starboard.
TYHW	Risk for pollution
TYIT	Check that the painter is made fast to a secure point and that the sea below is clear
TYIV	Tug towing line is given by D on the figure
TYPE	Toxic substances
TYQG	The oxygen content shall be measured to 21% by volume
TYRF	Propane, Butane, Isobutane, Ammonia and some chemical gases as VCM, Propylene and Butadiene can be condensed against water
TYXA	Wet pipe system
UABH	Machinery and boilers out of operation due to lack of electric power
UACB	Salt
UADA	Dairy products
UAGL	Sierra, Alfa, Tango, Charlie, Oscar, Mike
UAHF	Use a proper torch
UAIF	It depends on wear and tear, but approximately every 12 - 18 month.
UANC	Blocked condenser.
UAXF	Any of the listed alternatives.
UAXV	Transmitter and receiver to be tested with intervals of not more than one month
UBHE	The hazards of exposure and the need for warm clothing
UBKP	Rotary positive displacement (mono type).
UBQJ	All of the listed alternatives.
UBSU	Too little gas in the system.
UBVG	To assist in the efficient and safe watchkeeping.
UBYW	The Master
UCDU	Multipurpose powder
UCWT	Crude oil and refined products.
UDAD	All prescribed life-saving appliances shall be made of non-combustible or fire retardant material
UDFB	Bandpass filter                                                                 
UDHS	She will most likely sheer to starboard and gradually lose headway
UDJL	Do not reply to any questions from outside parties, except the Solicitor appointed by your company.
UDKE	On Scene Commander
UDLC	0,5 l if the de-salting apparatus is capable of producing this quantity in 2 days
UDMX	handholds or a buoyant lifeline becketed around the outside, except in the vicinity of the rudder and propeller
UDOI	 two buoyant smoke signals
UDQB	operation of davits used for launching liferafts
UDSO	vessels of a certain shipping-company
UDSU	CO2                                                                                  
UDWT	Saturated hydrocarbons are colourless and odourless liquids and they are chemically non-reactive
UDYO	Same number as beds in the cabin
UEAJ	Stop the purifier immediately. Check the bowl for heavy side,   deposits, bearings, housing, and the spindle for damage.
UEMR	lifebuoy with light and smoke
UERN	Alkanes has only single bond between the atoms
UETJ	The Operator should immediately set continuous watch on the radiotelephone frequency that is associated with frequency band on which the distress alert was received.
UFAB	Make two round turns fast on the leading bitt and then figure of eight on both bitts, fig. 4
UFBC	One hose for each 30 meter length of ship plus one spare. Hoses for engine and boiler room in addition
UFCO	Make sure that the compartment has been evacuated
UFGR	lower liferaft to water
UFJI	Entries regarding the seafarer's service time, vacation days due etc.
UFUC	A thick rope to tie up the ship
UFVT	After the separator shell has warmed up.
UGCS	16 and 28
UGEC	The master or owner if the master prevent or fail to do so.
UGEE	In Act 3 June 1977 relating to hours of work on board ship, section 1
UGPX	Measure the specific gravity of the electrolyte
UGQS	Regularly, when preparing for sea and entering port
UGSI	At least two sets
UGTA	Let go starboard anchor 1 - 1,5 shackles
UGTD
12 miles
UGVT	Landing here is highly dangerous
UHDH	To keep constant surveillance of machinery and auxiliary systems.
UHIG	Secured via a weak link to a secure part of the ship
UHJX	Improve the scaling surface function, increase the service time of the exhaust valve in the engine
UHKQ	500 cm
UHKS	S = (A or B) and C
UHLS	Minimize corrosion, prevent deposits and scaling, and control of biologic. growth
UHPV	Aft breast line is defined as B on the figure
UHPX	The exhaust gas receiver.
UHQT	Vessel should be underway, minimum 7 knots, discharge max 30 litres per nm and be 50 nm from shore. The discharge should take place above the waterline and total oil discharged should not be more than 1/30000 of total cargo.
UHRI	be constructed of inherently buoyant material
UIGQ	the condition and results of tests of the main radiotelegraph installation
UIHJ	There is two types of membrane tank systems, Membrane system and semi-membrane system
UIME	Reduce the service interval.
UIMG	Upper Flammable Level / Lower Flammable Level of  explosive atmosphere?                                                     
UIOY	the frequency used
UIRD	Fuel pump timing changed.
UISB	a traffic list with the call-sign of the ships involved in alphabetical numerical sequence
UISC	Trying to ignite burner from hot brickwork
UISD	Quebec, Uniform, India, Charlie, Kilo
UIVO	The water level
UJBJ	500 kHz
UJCJ	The smallest diameter piston is the stage two piston
UJDD	The bow will be pushed away from the bank
UJET	The water can be applied in a fine spray starting from the front in a sweeping motion.
UJGH	one rustproof graduated drinking vessel
UJGM	All life-buoys shall be placed in holders with quick-release arrangement
UJIW	A ship receiving this call must set watch on channel 16
UJMG	1 VHF RT + DSC+ DSC watch receiver - 1 or 2 SART - 1 NAVTEX or 1 EGC receiver- 2 or 3 VHF portable - 1 EPIRB
UJNW	A command as dirtlx…+ can be given
UKAP	To keep the lifeboat steady against the sea/wind
UKEV	a buoyant bailer
UKQF	by cooling, smothering, combustible suppression, inhibition
UKRC	Blocking inductive kick from the solenoid                      
UKWD	The Master has no obligations to assist in towing a vessel
UKWE	Raise the feed water temperature.
UKYM	No welding or hot work on board ships carrying cargo with flashpoint below 60° C must take place in the tank area before the cargo has been discharged and gas freeing carried out.
ULBE	Maximum volume percent oxygen must not exceed 5 percent
ULCC	Indirect cargo cooling plant is utilised on cargoes that can not be compressed or be expelled for high temperature
ULIO	Open, when pressure in the boiler is in excess of normal working pressure.
ULLE	channels 06, 08, 72, et 77
ULVF	All winches be left with the manual brake on and gear out
ULWC	No specific word will precede a routine message
ULXU	a boarding ladder that can be used at any entrance for persons in the water
UMHW	 Foam monitor gun
UMJJ	B
UMKH	Hysteresis
UMMV	not later than 1 month
UMNT	Figure 1
UMOO	Quadruple
UMVC	TX: 2189.5 kHzRX: 2177.0 kHz
UMWW	which officers are assigned to ensure that life-saving and fire-fighting appliances are maintained in good condition
UNAG	As shown in figure 1.
UNCQ	Identify the hazards, quantify the risks, put control measures in place, monitor the work activity and review
UNCR	Monthly
UNHM	a frequency
UNIK	You are seen - assistance will be given as soon as possible
UNIL	60°C
UNJE	8 minutes
UNKG	A material that neither burns nor emits flammable fumes in such a quantity as to experience ignition, when the temperature rises to 750 ?C
UNMM	Bunkering of bulk lubricating oil.
UNNK	70
UNQS	To individual employment agreements for service on NIS ships
UNQV	The appointed lifeboat commander.
UNWO	2.0 bar
UOHS	To prove that the vessel has had the official number and net tonnage marked into a main beam, and that the ship's name has been marked on both bows and on the stern and the port of choice marked on the stern.
UOJH	Starboard bow is given by A on the figure
UOUV	5 litres / m2/ min
UPAV	Start air supply
UPCJ	Very High Frequency
UPEB	Capstan is given by A on the figure
UPGP	8414.5 kHz and on at least one of the following DSC frequencies: 4207.5 kHz, 6312.0 kHz, 12577.0 kHz or 16804.5 kHz
UPLP	In the Fire and Safety instruction manual
UPOC	All passengers that will require some form for assistance in case of evacuation, etc. must be registered, so there can be sent crew to assist them if needed.
UPVQ	the detonating gas can be discharged
UPXL	secure all burners
UPYX	Too much lub oil in one or more cylinders.
UQAQ	the use of SART transponders
UQEW	Seagoing service
UQGM	The transmitting mode is not compatible with the chosen frequency
UQLK	You will get harmed by the fumes before you are able to smell it. 
UQMH	They may require him to make a safety inspection and report his findings
UQNE	8 hours a day?
UQNI	It adheres to the boiler tubes and reduce the heat transfer. It combines with solids to produce sticky deposits.
UQUR	Start an additional auxiliary engine
UQUT	The Norwegian Maritime Directorate
UQXF	SILENCING DISTRESS followed by the silencing station's call-sign
UQYV	Forecastle head, manifolds, maindeck?
URMH	A large temperature drop across the drier.
UROS	Heavy seas from behind
URQL	Every lifebuoy shall be constructed of inherently buoyant material or have sufficient air compartment for buoyancy
URQM	Exhaust gas leaking into the oil chamber
URSV	20.000 tons
URVO	adjust the noise threshold of the mariphone receiver
USQH	when floating in the inverted position it can be righted by one person
USQI	with weak incoming signals distortion is reduced
UTOQ	A certificate issued by the authorities of a state which has acceded to the STCW-Convention
UUAG	85° C
UUAM	All the mentioned alternatives.
UUBH	Change in output signal divided by change in input signal
UUCY	L(S) =  18 H                                                                     
UUHU	November, Alfa, Victor, Tango, Echo, X-ray
UUOJ	It will be discolored and turn pink.
UUXR	Pressure
UUYM	Speed governor and voltage regulator
UVAC	Lower than -18?C
UVBV	differs for each country
UVBY	They must wear the protective equipment or clothing supplied when they are carrying out a task for which it is provided and follow appropriate instructs for use
UVCQ	the two lifebuoys of the quick-release system and at least two other ones, one on each side of the ship
UVJL	The passengers get familiar with emergency procedures, life jackets, musterstation. And the crew get training in growd handling.
UVWR	All bolts to be in position and tightened?
UWDG	Segregated ballast tanker.
UWLS	Copy of the fire control plans/folders to be stored in a watertight prominently marked container outside the deck house
UWLX	for ship-shore telephone-traffic on the MF/HF bands
UWQP	Overhaul the unit to determine faults such as: piston ring blow-by, exhaust valve malfunction, clogged scavenging ports, delayed ignition etc.
UWQU	Ulsan, Korea
UXCM	Push shore line content to shore tank or compare the ship`s/shore flow measurements.
UXDK	Sound three blasts in succession, namely one short, one prolonged and one short blast
UXEF	15 compressions followed by 2 full ventilations. 
UXOB	International Convention for the Safety of Lives at Sea
UXPU	Ventilate the tank and perform procedure for tank entry according to company manual, then fit the portable machines.
UXQJ	lifebuoy with light and smoke
UXTG	Yes, and as listed in the Maritime Act.
UXUE	One control book for special medicines, one approved by Norwegian authorities medical book ("International Medical Guide for ships") and three pamphlets regarding first aid.
UYCL	Place the injured part under slowly running cold water for at least 10 minutes, but preferably until the pain is gone. If no water is available, use any cold, harmless liquid.
UYGR	4.5 meters
UYHP	Approximately 85% dry.
UYNH	Certain sections of the Act 3 June 1977 relating to hours of work on board ship and section 7 of the Act 12 June 1987 relating to NIS
VABS	All passenger ships, all cargo ships of 500GRT or above
VAEE	The purpose of the priming unit on centrifugal pumps is to evacuate the suction line if air is present
VAEJ	closing of watertight doors, fire doors, valves, scuppers, side scuttles, skylights and portholes
VAFF	store & forward messages
VAKD	The position ensures that an open airway is maintained.
VATG	No
VATI	The person may be very pale, and pulse is slow at first and weak.
VAVS	0°C
VBHL	Overhaul the compressor unit.
VBNC	Lower the boom, raise the load.
VBNE	Report to relevant authorities.
VBOE	That the wires are just above the water line at all times
VBRJ	802 ohm at 20° C
VBSE	They are going to weigh the anchor
VBUV	 All these actions are required.
VCEY	A non-emulsifying agent with self splitting emulsifiers.
VCIB	Line-throwing appliance
VCJW	L2330
VCNH	According to the nomograms You select a gravity disc with larger hole diameter.
VCSD	30 m
VCTS	Passenger ships carrying more than 36 passengers
VCTT	Weekly
VCWK	6 knots for 24 hours
VDCJ	muster station
VDDD	The tug was made fast at the centre lead astern
VDEU	The wheels of hatchcover No. 7 came off their tracks
VDFX	they should prepare survival crafts and in general render assistance where need
VDHL	a rustproof dipper with lanyard
VDNH	The company responsible for the operation of the ship
VDPN
15 mtr
VDQK	J3E
VDVM	Where the fire breaks out, how many fire teams are available, the strength of the fire, the ships mobility, what is burning and communication
VEDU	By putting the vessel mooring ropes as an oil boom around vessel and oil slick
VEES	2200 ohm
VEGG	A combined scouring and polishing machine.
VEIR	ALC 1c
VEIW	a first-aid outfit
VEKN	lowering of at least one lifeboat after any necessary preparation for launching
VEMB	simplex
VEON	In case of an emergency situation, the car deck can be difficulty to find the way around, and cars can shift position caused by ships movement.
VEVE	Multistage centrifugal.
VEYS	Yes, it will give the stern a lift force to starboard
VFAI	2500  mm wg?
VFDY	RF-Gain
VFFK	That people are well trained
VFUM	A cascade controller.
VFYT	Stern is given by C on the figure
VGAF	be prevented from pressure exceeding twice the working pressure, either by relief valves or by limited gas supply
VGAH	highest point of the steam and water drum
VGBF	another channel is chosen
VGCO	Survival craft portable radio
VGMS	Lower the boom.
VGMU	0,04 %
VGON	Annually.
VGSS	Accounting Authority Identification Code
VGTP	To neutralize the acids occurring in the condensate system.
VGWV	8
VGYN	A document, which together with the national certificate is entitling the holder to serve in a position for which a certificate of competency is required
VHHU	Make a bold alteration to starboard and pass on his port side
VHKD	Inhibition and smothering 
VHLB	Ensure adequate circulation in all conditions of steaming.
VHNO	use a proper torch
VHXP	5 %
VHXQ	A fixed sprinkler system at the cargo manifold
VHYL	low-expansion foam
VIBR	In the fire control plans or booklet that must be stored in a watertight prominently marked container outside the deck house
VIDL	Boarding, launching and clearing of survival crafts (lifeboat/liferafts) and rescue boats
VIGB	Secure the wire all way aft, to prevent wire moving out of center
VIGS	For 3 minutes starting on the hour and half hour.
VIGU	About same position as the center of gravity
VIHN	For all vessels.
VIHV	The stripping capacity has to be 25% more than supplied liquid.
VIMQ	by muster lists exhibited in conspicuous places
VIRV	length = 480 mm, breadth = 115 mm, depth = 25 mm
VISK	He is to check the heater for the hydraulic oil
VIWM	When a particular work activity  may cause ill health, when an identified disease or adverse health condition is related to the work recognised testing methods are available  for early detection of an occupational disease
VJBP	Correct flow, pressure and temperature (viscosity).
VJDM	1,5 l
VJHL	8
VJJH	liferaft
VJLP	Muster and embarkation stations shall be readily accessible from accommodation and work areas
VJLS	Yes
VJYC	Reduce the RPM to reduce the scavenge air temperature. When the temperature is reduced and in case the fire is not extinguished by  itself, insert carefully CO2 
VKNG	6
VKRK	To observe traffic movement in the English Channel, give advice on traffic move-ments and alert vessels which are making improper use of traffic separ. scheme
VKSG	Air draught is given by C on the figure
VKUS	A remedy to which the mooring lines are made fast
VKXI	5% by volume.
VLBK	a mock search and rescue of passengers trapped in their staterooms
VLER	Construction of all internal divisional bulkheading of "B" or "C" class divisions, without the installation of an automatic sprinkler extinguishing system
VLOB	All of the mentioned
VLOY	By entering the alarm instruction with your cabin number
VLPT	By double blank flanges with a drain between them?
VLPX	climb up and down a vertical ladder of at least 5m in length
VLTY	That people are well trained.
VMGH	Where the mooring lines lead.
VMJP	 Sprinkler horn
VMKT	Blue
VMLM	Either of the mentioned elements
VMRC	All SOLAS, MARPOL and Loadline convention Certificates
VMSE	independent of the destination
VMYA	To gas free a cargo tank means that we remove flammable-, neutral- or toxic atmosphere from the cargo tank
VMYX	The three most common energy forms are mechanical energy, chemical energy and electrical energy
VNAJ	60 %
VNDU	A bearing is damaged.
VNEP	Stop
VNFF	To evacuate air and water out of the system in order to prevent problem during operation.
VNFK	The piston clearance is too large. Worn piston or cylinder liners.
VNIW	the use of MF and/or VHF R/T
VNJR	To prevent serious damages on the plates.
VNJT	As in example 2
VNMW	immersion suit
VNNX	distress
VNOO	Immersion suit
VNRE	24 houres
VNWE	All of the mentioned equipment.
VOFH	is equipped with a pocket for a portable VHF
VOMW	the length of the ship
VORQ	They are not normally used for pumping oil
VPHR	A deck officer or certificated person shall be placed in charge of each survival craft to be used
VPHS	Power-driven vessel making way on port bow
VPLV	  Every UK ship except fishing vessels and pleasure vessels
VPMV	Search for missing persons. Continue to monitor situation and prepare for abandonment in case it become necessary.
VPRU	You inform the NCS that the SES is available for comunications.
VPSJ	Wait three minutes and if no acknowledgement is heard from a coast station you should relay the alert.
VPSL	Stainless steel?
VPTN	Cold drinks and salt.
VPUB	On Scene Commander
VPUH	Start water-spray
VPVW	all entrances fitted with rigid boarding ramps for boarding the liferaft at sea
VPWQ	Master, Chief Engineer & Chief Officer.
VPWS	unit which automatically releases the liferaft/lifeboat at a depth of approx 4 metre
VPXS	A cut of veal topside.
VQGV	Use water extinguisher to put out the fire.
VQHP	Cut it with the safety knife stowed on the exterior of the canopy close to the painter attachment point
VQKC	The ITU List of Ship Stations
VQLA	1min
VQNJ	Dose with coagulent and blow down the boiler.
VQQB	must be replaced before the expiry date is exceeded
VQRP	Put the rudder hard to port to reduce the water flow to the right side of the propeller
VQTJ	9 GHz
VQVT	MAYDAY
VRFB	Seeing that the passengers are suitable clad.
VRFY	According to the nomograms You select a gravity disc with    larger hole diameter.
VRGS	Aft of the forecastle secured with the use of a hydrostatic release device
VRGW	Whenever the gangway is rigged.
VRJS	Fire extinguishers equipped for powder or CO2 only.
VRKW	The turbine rotor is not balanced
VRKX	A decrease in strength of 20 %
VROD	J3E
VSGQ	Water contamination.
VSGR	Exhaust valve
VSJW	To wash all lines and pumps properly.
VSMF	It reduces the visibility, provokes panic, is irritating and may be toxic
VSMN	safety
VSQN	International Maritime Satellite Organisation
VSWN	Channel 70 DSC.
VTAM	All fully bolted except those actually in use.
VTAU	Solution of potassium hydroxide (KOH) and water        
VTBP	Only during day time when visibility, traffic etc make it safe
VTCO	Generation of carbonic acid causes the water quality to drift towards sour and lower the pH - number.
VTIY	immersion suit
VTLR	All the mentioned alternatives
VTML	The use of all survival equipment
VTOD	Transfer it to the sloptank, and later discharge it to a reception facility
VUCY	VHF channel 16
VUET	fixed sign on the mast plus signs on each radar when work is in progress in mast
VUFP	One month
VUUN	Pressure-reducing regulator.           
VUUP	Pos. 8
VVCC	not less than half the total number of lifebuoys shall be provided with self-ignition lights.
VVDU	the tanks should be fitted with audible and visible high and high-high level alarms
VVKQ	Every month
VVOQ	By smothering and also providing some cooling 
VVPP	Maintain course and speed with caution as he is the give way vessel
VVQI	Make the pipes capable to move back and forth inside the coupling.
VVRA	Pressure surge and liquid pressure.
VWJK	The atmosphere in the tank where hot work is to be carried out, and adjacent tanks shall be checked immediately prior to commencement of hot work.
VWQC	Gas carriers and chemical carriers
VWWX	25 watt
VXCB	If the face mask has a leak toxic fumes/smoke would still not enter the mask.
VXFE	He is worried that oil will run through the outlets and into the sea
VXJJ	The secondary controller
VXPE	Yes, in regulations on medical examination of employees on ships.
VXQD	All the mentioned alternatives
VXXW	A dedicated set of pages in the Official Log Book for entering details of draughts, freeboards and allowances when departing from any port or place
VYBS	Sound the General Alarm - carry out emergency actions.
VYEN	four rocket parachute flares
VYFW	Beef
VYGV	Weekly
VYJD	An efficient and reliable service
VYLW	ship's radio log
VYXN	Dispersant
WACC	Inert gas is utilised on board gas carriers to neutralise atmosphere in cargo tanks, pipes and hold/ interbarrier spaces
WADB	11 times 0,17 SDR
WADV	All answers
WAIW	10 to 11%
WAIY
Cover the spillage with a layer of foam.
WAPG	Ear muffs
WARV	Before the tank is entered, lifeline, rescue harness and compressed air apparatus shall be ready at the relevant hatch
WAUD	The cargo tanks are to be washed that often so recidues do not accumulate in large quantities.
WAUH	Warm clothes, blankets and lifevests.
WAVF	Diamond shape
WAVJ	C(S) =  18 µF
WAYO	…..
WBBD	two buoyant smoke signals
WBCA	Just prior to reaching the water, the lanyard should be pulled. This sets the hook which will automatically release once the raft is waterborne
WBFJ	A noxious liquid with melting points less than 15°C, is at a temperature, at the time of unloading, of less than 5°C above its melting point, or in the case of substances with melting points equal to or greater than 15°C, is at a tempera-ture, at the time of unloading, of less than 10°C above its melting point.
WBLW	Survival craft portable radio
WBOG	Commence sounding the fog signal, engines on standby, call for lookout, call Master
WBST	permission for availability, installation and use of radio transmitters on board
WBXU	distress
WCFC	Strain gauge
WCFW	Hotter due to increased current
WCIK	He needed to get acquainted with the officers.
WCKY	5% extra
WCRQ	Simplifies the overview
WDBR	Blue 
WDCV	an omni-directional aerial
WDED	Low oxygen alarm
WDEY	1
WDFD	Lifebuoy with light and smoke
WDLY	Central gas extinguishing system and/or waterfog
WDRO	Two valves segregation.
WEGK	duplex
WEGM	because the volume adjustment of the speaker is too high
WELN	The governor
WEOA	Inner diameter of impeller is bigger due to cavitations, or outer diameter reduced by erosion.
WESJ	I am manoeuvring with difficulty - Keep clear of me
WEXL	Centrifugal force
WFAW	watertight lockers or compartments
WFTX	In the meat locker
WFTY	Do a 20/20 degrees zig-zag manoeuvre
WFUR	All independent tanks are self-supported
WFYY	All the mentioned alternatives
WGJB	Check for presence of hydrocarbon gas using a CGI and oxygen  using an oxygen analyzer and if you obtained readings of 0% LEL and 21% oxygen respectively, you would enter?
WGLO	Secure hatches
WGNA	Engine Room
WGOY	Difficult to seal plates above this pressure.
WGRF	Weekly
WGRL	Interface towards center.
WGUM	evacuation slide
WGVS	5 years
WHIT	it lessens the survivor's heat escape
WHLC	All ships.
WHNY	activating the SART and checking the effect on the radarscreen
WHPM	SOLAS A PACK or SOLAS B PACK according to the type of emergency pack enclosed
WHRB	prevent excessive furnace heat losses
WHRL	5 miles
WHWE	The appointed lifeboat commander.
WIAM	A reduction in strength of 10 % to 15 %
WIAN	A signal will sound in the crew accommodation spaces after 2 minutes
WIBF	A vessel without ordinary bottom lines where the cargo flows from tank to tank through bulkhead valves.
WIEO	9 GHz.
WIFG	in the event of capsizing it will automatically attain a position providing an above water escape
WIFK	On area A1 this function is based on the use of VHF NBDP telex
WIJM	Chapter 30
WIJO	reduced heat capacity of the heater
WIKE	Radiotelephony - Phase modulation
WIKN	location of embarkation ladder
WIME	is not fine-tuned
WIOO	Notify nearest Norwegian Consulate
WIQA	Broken water seal, oil outside the top disc.
WIUM	+ 1.0 bar
WIYL	Operational amplifier                                                       
WIYR	Allow for increase in water volume
WJBE	To determine if there is any danger of grounding or colliding with objects during drifting
WJCW	The pump's delivery valve (discharging valve).
WJFH	the captain/ master
WJIU	All the mentioned alternatives.
WJMV	Cavitation.
WJOP	If packing fails the pump can be kept running by tightening the glands, but if a mechanical seal fails it must be renewed to stop the leakage
WJPF	Increase.
WJUF	Seawater
WJYK	Only in conjunction with paper charts
WKCR	3 sets. New-builds from February 1992, other vessels from February 1995
WKJJ	Plate
WKKA	According to the nomograms you select a gravity disc with larger hole diameter
WKSS	Adjustable wrench
WLEH	Familiarization, and other drills identified as necessary by the ship
WLIK	Person in charge
WLQU	Plaice
WLVA	To everyone engaged in work on board, except those who only work on board while the ship is in port
WLVX	The route to musterstation, how to put on lifejacket and different emergency signals used onboard the ship.
WMED	Figure 3.
WMEF	The maximum possible percentage of oil being burned effectively in the cylinder volume available.
WMIK	NOR gate
WMMO	date when last serviced
WMOG	AF-Gain
WNDB	Before being employed
WNGV	R(S)=  4  ohm
WNJV	the use of VHF DSC
WNLO	The crew members embraced by the Act 3 June 1977 relating to hours of work on board ship
WNLU	5 miles
WNLW	call sign
WOCH	Wire for pulling burning ships off the pier
WOIF	raise the water level a couple of inches above normal
WOTT	I am dragging my anchor
WOWG	A license, given by or on behalf of the Minister of Traffic department
WOXB	The master and department heads.
WOXE	To detect oil mist (explosive atmosphere in the crankcase).
WOXY	Raise the boom, hold the load.
WOYY	Start engine
WPER	No, there could be a conflict of interest
WPIT	Yes
WPOW	Formula 1
WPOY	6
WPQH	1.0m?
WPSE	The tug may be turned across your bow with the danger of being turned over
WPUO	Mandatory.
WPWE	To avoid high wear down of chain and chain wheel tooth and a potential breakdown.
WQEP	With given density at observed temperature we find a corresponding density at 15 degrees Centigrade.
WQFO	Seven short blasts followed by one prolonged blast
WQKG	Position A
WQRV	On all areas this function is based on the use of SARSAT COSPAS Epirb
WQXT	ARQ-system
WQYO	Charge air temperature is too high.
WRBX	High delivery pressure
WRIS	During navigation between ports
WRKF	be capable of operation from fire stations aboard the ship
WRQF	Under the forecastle.
WRTO	Once every month
WRUH	the first digit of the identification
WRYM	It is easier to damage a centrifugal pump than a piston pump if they run dry.
WRYO	95 Celsius
WSBC	2°C after a period of 6 h immersion in calm water at a temperature of 0°C ... 2°C
WSDQ	That the strainer needs cleaning.
WSEL	the space where the batteries are stored is properly ventilated
WSGV	Means of escape - escape routes
WSLD	That the collective wage agreement states (1) that it applies to such service and (2) that the agreement is subject to Norwegian laws and Norwegian courts of law unless courts of another country is explicitly mentioned
WSMA	SECURITE (3x)
WTJH	The use of radio life-saving appliances
WTUD	Electrodes
WTVT	+ 1.0 bar
WTWR	Approved training
WTWV	Monthly
WUAA	In the main Section numbered VII
WUFC	Lowers oxygen content in the tank
WUFW	Fasten seat belts
WUIH	A publication which contain all information regarding the product in question and should be posted in public areas so all crewmembers have access to the necessary information.
WUIM	Gas dangerous areas onboard gas carriers are cargo compartments and cargo piping, hold spaces and other spaces where cargo pipes are located, compressor and pump room, open deck over cargo area
WUIO	Oil Detection Monitoring Equipment.
WURM	The same as suction pressure.
WURR	That the pump is stopped in time to avoid overflowing.
WUUC	To take part in public traffic
WUVR	a buoyant lifeline bucketed around the outside of the liferaft
WUWJ	The Medium Frequency (MF) band.
WUWN	MF-transmitters
WVDH	They have to bunker fuel oil and diesel oil
WVFS	Less than 5 min
WVHL	500 ?C
WVKS	5 sec
WVLL	Emergency diesel and batteries
WVLQ	The wind and sea should be from ahead or nearly ahead
WVMK	To reduce danger of fire and the risks of sliding.
WVMM	Differential amplifier                                                       
WVNC	2,2 kN ± 0,4 kN
WVQO	Damage to piston and liner.
WWGO	Weekly
WWKT	Makes the meat take on a reddish colour after preparation.                                                             
WWLL	Forecastle is given by B on the figure
WWME	He will find a lubricating chart in the maintenance manual
WWND	Organic peroxides.
WWNH	Radiotelephony - Phase modulation
WWOX
MCA only
WWTX	All safety surveys except Passenger Certificate will be carried out at the same time every 5 years
WWYS	Uncovered manila rope.
WXCD	emit smoke of a highly visible colour
WXDB	volt x hours
WXEU	They turn yellow
WXFP	PAN PAN (3x)
WXFR	2 min
WXJR	The clearance between the rocker arm and valve pushrod.
WYCJ	six hand flares
WYFH	Yes, as per the General Civil Penal Code Chapter 42
WYSA	Public announcement system to be used for informing. The cabin attendant should proceed to their cabin section, and search all cabins. If the area is inaccessible report to their superior.
WYUO	Normally use it, as free or dissolved chlorine is not aggressive towards stainless steel?
WYWC	To prove there is no liquid in the cylinders.
WYXA	Diesel oil.
WYXW	Vegetable / Fish Oil
WYYU	the safety certificate (S.C.)
XAAT	All ships carrying flammable cargoes must have deck water spray to flush cargo spill overboard and cool cargo area if fire
XAAV	Highest point of the steam and water drum
XABR	The interface moves outwards
XAKS	Not recommended at all
XALN	H = - 0.178
XAML	Low differential pressures
XAMN	The alternators are not generating the same voltages and should be adjusted on automatic voltage regulator rheostats
XAPL	The secondary controller in a cascade control system
XAPT	Centre line is given by A on the figure
XAQK	Grease was blocking the grease pipe
XAQS	R(S) = 25 ohm
XATX	To reduce the general risk of fire in an unmanned engine  room.
XAVI	2m
XBEW	2
XBFO	2
XBIB	Putting in auto order when on stand-by, to be effected every 10 - 15 minutes
XBQI	+ 5 ° C
XBQJ	Register of Shipping and Seamen
XBSC	a working channel of the nearest shore-station of that coast-station
XBSD	lifebuoy with light and smoke
XBSE	This concerns a mobile station
XBTP	1 VHF RT + DSC+ DSC watch receiver - 1 or 2 SART - 1 NAVTEX or 1 EGC receiver - 2 or 3 VHF portable - 1 EPIRB - 1 MF RT + DSC+ DSC watch receiver
XBTW	All alternatives
XCAI	If the hot work is to be carried out at the bottom of the tank, the entire bottom shall be thoroughly cleaned and all sediments removed.
XCFI	F1B/J2B
XCFJ	Reduce the rate of flow, and topping up one by one tank
XCHD	a license
XCNV	Radiotelephony - Frequency modulation
XDAR	DSC has fully taken over watch-keeping on 2187,5 kHz
XDGC	All mentioned.
XDGE	Development of toxic gases?
XDIN	Life buoy with line
XDIW	To disconnect the power source
XDPI	8 %
XDYT	Frequency in an Alternating Current (AC)
XEAC	Discharge the slop tank completely first then refill it from a cargo tank from which a layer of 1metre has already been discharged. 
XECW	davit launched liferaft
XEEG	this message is stored in the memory under TX4
XEFB	In ICS Tanker safety guide
XESU	The control  valve for the cooling water cooler is sticking.
XETN	Starting achieved within 2 min of commencing the start procedure at an ambient temperature of -15°C
XEUD	Treat and reassure the casualty and stay with the person at all times.
XFHP	When he is properly relieved.
XFIN	CBTs cargo tanks are also used for ballast, SBTs are not.
XFMY	every month
XFOH	9
XFOI	no entry with naked light and/or flame
XFQV	35 kg
XFRU	The floor of the raft has a second layer which can be inflated to help insulation, in addition to the thermal protective aids (10% of complement, minimum 2)
XFUD	Mooring buoy is given by B on the figure
XFYK	Every four months
XGHL	MERSAR
XGHQ	Overhaul the compressor unit.
XGIJ	Scharnow Turn 
XHCJ	Reduce the sea water flow through the condenser.
XHDE	Rocket line
XHEB	From the system pipeline.
XHGT	a AAIC
XHJF	Lower than 23°C 
XHJG	Mooring buoy is given by B on the figure
XHJI	Bridge is given by A on the figure
XIAY	In the Captain's office
XIEB	This call will normally be followed by an acknowlegment call on DSC
XIHN	Use large quantities of water as soon as possible
XIPW	The ship's management team must organise the fire teams and then the teams have to rescue missing personnel
XIVI	Generator overload due to many motors starting at simultaneously
XIWI	The rags may be caught by a revolving shaft.
XIWJ	Capacitor                                                                          
XIYA	Figure 2.
XJCC	listen on the radio-telephone distress frequency in the pertinent band
XJEW	this message is the 6th message in the memory
XJGJ	We are not allowed to load ammonia on inert gas
XJIB	The percentage of the L.E.L. in the ambient air
XJQK	Open and closed circuit apparatus
XJVL	IMDG
XJVM	Outside the ship itself
XJVO	The recognized classification society, were the vessel is classified.
XJXU	two hatchets
XJYW	Request lower loading rate?
XKNB	Warm clothes, blankets and lifevests.
XKOO	Resistance temperature sensor                                         
XKPN	Clogged air inlet filter
XKQI	A part of the Norwegian Maritime Directorate, on NIS ships mainly doing unscheduled inspections
XKXS	Life buoy with line.
XKYT	ASCII
XLBJ	Making use of Risk Assessment as a means to improving safety
XLDW	F1B
XLIT	About 20%
XLOO	Insufficient air supply
XLSX	To persons in certificated positions as per the manning certificate and certificated positions of additional manning, if any
XLYN	yes, provided that he has a Certificate of Equivalent Competency issued by MCA
XMCY	Gauge pressure
XMFE	Radar transponder
XMHR	Correct water level is obtained by refilling the cooling system, and the entire system is checked for leakages
XMIP	Nothing for the first 24 hours, then 1/2 litre or more, if possible, per day
XMKJ	Products with users instructions telling you how and where to use them.
XMKL	9 GHz
XMPH	use of communication equipment
XMPL	The International Maritime Organization (IMO)
XNAH	Only licensed officers
XNBA	Height of liquid in the tank
XNFD	Level control
XNGY	Flag state
XNIP	you must wait 3 minutes minimum before repeating your call
XNMW	Not less than 10000 kJ
XNPG	combustible, oxygen, heat and chain reaction
XNRP	Be constructed of inherently buoyant material.
XNWV	To avoid cold cargo to came in contact with the ship's hull
XNYM	Resistance sensors
XOBX	seeing that passengers are suitably clad and have done their lifejackets correctly
XOCQ	tlx..+
XOFD	personal call
XOJI	a solid (cardboard or wood…)
XOKD	13.0 mm?       
XOTD	the seasons
XOVR	Liferafts shall be stowed with its painter permanently attached to the ship
XOWT	the use of VHF R/T
XOYF	He has disengaged the windlass and put the brake on
XPDF	10 bar.
XPLR	lowering all lifeboats
XPNC	One year.
XPNH	Rescuing of life
XPNI	Take separation of the two vessels into immediate consideration,  but consider that a separation may create a larger oil spill
XPOJ	On Scene Commander
XPPV	All of the mentioned must be performed
XPPY	Natural bends at intervals?
XPRJ	compensate the movements of the vessel
XPUU	one set of fishing tackle
XPXH	Checking that life-jackets are correctly donned.
XPYA	at least 24 distributed on both sides of the ship
XQCL	CO2 plant.
XQJH	Leave the engine room as quickly as possible, closing all doors behind you
XQJW	The patient placed in a "face -to-the-floor" position, and with arms and legs arranged in  order to stabilize this position.        
XQKQ	Sudden crushing, vice-like pain in the centre of the chest.
XQKW	Call an hospital for professional medical assistance by radio when needed.
XQMM	The heart.
XQNF	Fixed CO2 fire-extinguisher system
XQNI	handholds on the underside of the hull
XQQM	one whistle or equivalent
XRAV	A series of tests run by the computer at power on
XRBP	Its readiness to perform as specified.
XRGG	f o =   1 / (2 sqrt (L/C) )
XRGN	Oil Record Book.
XRKU	the use of VHF DSC
XROP	Operate the engine room on manual mode until the cooling pump is in operation, switched in stand-by mode.
XRRF	the DSC-watch receiver
XRRH	J2B / F1B
XRVK	Prevent contamination if leaks are developed
XSBN	They are economical to operate
XSCY	The release mechanism shall be of an automatic type approved by the Administr
XSES	It is possible to predict the control mathematicallyIt is possible to predict the control mathematically
XSGK	inversely proportional to the frequency
XSIX	sky wave
XSOW	Constant flow, clean probes and temperature below 60 Degr.C.
XSPO	When the provisions and /or water is unfit for consumption
XSPR	The ITU List of Coast Stations
XSRF	Authorised radio surveyors employed by Marconi
XSVL
Notify the US Coast Guard
XTEQ	an area excluding sea area A1 within the radiotelephone coverage of at least one MF coast station in which continuous DSC alerting is available
XTGI	No
XTHE	The acidity (ph) of the cargo should  be between 5 and 7 when diluted with 10 parts of water to one part of cargo.
XTLK	Difficult to seal plates above this pressure.
XTMX	Start water-spray
XTTR	4 m
XTUM	All mentioned.
XTVH	To keep constant surveillance of machinery and auxiliary systems.
XUFH	Only cargoes included in one of the categories, A, B, C or D.
XUOI	that need not meet any of the requirements relative to smoke and flame nor limitations relative to temperature rise
XUON	Intermittent signals on the ship's alarm bells
XUOR	If it is decided that work shall be carried out, the decision and the reason for it shall be entered in the ship's log book.
XUWB	be taken by the crew to the rescue-boat and turned on manually
XUXV	on the date of replacing the battery
XUYL	All the other mentioned alternatives according to the situation
XVAJ	A system that's displaying the way to the nearest exit from all locations onboard, by using flurosent signs at floor level, or light system powered by battery.
XVBW	All of these cargoes are incompatible.
XVIM	Stand behind the casualty. Clench your fist with the tumb inwards in the center of upper abdomen. Grasp your fist with your other hand and pull quickly inwards.
XVJN	When Under Keel Clearance is 50% or less
XVMA	It will be much shorter
XVMY	only be given receipt, if the master has confirmed that assistance indeed can be given
XVPE	telephone country codes
XVTJ	The hours of work Act and the NIS Act.
XVXP	We find 5 annexes in MARPOL 73/78 and annex 1 is the regulations for the prevention of pollution by oil
XWEN	Coordinated Crab
XWMR	Visual and radar observations
XWNM	Daily cleaning in cabins, messrooms, galley, etc.
XWSI	Over time we got more experience with products and systems that give us reason to change rules and regulations
XWWU	Inhibitor is used to prevent polymerisation of the cargo
XXBP	Notify Ch.Eng., find cause of leakage, remedy the leakage and then immediately start cleaning of the tank top.
XXBT	alkaline.
XXCN	Go to your lifeboat station
XXCO	On the navigation bridge
XXYE	Electrically isolated by special isolating switchboxes in the accommodation and the keys of these retained by a responsible officer?
XYFU	davit launched liferaft
XYFY	The Norwegian Maritime Directorate
XYGW	Manoeuvring levers/wheels for mechanially operated ports shall be properly secured when not in use.
XYPU	8 %
XYPY	Remote level controller with indicator
XYQS	In 440 V section: Two lamps bright.  In 220 V section: Two lamps bright.
XYXF	name of the ship in distress
YADO	The entry is left as it is. An additional entry is made referring back to the erroneous entry and noting what the correct entry should read
YAHQ	Merchant Shipping Notices (MSNs), Marine Guidance Notes (MGNs) and Marine Information Notes (MINs)
YAJD	Under keel clearance is given by C on the figure
YAKE	The ship's officer in charge of the oil transfer
YAPA	The slave controller with the master controller in manual mode
YAPE	two sponges
YARM	will conduct electricity with very high voltage 
YATK	all vessels in the Ocean Region concerned can read it
YAVX	Turn the rudder towards midship, but normally not all the way to midship position
YAWR	He should be aware of the steel thickness of the valve
YBEA	increase
YBGW	Centrifugal pump.
YBHU	ICE-method.
YBJC	They are to let go of the stern lines
YBRQ	300   -   3000 kHz
YBTF	Maximum allowable working pressure
YCAS	Both in a conspicuous place in each machinery space and in a conspicuous place at the bilge and ballast pump control station
YCDB	The tug may be sucked into your stern with danger of striking the propeller
YCDF	96 hours
YCEY	At any time, provided he is confident that the engine room will operate in a safe and efficient manner for the period it will be left unattended.
YCIJ	Neutral to Alkaline solution.
YCKT	Radiotelephony - Phase modulation
YCLM	If at sea, the master shall immediately undertake an investigation, secure evi-dence and take statements, inform Norwegian Consulate/Maritime Directorate
YCLR	pressed in constantly to work duplex
YCRJ	the oxidising agent in the presence of which fuel may burn. The oxygen is a comburent par excellence
YCRN	It would be determined by risk assessment, but at very least would comprise safety line and harness, lifebuoy standing by, safety hat, boiler suit safety boots
YDAV	Chapter II-2
YDTC	95° C
YDUN	Tell the person to sit down and lean forward with the head between the knees taking deep breaths.
YDVL	During crossing, ports on the car deck shall be closed and battened.
YDWL	Not allow the clothes to be hung anywhere in the unmanned machinery spaces
YEDY	To comply with MARPOL requirements
YEIA	Class C fire 
YESY	Change the lube oil.
YEYS	Piracy is increasing
YFBB	A liquid change to gas.
YFBK	Development of toxic gases?
YFKM	From the condenser.
YFKP	4
YFPM	Printed Circuit Board
YFQI	Telephone
YFXS	Neutral.
YFYM	Soot would be swept toward the uptakes
YGGF	Water can be removed in the separator but not in the filter
YGJV	swim through the water at least 25m and board a survival craft
YGMX	Has to contain a work-frequency
YGNT	lifejacket
YGVH	Yes.
YHAK	Total pressure head
YHDN	Green
YHFJ	can be unpacked and donned without assistance within 2min.
YHJP	2 min
YHQE	That the separation may cause sparks that can possibly ignite the oil or any other flammable substances.
YIEH	300.000 kilometres per second
YIHT	the frequency actually used by transmitter and receiver
YIIO	In stairways and corridors
YIKG	Yes, you must attend to a course held by certified personnel, and then be certified by national authorities (NMD, USCG, etc)
YIPI	Ensure the valves are of the correct discharge capacity for the boiler.
YISM	25 %
YITG	Give the coating time to "weather out" the trapped solvents using good ventilation, and recover it's hardness again, prior loading the next cargo?
YIVB	In % of full scale
YIXM	received messages, which aren't intended for own ship are not passed on
YJCM	amplitude is variable and frequency of carrier wave is constant
YJGQ	O2: 21%  N2: 78%  H2O: traces  CO2: traces  Rare gases: traces
YJIM	The heat given to or given up from a substance is called latent heat
YJMJ	Yes, must be cooled to 25 Degr. C.
YJNK	Every day.
YJOA	The Stevedore company?
YJRK	To prevent the circulating oil in the crankcase from being contaminat with fuel oil
YJTI	the number of persons the liferaft is permitted to carry
YJUB	Fasten seat belts
YKDF	Water with less than 15 ppm vitiation of oil
YKIE	Large fenders meant for floating between vessels and absorbing considerable impact. Example of fender size: L - 4.5 m. Dia. - 3.3 m
YKKV	Not less than 10000 kJ
YKKX	All of the other alternatives.
YKMK	A wheel with which the ship is steered.
YKNC	Use the intercom to inform crew and passengers of the reason for the alarm
YKQR	In G3E mode - on simplex basis
YKVP	to suppress noise
YLDC	 Portable foam applicator
YLEB	Fouled cooling water system.
YLFV	In a clarifier solids are removed from oil, whereas in a purifier solids and water are removed from oil
YLII	Put the plates in  water with qualified cleaning chemicals, and use soft brush, or high pressure cleaner with care.
YLKO	A ship which carries more than 12 passengers
YLLJ	10 to 11%
YLLL	Forward breast line is given by C on the figure
YLNB	only the master
YLNC	Release falls
YLPV	A Norwegian Consulate has already duties on behalf of the NMD and the directo-rate can in addition instruct a Consulate to act on the directorate's authority
YLQT	LAPQ4
YLRD	an indication of aerial problems
YMBN	Uncertainty - Alert - Distress
YMCC	Spherical cargo tanks are used on all types of gas carrier, fully refrigerated, semi-refrigerated and fully pressurised gas carriers
YMFJ	Bow/stem is given by B on the figure
YMKS	Feed-check valve
YMYA	Seelonce mayday
YNBN	You set watch on channel 16
YNDB	time (in UTC) whereupon the telex for the subscriber is delivered.
YNDY	call-signs of ships for which a radio-telephone call, a telegram or another call is intended
YNEO	5 knots
YNET	All alternatives
YNKQ	Fully-refrigerated gas carrier can be discharged by condensate the cargo to shore or another cargo tank or let it boil off
YNKS	8 hours a day?
YNPN	Open steam valve very slowly, considering system expansion.
YNRG	 Emergency fire pump
YNRH	every 4 months
YNUN	Message concerning an important navigational message.
YNUO	To prevent oil spills in US waters?
YNVI	Fuel tanks should be topped off with no room for expansion.
YNXB	That no solid beam of fuel shall be present
YNYU	Warm clothes, blankets and lifevests.
YOAM	a telephone conversation with a person whose name is known, department or extension on the telephone number given
YONW	 Sprinkler section valve
YOOK	Increase in condenser pressure.
YOPO	One short blast, one prolonged blast, one short blast
YORY	5 sec
YOSR	Circle the vessel.
YOUP	is marked that it must be worn in conjunction with warm clothing if it is made of material which has no inherent insulation
YOWU	An observed situation where objective evidence indicates the non-fulfilment of a specified requirement
YOYO
automatically send a non-delivery notification (NDN) to the sender
YPAH	A whistle and a light
YPCU	At a place easily accessible from the shore
YPCX	All the mentioned alternatives?
YPPE	the use of MF and/or VHF R/T
YPSO	automatic self-righting abilities when every persons are held in their place
YQFW	Line currents: 0 A, 180 A, 180 A. Trip condition: trip on overload.
YQGU	Ships can use their own boats if they cannot safely lift hired boats, but boat crews must be hired from shore
YQGV	Silicon controlled rectifier (SCR)                                    
YQHS	Midwinter
YQIL	To prevent too much shrinkage.
YQIM	General cargo holds
YQOD	neither for …
YQPA	30 months before the expiry date- +/-`6 months
YQPX	The flash point for an oil or liquefied gas is the temperature at which it is possible to ignite the vapour above the liquid
YQTK	Put on the life jacket
YRFW	Aft of the manifold.
YRFX	Vegetables
YRRM	Blue 
YRRO	Enclosed Space Entry Permit and Cold Work Permit.
YSGL	the name of each inoccupants (passengers included, if any)
YSJC	J3E
YSSE	Yes, the quick closing devices shall be tested and maintained frequently to ensure proper function in case of fire in the  engine room.
YSTY	 5 - 10 Degr. C.
YSUB	Any of the below.
YSUD	Water leaking into the combustion chamber.
YSUS	EPIRB
YSVQ	1.5 litre
YSYB	If a sudden drop in pressure appears after the valve is supposed to be closed, this is caused by a leak
YSYG	This call is an all station call
YTKY	At least one member of the crew shall hold a repairman certificate for life-saving equipment
YTQK	three tin-openers
YTQQ	Mixing of : Incompatible cargoes, Annex 1 and Annex II cargoes and veg oils with chemical slop.
YTSF	The GPS system gives information about position, speed and time continuously world wide.
YTTD	Length overall is given by B on the figure
YTYS	The welder shall have been instructed in the use of the ship's welding plant.
YUKR	30.5°C  ET?
YUNF	Close the valves, oxygen first. 
YUNY	3,5 - 3,9%
YUOW	Roller fairlead is given by B on the figure
YUTT	an area excluding sea areas A1 and A2 within the radiotelephone coverage of at least one Inmarsat geostationary satellite in which continuous alerting is availabl
YUVL	the use of VHF DSC
YUVN	To be briefed about what to expect and when ships and lights should be detecte
YUYX	One year.
YVFL	The lower speed the higher ratio of oil/oily water can be discharged?
YVGK	The point where the sideways motion of the ship`s centreline is zero
YVGL	Returned to the Ship Control via a Norwegian Consulate
YVJT	2 PSI above / 0,5 PSI below?
YVJW	A converter that converts an analogue signal to a digital signal and vice versa
YVNV	one drain valve fitted near the lowest point in the hull, except for free-fall lifeboats
YVQI	Maritime investigators, The ship Control,, the Electrical Inspectorate, and other public institutions, Det Norske Veritas and other approved survey institutions, other private institutions of foreign countries, the authorities of foreign countries
YVTS	Measure oxygen contents in the atmosphere.
YVXD	Check that the painter is made fast to a secure point and that the sea below is clear
YWBF	The Seaworthiness Act
YWEO	Dilute the remains by 10 times with water, then overboard if the vessel is more than 12 miles off land and proceeding at a speed of 7 knots or more.  The discharge need not take place below the waterline.
YWEP	At least one portable foam applicator unit
YWFH	Electrostatic hazards?
YWIY	A Shipboard Oil Pollution Emergency Plan
YWMB	pressed in during transmitting only to work simplex
YWNV	the way radio waves are propagated
YXCS	to swim a short distance through the water and board a survival craft
YXDO	the use of VHF R/T
YXEN	30 miles
YXVD	The manoeuvring vessel presents her port side to the constant direction vessel
YXWV	At least two jets of water not emanating from the same hydrant, one of which from a single length of hose, may reach any part of the ship normally accessible to passengers and crew
YXWW	He is steering the ship.
YXYL	At about 1/6 of the ship's length from the bow
YYBW	By using rubber gloves.
YYFY	Rescuing of life, fighting the fire, limitation of the fire and secure the retreat
YYMW	Absolute pressure
YYNQ	0° 
YYNS	The asphalt unlike sulfur is a viscous product and does not transmit its heat easily to the steel bulkheads, allowing the steel to stay cooler than the cargo
YYPD	One on each side of the ship
YYRO	To prevent serious damages to the plates.
YYRT	if they are more than 25% of the total crew
YYSM	Sea water
YYSQ	He is to notify the Chief Officer
YYXR	Anchor ball.
zxsd	 All the mentioned alternatives


#################################
CES 5.0 | Deck | Management
#################################

AHWA - Tpassage plan is always required, irrespective of the length of the \ voyage, or if the ship is under pilot	
APRH - All vessels and on all voyages
AQCC - The first rescue unit to arrive at the scene will normally assume the role of OSC, until the unit appointed as OSC by the SAR Mission Coordinator at the applicable RCC is in a position to take control.
BDRI - The position of the tug relative to the ship's pivot p^int^^
BEXX - Organise someone to assess the extent of damage and the residual J stability of the vessel.	__
BFDT - Inform the local coast radio station of the incident and submit your \ _^name as a witness._____
BUGF - Use the Arpa for early identification of all other ship movements within the traffic lane and give rogue vessel a wide berth
BXKL - I Organization and Management II Mission Co-ordination III Mobile Facilities.
CBBT - About 80 %
CDSB - 1.1 times the total mass of the lifeboat when loaded with its full complement of persons and equipment.
CHRU - The speed should be less than 5 knots, normally 3-5 knots
CLVE - 5 years.
CUCF - The approach speed is too fast. "I
CXSS- Pushing on the ship's side and made fast in case the vessel's movement towards the berth requires reducing by the tug pulling off.
ENHB - The ships moving together in the swell/seaway will cause a spark an consequently an explosion.	_______
FJBB - Between 1/4 of the ship's length from the stern and the rudder post
FXYP - The International Aeronautical and Maritime Search and Rescue (IAMSAR) Manual.
GOYB - Make sure your vessel + crew are safe and then offer your assistance to the other vessel
GYAW - Use the Bow Thrusters to change the ships head and monitor any changes in the drift
HBJX - Alarm the rescue centre and commence searching for any survivors
HFLG - Much greater power on the forward tug than on the after tug while monitoring the gyro heading
HKEH - Approx 5,000 square metres.
HVGC - Williamson Turn
IAKL - J.30 tonnes
IERT - All of the suggested answers
IFLU - Two tongue-type/hinged bowstoppers with separate closed fairlea Capacity 200 tons
IKLV - Considerably more power on the aft tug than the forward tug, while monitoring the ship's gyro heading__
IWES - The tug made fast on a line through the centre lead astern, (figure 4).
JDUG - About 20 %
JHYC - Deciding safe speed consider: 2 miles visibility; traffic density; manoeuvrability of vessel; effectiveness of navigational equipment (ARPA etc); state of sea and currents and navigational hazards.
JMUI - The force will be Quadrupled
JVMT - SITREP
JYJE - Rudder hard to port, full astern. After gaining some sternway, rudder hard to starboard and full ahead
KEKK- The heading should be carefully monitored, some port rudder may be required to start the swing, though starboard rudder may be required to balance anvbank rejection.
KFMF - Risk is a situation involving exposure to danger and includes both identification of the occurrence and the likelihood that it will happen.
KQEI - Name; Port of registry; Port of destination of your vessel.
KRBW - An effective detailed passage plan fully understood and followed by a competent bridge team.
KVUM - Increase the safety of all ships and the protection of the environm* in the vicinity.
KVVK - All of these answers
LGWL - Wire from a deep sea tug connected to the ship's anchor chain?^
LRWC - The anticipated weather and the need for weather routing. The distances gained by sailing by great circle. The ship's draught and the leadline limits
LUHR - The Hague-Visby Rules.
LWKS - After checking the extent of the damage and welfare of your crew, possible your vessel should standby and offer assistance, until beii relieved of that obligation by the other vessel.	
MKTY - When both vessels are underway, fig. 1
MLRU - There is an increase in the water velocity and a decrease of water pressure around the ship's hull
NIBB - A responsible Officer
NTAR - Select WGS84 and when plotting on the chart apply the stated j .corrections.	_
OBLY - Only if approved by the Flag State
OHFV - Determine when the seaman was last sighted and concentrate the search round the course line between the last sighting and presen position, taking into account any prevailing current.
OSKG - The large volume of water dragged behind the vessel continues to move forward and cause a strong turning moment on the stern oft vessel
OWQM - Gyro compass bearings from two lighthouses
PBKT - Put the ship aground on a soft sandy bottom as soon as possible
PCCF - No, the diameter of the turning circle would be almost the same.
PHEK - Expanding Square Search..
PJUX - Increase the officers on the bridge to allow greater use of visual navigation
QGDC - The Classification Society.
RBCW - A passage plan should be discussed between the Master and pilot, when under pilotage in the same way as discussed with the bridge team when deep sea
RCAM - With the Loadline Certificate.
RGKG - The Automated Mutual-Assistance Vessel Rescue (AMVER) System.^
RKIR - About 10 %
RLDL - No, when the ship's speed exceeds about 5 knots it will be expect* that there will be a reduced pull exerted by the tug
ROHD - On VHFCh 16.
ROQU - Annually.
JYJE - Rudder hard to port, full astern. After gaining some sternway, rudder hard to starboard and full ahead
SHWX - 3.6 nautical miles.
SPGA - 11 shackles
TCUD - 5 years.
TIFL - 100A1ESP.
UGTA - Let go starboard anchor to about 1 shackle on deck
UTRU - Inform the appropriate search and rescue authorities of his decision and enter the reason in the ship's logbook.
VCLF - me master or a snip at sea wnicn is in a position to De aoie to provide assistance on receiving information from any source that persons are in distress at sea, is bound to proceed with all speed to their assistance, if possible informing them or the search and rescue
VGON - Annually.
VPMV - Complete soundings of all compartments to determine the number compartments flooded. Check the vessels stability limitations withir statutory loadline requirements to determine if still adequate.
WGKM - Less than 3 hours.
WYXD - The Cargo Ship Safety Construction Certificate.
XJVM - At a position outside the hull of the ship itself
XPNI - Take separation of the two vessels into immediate consideration, t consider that a separation may cause a fire and also create a large spill
XQCA - The Certificate of Compliance with SOLAS V/19-1, bearing the serial number of the equipment installation.
XYBO - The squat effect will be reduced to a quarter of its original value



#################################
Áåç êîäà
#################################
Âîïðîñ: -A coastal passage or voyage plan should indicate the appropriate methods of determining positions and include which of the following?
Ïðàâèëüíûé îòâåò: All of this suggested answers.

Âîïðîñ: -What is understood by the term "Balansed rudder"?
Ïðàâèëüíûé îòâåò: A rudder with part of the rudder area forward of the turning axis, therefore reducing the load on the steering motor.



#################################
Áåç îòâåòà
#################################
CXJR - Why does a ship move laterally (sideward drift) when turning.
SELECT ANSWER:
-The ship moves laterally because it always tries to continue in a straight line.
-Because the pivot point is not at the centre of the ship
-The ship moves sidewards because of all the external forces on the vessels hull.
-Because the turning moment is created by the rudder, which is positioned at the stern of the vessel
-I don't know

LOIB - Where is the normal position of the "Pivot Point" of the vessel when going ahead?
SELECT ANSWER:
-Amidships
-1/4 of vessel's length from the stern
-1/3 of the vessel's length from the bow.
-Normally varies dependant on the speed ahead
-I don't know

#################################
//ÊÎÍÅÖ CES 5.0 | Deck | Management
#################################





#################################
CES 5.0 | Engine | operational
#################################

FSYD	To prevent biological grown in the system
OBJN	The load connected to the switchboard
QQBE	He shall have all the knowledge as listed in the other alternatives
DNOC	The main supply valves in the deck storage are closed and checks made that no fire risk
exists prior to switching on the fire alarm system and going to UMS-mode.
SYPY	Continue with manual operated engine room until the maintenance work is finished.
UABH		"Dead Ship" means that the machinery and boilers are inoperational due to lack of
electrical power
PKPS	To ensure cylinder lubricating oil enters the cylinders when the piston is in the required
position.
WCIK	The new Cadet wanted to go to the messroom to become acquainted with the officers
ETYX	Initially rise, then reset to the set value.
FKSJ	Prevent manual synchronising outside permitted limits
TYDR	Postpone the inspection until the correct oxygen content can be achieved
DRKO	Water contamination of the oil.
UHPX	A constant pressure system has a larger volume exhaust gas receiver
YJMJ	Yes, the samples should be cooled to approximately 25 C.
QPKF	Cold drinks and salt.
TPXQ	Incomplete combustion of the fuel.
JNOB	10 M ohm
AAET	Transistor
HLFN	Inverting amplifier
VMKT	Blue
JUES	To check for weardown of the main bearings
JGGR	Permission must be obtained from Chief Officer?
HJLS	Re-pack the stuffing box loosely with the correct size packing at the earliest opportunity.
OHCB	Gently heat the bearing in an oil bath and use a bearing puller to draw it onto the shaft..
ITRV	Secure the ladder top and bottom and have a shipmate standing by while you are working on the ladder.
FRKL	A leak of exhaust gas from a boiler or diesel engine exhaust.
JFFG	25 miles
OBNV	Wrong installation will result in a major deviation in measurement
JYNF	The control system is depending on the best possible process signal
CPEQ	The difference between possible maximum and minimum measurement
TIJL	The pressure falls off on the pressure gauge when trying to hold the pressure in the
injector below normal opening set pressure.
SLKR	Low-pressure cut-out is stuck in closed position.
CEBM	System undercharged with refrigerant
FQEL	The interface will move outwards allowing oil to discharge from the water outlet.
LCFH	65 -85 C.
YKDF	Water with less than 15 ppm vitiation of oil
BFGY	The Chief Officer wants the First Engineer to empty the starboard bilge in No. 5 hold
SJUT	Lifeboat
MMCW	5 compressions after every 1 inflation
RRYQ	Yes
OIEQ	No
QSXP	It stops the spreading of smoke and flames during one hour
IFJW	The uppermost deck to which transverse bulkheads are carried
XUON	Intermittent signals on the ship's alarm bells
JTQE	up to 150 persons
QKMN	Start engine
YSUS	EPIRB
VQLA	1 Min
WLEH	Familiarization, and other drills identified as necessary by the ship
YVTS	Measure oxygen contents in the atmosphere.
KDBI	Do not touch any suspicious packages
SWFO	Wear skin protection and a facemask.
BXAA	To detect and give an alarm and slowdown of any potentially explosive atmosphere in the crankcase.
EVKX	Water carry over from charge air cooler to engine cylinders.
UVMW	The prime mover speed and excitation current.
SUOY	Disconnect, isolate, earth (ground)
SSXM	Problems with a gas (SF6) circuit breaker
QWVK	Frequency in Cycles per second
UJDX	8000 - 12000 hours.
LWLR	To ensure the strength of the oil film is sufficient to keep lubricated surfaces apart.
BUMG	It should automatically operate before the normal start sequence following an engine
stopped period of more than 20 to 30 minutes when manoeuvring.
AAQB	Adjacent pipework should be slackened off to allow the pipe to be aligned. Any incorrectly positioned brackets should be adjusted after the pipe is refitted.
GXQS	The pipe should be returned to the shoreside workshop for modification or to be remade to the correct dimensions.
XBEC	A fixed pitch propeller can operate with reasonable efficiency at the same sort of speed
as the engine.
YGBV	VIT increases engine efficiency by automatically maintaining the maximum cylinder
pressure over part of the load range.
SNWM	Remove the excess length using the ship's lathe
TFHH	Remove the puller and try and warm up the bearing and cool down the shaft a little before trying the puller again.
SEDE	The angle the ship will lie when the ship has a negative GM
FJMV	All of the suggested answers
TMVR	Temperature variations across the cylinder cover result in uneven thermal loads on the
studs.
FNBO	Turn the engine so that the piston skirt is at the bottom of the liner. Use wedges to
centralise the piston. Measure the clearances along the length of each bar and shoe and fit shims to equalise the clearances
MLJI	Check the hydraulic release pressure for the holding down bolts.
YMJJ	Reduce the width of the proportional band for the controller.
JYTJ	Near the bottom of the liner.
JGXH	With the governor in operation open the compensation needle valve to introduce
instability and disturb the engine load to make the governor hunt.
TMPQ	By measuring a standard gauge block or rod at a common temperature.
MHRU	Check the resistance change in the sensor over a known temperature range against the
resistance values in the product sheet.
CRKY	Pass fresh air through the sample chamber.
UXSI	1000Volts ac or 1500Volts dc.
IXFW	Hypothermia is the condition when the core temperature of the body is lower than normal
CDJB	The ship chandler
PLDX	To check that the correct concentration of corrosion inhibitors are maintained.
QAJN	To prevent corrosion of the metals used in the system
NWDX	The frequency of the incoming alternator is the same as that of the main switchboard
LFXF	3 phase excitation winding/rectifier bank/main field winding
XAKS	Only on the fuel injection valve test rig.
TYHW	Risk for pollution
NIHX	It can cause fouling of the charge air cooler with wet sludge lodging between the fins.
DBXA	Piston rod and stuffing box.
FUVP	A thorough check inside the engine to make sure all tools and cleaning rags have been
removed.
NWHD	Bimetallic strips need time to cool down
OEVU	Follow all ISM procedures relating to hot work including permit to work and hotwork
permit requirements.
YJRK	To prevent any fuel leakage from the high pressure fuel pumps contaminating the oil in
the main lubrication system.
EATY	Pump the system down to the condenser, continue cooling water flow until the condenser is at the same temperature as the cooling water and vent off the air from the top of the condenser.
HKLJ	+ 85 ° C
BLGF	To indicate and relieve excessive high pressure in the cylinder to protect the engine from being damaged.
XMCY	Gauge pressure
KYGT	Figure 2.
LJBE	A zener barrier is a unit made to obtain intrinsic safety in installations for instrumentation in hazardous areas.
BTPM	A compressor in which the compressed air from the first stage is further compressed in
the second stage before being delivered to the air receiver.
RIPO	In conjunction with the senior watchkeeper and electrician, isolate valves, electrical
supply, automatics and post 'Do not operate' signs before commencing work.
FRKL	A leak of exhaust gas from a boiler or diesel engine exhaust.
UBQJ	Securely rope off the area around open hatches and post notices at the site.
UNMM	Bunkering of bulk lubricating oil.
XTVH	The primary duty of a watch-keeping engineer is to maintain constant surveillance of the main engine and auxiliary machinery
CKFA	Comparing input and output values against a documented standard
WTUD	Electrodes
QHQI	The pump will eventually overheat.
AKAH	Collapsing vapour bubbles due to cavitation.
TUSK	Once the engine is properly prepared and tested and the engine room is correctly
manned
NSNF	Lifejacket
JMMT	Raise the fire alarm.
BVQC	10 minutes
CVOV	A manually operated release system only
GMUY	Yes
FGEQ	All the alternatives are correct
QQEL	Survival craft portable radio
PSXB	Rocket parachute flares
CEME	Ship owner has Document of Compliance issued, and vessel is assessed and holds all
statutory certificates
DPOW	At all times when identified as a control method with risk assessment
NIBX	Hypothermia
OWWM	"Stand quietly in various spots around the space, listening for unusual sounds like the tick tock of a clock mechanism."
IELO	Pallet scanner
AMDV	To improve valve sealing by compensating for pressure and temperature effects on the
valve during engine operation..
LWOA	Bipolar transistor
HFKD	6.6kV
AVPP	Shims should be fitted between the motor and compressor feet and the skid to ensure
correct vertical, horizontal and parallel alignment of the coupling halves before it is bolted up.
WLXS	The running surfaces oscillate relative to each other during operation rather than rotate and therefore full film hydrodynamic lubrication is not possible
VFTT	Aluminium brass.
YADQ	Short sharp period of roll associated with breaking lashings and shifting cargo
GWCT	Panting beams and stringers
EXKB	The fillet radii
MLHS	A tapered guide sleeve should be fitted over the threaded end of the piston rod.
DYHF	The governor droop should be reduced.
MWXV	Back pressure control valve.
LXML	Check the gauge on a deadweight tester
BKQS	Immerse the thermometer in a mixture of distilled water and ice made from distilled water to check the zero reading.
TGRL	Pressure variations in the sample chamber can cause errors so restrictions must be kept
to a minimum.
DMAY	The Second Officer would tell the master the visibility had reduced to probable range of 2 miles and the engines were on standby.
EXUJ	If he finds something missing from a lifeboat, the Third Officer should notify the Chief
Officer
LIPD	At least two
AWNQ	Fabricate a conical guide from tin plate or similar with the large diameter just bigger than the compressor piston so the rings can be eased open for fitting.
PDWB	Low voltage.
BRYX	After at least 20 minutes
JAKS	Zero
NXEM	All combustible materials
LBWB	Stopping the engine to check the bearing temperature after a short period of operation
and repeating this procedure at increasing running intervals.
QSYH	Engage the turning gear and put a notice at each engine control position.
XXBT	It is strongly alkaline.
LUAE	He studied the contract in detail before signing it because he wanted to know his duties
ANQS	Steering gear and engine room alarm system
DGRN	A short circuit occurs between earth faults and the ventilation fan fuse blows
OJRA	10 Mohm
UMOO	Quadruple
XRBP	Its readiness to perform as specified
QBHO	The chemicals make it difficult to remove the oil from the water
FEWH	25 nautical miles off the coast
IGGI	Overboard discharge valve should close automatically.
QOTU	Stop the OWS and pump the oil to the incinerator tank.
DDNQ	Clean the heat exchanger.
BSVJ	L(S) = 4 H
GLKF	Strain gauge
DIKR	A transducer that converts a known electric current to a pressure proportional to the
current.
HHWS	3 sets
BLBF	Forced convection.
OUTI	Increase the dosage of boiler water treatment
HGGY	Open and ventilate the tank, test oxygen content, have someone standing by with rescue equipment, complete a permit to work and a tank entry permit and then commence work.
CYHA	The gravity disc is too small and/or the flow rate is too high
ILDJ	Prior to every plant start-up following a shut down of 8 hours or more.
RDFC	With the engine running, change over to the other filter after priming it and replace the
dirty element after checking there is no pressure on dirty filter housing.
AGGL	All mentioned.
NBQX	The longitudinal Bending Moment at any section within the ship is the total moments
tending to alter the longitudinal shape of the ship
JHKS	Line-throwing appliance
JHND	Complete 15 compressions at the rate of 80 compressions per minute
NWFJ	The infrared radiation and ultraviolet radiation given off by flames
IVWK	60 bar
WIKN	location of embarkation ladder
SWRC	Right if the immersion depth is smaller than 100 mm
YOWU	An observed situation where objective evidence indicates the non-fulfilment of a specified requirement
ODTM	2 - 3 %
IYEL	3 cm
FGBH	Rapid recovery shall be possible with the boat's full complement of persons and
equipment.
EEHC	Go to your lifeboat station (muster station).
KGMX	Protect your ship from risks posed by security threats or incidents
IFXF	Recognize its components.
JIOE	By mixing with water from the low temperature circuit.
BOVF	Use a suitable chain block suspended from the crane hook to 'break' the motor free after slackening all of the retaining bolts.
EYFC	It avoids the risk of the ends of the piston rings being forced out by the gas pressure and
catching on the scavenge ports.
DRHE	Ring spanner or socket.
LJHM	If the gaps are too small they could close due to the radial wear of the rings before the
next scheduled overhaul preventing the rings from contacting the piston rod and sealing
it.
RDJB	PID controller for tuning
PYLL	Gradually shut in the condenser cooling water valve or the condenser refrigerant inlet
valve while closely monitoring the compressor discharge pressure.
MRSN	The tie rods should be fully tensioned before the jacking bolts are loaded to avoid
overload of the bearing caps and frame structure.
JJEU	The throttle valve on the hydraulic system should be closed in.
DKWO	It will increase the offset across the demand range.
IKGN	..be fitted with a siphon loop between it and the steam pipe.
UCEW	The coalescer module is saturated and requires renewal.
AFVO	The HV cable carries a smaller current and therefore requires less copper.
JUHV	Pyrotechnics are the items which are capable of self-contained chemical reactions for the production heat, light, smoke and/or sound
DSML	"My ship is under attack by pirates"
WTTL	To provide means of escape for the passenger and crew
PFXR	Use a deadweight tester to mark a new scale on the gauge throughout the working range.
NSAY	Gear pump
BNKJ	Cooling water velocity too high.
MHMP	Prevent seawater contaminaton of the central cooling system in the event of seal failure
KOIR	To prevent the alternator from "motoring" by being supplied power from other parallel
alternator and thus being damaged
ETBH	Varying the excitation field strength by regulating excitation voltage/current
MNGY	(Y)
NXCD	Prior to arrival and departure from port and following maintenance
AIXA	A 2 stroke engine completes a full cycle every revolution
PUSR	Throw a lifebuoy over board and report to the bridge immediately
YQFW	Line currents: 0 A, 180 A, 180 A. Trip condition: trip on overload.
NJXQ	Short circuit protection.
POVX	Due to temperature expansion
YUNF	Close the regulator valves immediately, oxygen first.
ASUJ	To control the flow rate of liquid refrigerant to the evaporator
UJCJ	The smallest diameter piston is the second stage piston.
BRKO	Water contamination of the oil.
YYRO	To prevent serious damages to the plates.
HYVW	G = 1 / R
VUUN	Pressure-reducing regulator
XNYM	Resistance sensors
ISRV	Figure 2.
VATI	The person may be very pale, and pulse is slow at first and weak
BRUR	Never carry lighters or matches on the tank deck.
MOGR	When they have been properly relieved of their watch-keeping duties.
SBXF	Rotation of the plunger by the fuel rack from the governor signal.
DSVC	Ensure all doors are in closed position
GMUY	Yes
GTGB	30 minutes
DERP	It is both a prevention and protection measure
EICL	Make sure that the compartment has been evacuated
APLT	Collect rain water
AMYI	Red
HQGU	Continuously after having been immersed for a period of 10 seconds under 100 mm of
water when underwater
WLEN	Familiarization, and other drills identified as necessary by the ship
NRCW	Everyone
RCCV	The Chief Engineer
AOJD	17 - 20° C
KECH	Cold work permit + Permit for entry .
PEIT	Gun
IHKR	The individual wears bulky or out of season clothing
VMSD	Arcing at badly connected bus bars
XEXE	Smaller conductors, machines and switchgear
OEUS	Hydraulic tightening avoids the risk of unwanted bending stresses when compared to
other methods.
HCFX	Drawing a tangent to the curve through the origin and erecting a perpendicular through
the angle of heel of 57.3 degrees
JLHM	If the gaps are too small they could close due to the radial wear of the rings before the
next scheduled overhaul preventing the rings from contacting the piston rod and sealing
it.
HKXB	To protect the piston in the hydraulic system from possible impact damage as it may
reach the end of its stroke.
FXNN	Natural rubber sheet of approximately the same thickness and elasticity as the original
diaphragm material.
VVMY	To isolate a single frequency of vibration associated with one of the pumps components.
KLTB	Draught is indicated by D, in the figure
UNUM	The correct form of response would be: Visibility in my position is two hundred meters
GITV	To ensure that the correct levels of chemical treatment are maintained at all times
AGYC	Specific heat or specific heat capacity.
RCTK	Prevent damage to sensitive electronic components from high voltage tester
REOI	The engine load has increased due to external factors such as current and wind.
IYQF	1000 A
SVUP	Voltmeter and synchroscope
GTTS	Contain any oil-spill onboard the ship
VNFF	To remove any air and water from the system in order to prevent problems during
operation
EKUQ	Leave the engine room immediately.
HQEF	Figure 1
CQXU	Caps and cocks should be closed at all times, except when sounding tanks, to prevent
ingress of water or oil into the engine room in case of tank bottom damage or overflow
RIUL	Either Oil fitting equipment , or Oily-water separating equipment , or combination of both
DYIY	To inform the Chief Engineer of any situations that cannot be controlled during the watch
OOAU	Power dissipation capability
HKNF	Check linearity
PBVP	Faulty fuel injection valve.
FCNJ	Act according to instruction given in the fire plan.
DLNN	The same as the suction pressure
NGFM	Watertight doors can be closed adjacent to the door and remotely from bridge and also
one emergency remote control station
ANXC	The Chief Engineer
CKSH	15 compressions followed by 2 full ventilations
KTXA	Place the heel of one hand, two finger breadths above the bottom of breastbone. Cover
the hand with the heel of the other hand.
EBRI	Cargo holds and engine rooms
DFYJ	until - 15°C
RLMB	100% of the ship's complement on each side
NCUS	seven or more short blasts followed by one long blast
OIPL	21 %
OWAU	Cotton
VVBI	Security Level 3
MDRU	All alternatives
NVNP	Replace the complete cylinder cover with a spare unit and land the cover with the
jammed valve ashore for repair in a specialist workshop
MFYG	Only the fuel and starting air timing needs to be changed to reverse the engine
RQJY	Measure the flange diameter, PCD and bore using a ruler and callipers and then mark out the jointing. Use jointing scissors and hole punches to cut the new joint.
WJTA	Delay the work until a new spring compressor is available or fabricate a suitable
replacement onboard if the work is urgent
UBKW	Bulkhead constructed of steel, suitably stiffened and insulated so as to be able to meet a prescribed fire test of one hour duration
SPEH	Completely lose its share of the load causing the auxiliary engine to speed up
SELD	Inform the Chief Engineer and the Bridge. Change over to manual mode, switch over
generators and repair the fault before returning to UMS mode
QERG	Switch over to the other pump and inform the CE of the noise immediately. Keep engine
room manned.
KHTO	Accommodation
LCRT	The rotor blades are damaged or the blades are not properly cleaned
ESCK	no fault - hard earth - light earth
YYNQ	0°
FCHS	Circuit breaker operating time
GBIW	Stop loading
SAHN	Separation of two insoluble liquids with different densities, and the removal of solids in the same process.
WVMK	To reduce risk of fire and the risk of slipping.
IHTT	Closed loop feed back system
POSK	Bulkheads constructed of approved non-combustible materials but do not meet any of the requirements relative to smoke and flame nor limitations relative to temperature rise.
HLJS	Higher measuring accuracy.
KILD	As shown in figure 1.
PGHS	Dispersement of chemicals?
QPJL	The pump impeller and wear rings have worn
PCHH	Transducer
NMKT	16 mA
GDDY	Pressure diaphragm
XQMM	The heart.
QBEL	37 m2
KEKN	Fasten seat belts
WGLO	Secure hatches
STYA	When it is fitted with a guard or similar device which prevents foreseeable contact
between a person, his clothing or items held in his hands, whilst it is in operation
WJIU	All the mentioned alternatives.
AGRJ	Get out of the engine room as soon as possible.
PNSN	The seal rings are brittle and can be easily chipped or damaged
NRAA	Change the indicator spring for one with a higher rating.
FWBY	This means: Emergency Position Indicating Radio Beacon
BAIG	All ships of 500 tons gross and upwards
XIVI	Generator overload due to many motors starting at simultaneously
DECL	The diesel speed and excitation current.
DADR	Fuel oil leakage into the lub oil system
SKKP	It will cause the oil to oxidise, increasing the viscosity.
WHIK	NOR gate
ENHX	The pressure switch has contact(s) that will change between open and closed
position.The pressure transmitter converts a pressure signal into an electric signal.
XEUD	Treat and reassure the casualty and stay with the person at all times.
OFPV	Can not produce enough energy to ignite a gas (explode)?
LDIQ	Thick paper (chart paper).
PODI	Every report or message must be logged including time and date
VBHL	Overhaul the compressor unit.
HWQG	Stand on dry insulating material and pull the person away with isulating material.
YDAV	Chapter II-2
BAIF	One set of fishing tackle
KDOW	Release gripes
EGNN	All of the below mentioned
VABS	All passenger ships, all cargo ships of 500GRT or above
UNCQ	Identify the hazards, quantify the risks, put control measures in place, monitor the work
activity and review
JALP	40 - 60 %
YJCA	0.15 metres
LCVH	Contain and suppress fire and explosion in the compartment of origin
KFCD	1500-3000 ppm Nitrite.
WJUF	With seawater
DVUW	Three hours
GHGM	To provide combustion air at start up, during manouevring and low load running when the turbocharger delivery is insufficient.
ACBX	To avoid pollution.
LFAT	Governor droop settings on each prime mover
KXLB	Human error
JDRX	The master
QVEY	The alkalinity of the oil.
CPDR	Coat the deck with non slip paint and use duck boards provided with drainage
PRHG	Pressure
EWKF	The process will oscillate and get out of control
VEES	2200 ohm
ANSM	Rectifier
MIOE	Poor fuel oil quality.
KFQH	In a clarifier only solids are removed from the oil, whereas in a purifier both solids and
water are removed from the oil
HLXE	The First Engineer would require an inspection of the heating coils
GUNS	Air, Breathing, Circulation.
VKNG	6
MIWH	Legs bent, back straight, using leg muscles to lift
DMDI	A 60
ABEN	not less than 300m
TWIY	8 minutes
DIUH	Pressure variations at the turbocharger inlet are damped out due to the large volume of
the exhaust receiver and the short lengths of pipe from individual cylinders.
IBGM	Tighten it to the manufacturer's recommendations using a torque wrench.
FEVA	Under Keel Clearance is indicated by C, in the figure
JNPC	ICE-method.
KVRG	Between 7 and 10.
RHYX	By audible and visual signals at the control panel
CVXD	It satisfies the SOLAS (and other) requirements for ship safety
CEHB	AVR and speed governor
PMCY	No.2 generator trips on reverse power
KTIK	When the machinery operates over a wide temperature range.
QWBM	Lube oil cooler.
XHEB	From the lubricating system pipeline on the discharge side of the circulating pump.
NRLY	15 PPM
CEIB	95 - 98 Celsius.
TTGW	Stop the purifier immediately. Check the machine for fouling or mechanical damage. Do
not restart until cause is identified and fault rectified.
EPXN	Soak the plates in a recommended cleaning solution and then use a soft brush or
pressure cleaner.
CUCJ	R(S) =18 ohm
WPOW	Formula 1
OEUA	It is more easy to give correct pressure to the fractured/injured area, and the control of
swelling and bleeding is more easy to observe.
JBGH	Monitor the operation of the machinery on a frequent basis.
QFBP	The ship’s safety plan.
JYLR	On the ship fire plan
YYPD	One on each side of the ship
EKWG	Line throwing appliance
ILMM	the "Abandon ship" signal is not specified, only the general emergency alarm signal is
stated
QWIA	Particulate detector
FHGB	Relatively non linear characteristic
MFYQ	Only the fuel and starting air timing needs to be changed to reverse the engine.
NWYL	Reduce the number of slack tanks
TGVK	Stable equilibrium means the buoyancy force upwards and the force of weight
downwards are equal and G and B are in the same vertical line
JNTH	Muster List
IPVS	"Vessel "name" has lost a person overboard in "position….."
TAIP	5 years
KFTT	By raising or lowering the pump plunger relative to the pump barrel
JBEN	It should be brought to the attention of the Chief Engineer so that remedial action can be decided upon.
IJOI	In permanently exhibited fire control plans
AOHG	Once a week.
YDUN	Tell the person to sit down and lean forward with the head between the knees taking deep breaths.
OMIP	TC
XYPY	Remote level controller with indicator
GHQV	Qualified Individual
AWPR	Separating efficiency is reduced
YHDN	Green
QYOS	By throttling of the pump discharge valve
MIJD	Lifeboat
YTYS	The welder shall have been instructed in the use of the ship's welding plant.
BJKR	Swelling below the bandage and heavy pain
GYQI	300 PPM.
XETN	Starting achieved within 2 min of commencing the start procedure at an ambient temperature of -15°C
LIDIQ	Thick paper (chart paper).
BNEO	Channels 6, 13 & 16
KILB	The opening pressure for the injection valve for the cylinder is set too high.
BQDK	Lubricating oil.
GVIO	Push the hook through the skin until the barb protrudes, then cut the hook between the barb and the skin and gently withdraw the hook
WNGV	R(S)= 4 ohm
PEVX	Nothing for the first 24 hours, then 1/2 litre per day (more in the tropics)
UKSI	The message means the yacht has been overturned in heavy seas
MBRG	All the answers are correct
JCFG	Remove the load from the alternator to be stopped
GMJM	Answer the alarm, top up the tank and check the system for leakage before resuming unmanned operation.
TNPQ	By measuring a standard gauge block or rod at a common temperature.
QAKI	At least one
BNOQ	Potentiometer, 10 kilo-ohms
ACYL	Notify the Chief Officer or officer on duty and run the ventilation for at least 15 minutes
BUFM	Plan for safety preparedness
HWBC	Too low suction pressure.
MHHP	Do not use dangerous liquid detergents in closed spaces
CFYN	To minimise risk of gas leakage and ensure correct clearance between piston and cylinder cover.
SEDA	The angle the ship will lie when the ship has a negative GM
IHCT	Raise alarm, identify means of isolation and apply before approaching victim.
NFVL	Stop the engine and check for a fuel or water leak.
TVTB	Stop all F.O. transfers and other fuel operations immediately and check all fuel tank levels.
DWPW	Yes, all kind of food waste can be dumped overboard
BOXP	There are 9 special area where it is forbidden to pump out any sludge or oil residues
CVXG	Into the crankcase and mix with the lube oil.
SJKT	Put on a life jacket
EUTX	Raise the governor speed controller of the incoming alternator and reduce the governor speed controller of the alternator already on the switchboard
YFPM	Printed Circuit Board
FXCG	The visible smoke that is a result of combustion
QQNT	Voyage itinerary and departure and arrival times.
JWXI	For as long as people are working in the tank.
XVIM	Stand behind the casualty. Clench your fist with the tumb inwards in the center of upper abdomen. Grasp your fist with your other hand and pull quickly inwards.
YFKP	4
TCGV	12 - 16 times per minute
CVNA	All the spaces mentioned
EYCQ	To make sure that they are properly closed with the self closing device so that any fire is contained and the extinguishing medium can be released without delay.
HJNL	A directional control valve.
AGXI	Increased delivery pressure
NCOX	OR
CGER	a manually controlled lamp fitted on the inside
CWBD	The number of persons should be clearly stated on the outside of the boats bow.
XIWI	The rags may be caught by running machinery or power tools.
EGOG	Inlet and outlet temperatures and pressure drops across the heat exchanger for both fluids.
NNOO	Lifebuoy with light and smoke
LDHS	a. blue b. grey c. orange
CHMA	Stop discharge, inform USCG and Qualified Individual.
BFUP	The correct form of response would be to give the wind force and direction, the range of visibility and the sea state.
AWXG	To ensure that the recommended levels of treatment chemicals are maintained at all times.
CLIB	Allow for changes in water volume due to temperature variation (expansion)
ORIW	C(S) = 4 ?F
JOKT	The heat transfer surfaces should be cleaned
NVCD	They all have opportunity to smuggle drugs
XLBJ	Making use of Risk Assessment as a means to improving safety
NLEG	Marine Pollution means that the marine environment is contaminated by harmful or unacceptable liquids, substances or particles
MTBD	Undue overspeeding
FIBF	Ball bearings on the shaft and the wear rings for the pump housing or impeller.
EXHS	Notify the Bridge and switch the UMS selector switch to manual mode and engage the "dead man alarm"
FRTI	All of the below mentioned
NIDT	The person who is designated in the muster list
SIOB	200-240 deg C
HPHR	Zener diode
MKAU	NOR
ONUY	No it is not
OVHR	Pale or grey.
YPYM	The parcel is addressed to no one in particular, arrives unexpectedly and seems heavy for its size."
RGCL	B-15
WFAM	The correct form of response would be: "I am using the 12 mile range scale"
DQSH	All the answers are good
NJUMP	Confirm with their search partner that the object found is suspicious
UNKG	A material that neither burns nor emits flammable fumes in such a quantity as to experience ignition, when the temperature rises to 750 ?C
QVCN	Wait for a resuscitator to be brought from the ship's first aid locker and use it?
UYAE	Flotsam
IDMA	The correct form of response would be: My vessel has a fire in the accommodation and we require fire-fighting assistance
JYMM	None of the answers is correct
PBHG	60 minutes
WCFC	Strain gauge
RXRQ	Stop pumps - report - clean up?
SUKO	Not less than 3.0 metres
KMWH	The International Management Code for the Safe Operation of Ships and for Pollution Prevention
JWIN	Total pressure head

#################################
//ÊÎÍÅÖ CES 5.0 | Engine | operational
#################################




